(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "AmigaPCI-040 Local Bus Card")
		(date "2024-12-31")
		(rev "4.1")
	)
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(3 "In3.Cu" signal)
		(4 "In4.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/home/jason/Documents/Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3V3")
	(net 3 "+5V")
	(net 4 "LVA2")
	(net 5 "+1V2")
	(net 6 "_CPUCONF")
	(net 7 "Net-(U111-GNDPLL1)")
	(net 8 "Net-(U111-VCCPLL1)")
	(net 9 "Net-(U111-GNDPLL0)")
	(net 10 "Net-(U111-VCCPLL0)")
	(net 11 "/Fast Memory/U109_SS")
	(net 12 "_CPURST")
	(net 13 "/Fast Memory/U109_CRESET")
	(net 14 "/Fast Memory/U109_SDI")
	(net 15 "/Fast Memory/U109_SCK")
	(net 16 "PORTSIZE")
	(net 17 "D12")
	(net 18 "D10")
	(net 19 "D15")
	(net 20 "D11")
	(net 21 "D9")
	(net 22 "D7")
	(net 23 "D14")
	(net 24 "D13")
	(net 25 "D8")
	(net 26 "D6")
	(net 27 "D1")
	(net 28 "D2")
	(net 29 "D5")
	(net 30 "D4")
	(net 31 "D3")
	(net 32 "D0")
	(net 33 "D22")
	(net 34 "D20")
	(net 35 "D21")
	(net 36 "D23")
	(net 37 "D31")
	(net 38 "D28")
	(net 39 "D30")
	(net 40 "D29")
	(net 41 "D18")
	(net 42 "D26")
	(net 43 "D19")
	(net 44 "D24")
	(net 45 "D16")
	(net 46 "D17")
	(net 47 "D27")
	(net 48 "D25")
	(net 49 "A5")
	(net 50 "A3")
	(net 51 "A1")
	(net 52 "A4")
	(net 53 "A2")
	(net 54 "A7")
	(net 55 "A6")
	(net 56 "A0")
	(net 57 "A15")
	(net 58 "A14")
	(net 59 "A10")
	(net 60 "A13")
	(net 61 "A11")
	(net 62 "A9")
	(net 63 "A12")
	(net 64 "A16")
	(net 65 "A22")
	(net 66 "A25")
	(net 67 "A19")
	(net 68 "A17")
	(net 69 "A20")
	(net 70 "A18")
	(net 71 "A23")
	(net 72 "A21")
	(net 73 "A31")
	(net 74 "A27")
	(net 75 "A8")
	(net 76 "A28")
	(net 77 "A29")
	(net 78 "A26")
	(net 79 "A30")
	(net 80 "A24")
	(net 81 "TT0")
	(net 82 "UPA1")
	(net 83 "_TCI")
	(net 84 "/CPU/_CDIS")
	(net 85 "TT1")
	(net 86 "/CPU/_MDIS")
	(net 87 "/CPU/TDO")
	(net 88 "UPA0")
	(net 89 "R_W")
	(net 90 "TM1")
	(net 91 "SIZ1")
	(net 92 "TM0")
	(net 93 "SIZ0")
	(net 94 "TM2")
	(net 95 "_TS")
	(net 96 "_TACK")
	(net 97 "unconnected-(U100A-_TIP-Pad141)")
	(net 98 "_LOCK")
	(net 99 "/CPU/SC0")
	(net 100 "_BB")
	(net 101 "_TBI")
	(net 102 "_TEA")
	(net 103 "/CPU/SC1")
	(net 104 "_IPL0")
	(net 105 "/Fast Memory/U109_SDO")
	(net 106 "_RSTOUT")
	(net 107 "_IPL2")
	(net 108 "_BR")
	(net 109 "_IPL1")
	(net 110 "_RESET")
	(net 111 "_BG")
	(net 112 "/Card Connector/U409_SDI")
	(net 113 "/Card Connector/U409_SS")
	(net 114 "EMA0")
	(net 115 "/Card Connector/U409_SCK")
	(net 116 "EMA10")
	(net 117 "EMA6")
	(net 118 "/Card Connector/U409_CRESET")
	(net 119 "/Card Connector/U409_SDO")
	(net 120 "EMA8")
	(net 121 "_UMBE")
	(net 122 "DA8")
	(net 123 "_EMCAS")
	(net 124 "_EMRAS")
	(net 125 "DA21")
	(net 126 "DA24")
	(net 127 "DA11")
	(net 128 "EMA1")
	(net 129 "_EM0CS")
	(net 130 "DA31")
	(net 131 "DA28")
	(net 132 "EMA5")
	(net 133 "EMA4")
	(net 134 "DA7")
	(net 135 "EMA11")
	(net 136 "DA14")
	(net 137 "EMCLKE")
	(net 138 "EMA12")
	(net 139 "EMA7")
	(net 140 "DA1")
	(net 141 "DA26")
	(net 142 "DA0")
	(net 143 "EMA9")
	(net 144 "EMA3")
	(net 145 "_UUBE")
	(net 146 "_EMWE")
	(net 147 "EMA2")
	(net 148 "DA30")
	(net 149 "DA23")
	(net 150 "BCLKC")
	(net 151 "DA19")
	(net 152 "DA4")
	(net 153 "DA15")
	(net 154 "_LMBE")
	(net 155 "DA25")
	(net 156 "DA27")
	(net 157 "DA16")
	(net 158 "DA5")
	(net 159 "DA18")
	(net 160 "_LLBE")
	(net 161 "DA22")
	(net 162 "DA9")
	(net 163 "unconnected-(U401-NC-Pad73)")
	(net 164 "DA20")
	(net 165 "DA3")
	(net 166 "DA29")
	(net 167 "unconnected-(U401-NC-Pad70)")
	(net 168 "unconnected-(U401-NC-Pad14)")
	(net 169 "unconnected-(U401-NC-Pad30)")
	(net 170 "LVA0")
	(net 171 "LVA3")
	(net 172 "LVA1")
	(net 173 "LVA6")
	(net 174 "LVA5")
	(net 175 "LVA4")
	(net 176 "LVA7")
	(net 177 "unconnected-(U400-VPP_FAST-Pad76)")
	(net 178 "LVA9")
	(net 179 "LVA12")
	(net 180 "LVA11")
	(net 181 "LVA13")
	(net 182 "LVA14")
	(net 183 "LVA8")
	(net 184 "LVA15")
	(net 185 "LVA10")
	(net 186 "LVA18")
	(net 187 "LVA16")
	(net 188 "LVA17")
	(net 189 "LVA22")
	(net 190 "LVA23")
	(net 191 "LVA20")
	(net 192 "LVA21")
	(net 193 "LVA19")
	(net 194 "LVA26")
	(net 195 "LVA24")
	(net 196 "LVA25")
	(net 197 "LVA31")
	(net 198 "LVA27")
	(net 199 "LVA29")
	(net 200 "LVA30")
	(net 201 "LVA28")
	(net 202 "unconnected-(U100A-PST2-Pad140)")
	(net 203 "unconnected-(U100A-PST3-Pad177)")
	(net 204 "unconnected-(U100A-PST0-Pad176)")
	(net 205 "unconnected-(U100A-TLN0-Pad126)")
	(net 206 "unconnected-(U100A-_TRST-Pad164)")
	(net 207 "unconnected-(U100A-TCK-Pad148)")
	(net 208 "unconnected-(U100A-_MI-Pad124)")
	(net 209 "unconnected-(U100A-DLE-Pad170)")
	(net 210 "unconnected-(U100A-TDI-Pad147)")
	(net 211 "unconnected-(U100A-PST1-Pad158)")
	(net 212 "unconnected-(U100A-TLN1-Pad120)")
	(net 213 "unconnected-(U100A-_CIOUT-Pad127)")
	(net 214 "unconnected-(U100A-_IPEND-Pad145)")
	(net 215 "unconnected-(U100A-TMS-Pad149)")
	(net 216 "_INT6")
	(net 217 "unconnected-(U401-NC-Pad57)")
	(net 218 "_EM1CS")
	(net 219 "unconnected-(U402-NC-Pad70)")
	(net 220 "unconnected-(U402-NC-Pad73)")
	(net 221 "unconnected-(U402-NC-Pad30)")
	(net 222 "unconnected-(U402-NC-Pad57)")
	(net 223 "unconnected-(U402-NC-Pad14)")
	(net 224 "DA13")
	(net 225 "DA2")
	(net 226 "SIZ1-3V")
	(net 227 "SIZ0-3V")
	(net 228 "R_W-3V")
	(net 229 "unconnected-(U203A-A1-Pad3)")
	(net 230 "DA6")
	(net 231 "_TS-3V")
	(net 232 "DA17")
	(net 233 "_INT2")
	(net 234 "DA10")
	(net 235 "_LBEN")
	(net 236 "Net-(X100-OUT)")
	(net 237 "/Card Connector/CLK40")
	(net 238 "BCLKA")
	(net 239 "Net-(U111-IO3_14A_GBIN6)")
	(net 240 "RAMCLKB")
	(net 241 "Net-(U111-IO2_81_GBIN5)")
	(net 242 "BCLKB")
	(net 243 "Net-(U111-IO2_82_GBIN4)")
	(net 244 "Net-(U111-IO1_140_GBIN3)")
	(net 245 "Net-(U111-IO1_141_GBIN2)")
	(net 246 "_TA-CPU")
	(net 247 "_TS-CPU")
	(net 248 "unconnected-(U203A-B1-Pad17)")
	(net 249 "unconnected-(U203A-B0-Pad18)")
	(net 250 "unconnected-(U203A-A0-Pad2)")
	(net 251 "unconnected-(U111-IO0_197_GBIN1-Pad128)")
	(net 252 "AA0")
	(net 253 "AA1")
	(net 254 "BUFDIR")
	(net 255 "A1_OUT")
	(net 256 "_DMA")
	(net 257 "LVDA7")
	(net 258 "_BUFEN")
	(net 259 "LVDA6")
	(net 260 "LVDA1")
	(net 261 "LVDA2")
	(net 262 "LVDA5")
	(net 263 "DA12")
	(net 264 "LVDA0")
	(net 265 "LVDA4")
	(net 266 "LVDA3")
	(net 267 "LVDA8")
	(net 268 "LVDA9")
	(net 269 "LVDA11")
	(net 270 "LVDA16")
	(net 271 "LVDA10")
	(net 272 "LVDA12")
	(net 273 "LVDA13")
	(net 274 "LVDA18")
	(net 275 "LVDA14")
	(net 276 "LVDA20")
	(net 277 "LVDA23")
	(net 278 "LVDA25")
	(net 279 "LVDA15")
	(net 280 "LVDA19")
	(net 281 "LVDA22")
	(net 282 "LVDA17")
	(net 283 "LVDA30")
	(net 284 "LVDA27")
	(net 285 "LVDA31")
	(net 286 "LVDA29")
	(net 287 "CDONE")
	(net 288 "unconnected-(U111-VPP_FAST-Pad109)")
	(net 289 "BANK1")
	(net 290 "BANK0")
	(net 291 "PCLK")
	(net 292 "LVDA21")
	(net 293 "LVDA24")
	(net 294 "LVDA26")
	(net 295 "LVDA28")
	(net 296 "LVDB13")
	(net 297 "LVDB2")
	(net 298 "Net-(CN100-Pin_c16)")
	(net 299 "_TEA-CPU")
	(net 300 "_TBI-CPU")
	(net 301 "_TCI-CPU")
	(net 302 "_CPUBG")
	(net 303 "_BB-3V")
	(net 304 "_BG-3V")
	(net 305 "unconnected-(U100A-_LOCKE-Pad144)")
	(net 306 "LVDB6")
	(net 307 "LVDB1")
	(net 308 "LVDB8")
	(net 309 "Net-(CN100-Pin_b12)")
	(net 310 "LVDB11")
	(net 311 "LVDB16")
	(net 312 "LVDB9")
	(net 313 "LVDB7")
	(net 314 "LVDB18")
	(net 315 "LVDB3")
	(net 316 "LVDB12")
	(net 317 "LVDB10")
	(net 318 "LVDB5")
	(net 319 "LVDB0")
	(net 320 "LVDB4")
	(net 321 "LVDB15")
	(net 322 "LVDB25")
	(net 323 "LVDB24")
	(net 324 "LVDB17")
	(net 325 "LVDB27")
	(net 326 "LVDB19")
	(net 327 "LVDB28")
	(net 328 "LVDB14")
	(net 329 "LVDB22")
	(net 330 "LVDB29")
	(net 331 "LVDB31")
	(net 332 "LVDB20")
	(net 333 "LVDB21")
	(net 334 "LVDB26")
	(net 335 "LVDB30")
	(net 336 "LVDB23")
	(net 337 "A0_OUT")
	(net 338 "unconnected-(U111-IO2_96-Pad61)")
	(net 339 "unconnected-(U111-IO2_102-Pad62)")
	(net 340 "unconnected-(U111-IO2_95-Pad60)")
	(net 341 "unconnected-(U111-IO2_103_CBSEL0-Pad63)")
	(net 342 "unconnected-(U400-IOR_60_GBIN3-Pad62)")
	(net 343 "RAMCLKA")
	(net 344 "unconnected-(U111-IO3_13B_GBIN7-Pad20)")
	(net 345 "Net-(U111-IO2_94)")
	(net 346 "unconnected-(U400-IOL_1B-Pad2)")
	(net 347 "Net-(CN100-Pin_a17)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 72.49 65.685 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C202"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.165 73.42)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R116"
			(at 3.615 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 7.635 0.02 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 243 "Net-(U111-IO2_82_GBIN4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 240 "RAMCLKB")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 118.26 101.75 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C137"
			(at 0 -1.43 135)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.011325 -2.800143 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 59.85 126.32 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C115"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 187.025 101.13 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C423"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 205.08 126.32 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C114"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:TSOP-II-86"
		(layer "F.Cu")
		(at 196.25 65.13)
		(descr "54-lead TSOP typ II package")
		(tags "TSOPII TSOP2")
		(property "Reference" "U401"
			(at 0 -12.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "SDRAM(16Mx32)"
			(at 0 12.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "AmigaPCI:TSOP-II-86"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/42-45R-S-32160F.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16M x 32 bit Synchronous DRAM (SDRAM), TSOP II 86pin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(clearance 0.1)
		(attr smd)
		(pad "1" smd rect
			(at -5.75 -10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -5.75 -10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 266 "LVDA3")
			(pinfunction "DQ0")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -5.75 -9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -5.75 -9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 264 "LVDA0")
			(pinfunction "DQ1")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -5.75 -8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 260 "LVDA1")
			(pinfunction "DQ2")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -5.75 -8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -5.75 -7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 265 "LVDA4")
			(pinfunction "DQ3")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -5.75 -7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 261 "LVDA2")
			(pinfunction "DQ4")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -5.75 -6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -5.75 -6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 262 "LVDA5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -5.75 -5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 259 "LVDA6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -5.75 -5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -5.75 -4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 257 "LVDA7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -5.75 -4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "unconnected-(U401-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd rect
			(at -5.75 -3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -5.75 -3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "_LLBE")
			(pinfunction "DQM0")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -5.75 -2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "_EMWE")
			(pinfunction "_WE")
			(pintype "input")
		)
		(pad "18" smd rect
			(at -5.75 -2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "_EMCAS")
			(pinfunction "_CAS")
			(pintype "input")
		)
		(pad "19" smd rect
			(at -5.75 -1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "_EMRAS")
			(pinfunction "_RAS")
			(pintype "input")
		)
		(pad "20" smd rect
			(at -5.75 -1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "_EM0CS")
			(pinfunction "_CS")
			(pintype "input")
		)
		(pad "21" smd rect
			(at -5.75 -0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "EMA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "22" smd rect
			(at -5.75 0)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 290 "BANK0")
			(pinfunction "BA0")
			(pintype "input")
		)
		(pad "23" smd rect
			(at -5.75 0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 289 "BANK1")
			(pinfunction "BA1")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -5.75 1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "EMA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "25" smd rect
			(at -5.75 1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "EMA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -5.75 2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "EMA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" smd rect
			(at -5.75 2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "EMA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" smd rect
			(at -5.75 3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "_UMBE")
			(pinfunction "DQM2")
			(pintype "input")
		)
		(pad "29" smd rect
			(at -5.75 3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "30" smd rect
			(at -5.75 4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "unconnected-(U401-NC-Pad30)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "31" smd rect
			(at -5.75 4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 270 "LVDA16")
			(pinfunction "DQ16")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -5.75 5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at -5.75 5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 282 "LVDA17")
			(pinfunction "DQ17")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at -5.75 6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 274 "LVDA18")
			(pinfunction "DQ18")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at -5.75 6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at -5.75 7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 280 "LVDA19")
			(pinfunction "DQ19")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at -5.75 7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 276 "LVDA20")
			(pinfunction "DQ20")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at -5.75 8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at -5.75 8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 292 "LVDA21")
			(pinfunction "DQ21")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at -5.75 9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "LVDA22")
			(pinfunction "DQ22")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at -5.75 9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at -5.75 10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 277 "LVDA23")
			(pinfunction "DQ23")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at -5.75 10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 5.75 10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "45" smd rect
			(at 5.75 10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 293 "LVDA24")
			(pinfunction "DQ24")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 5.75 9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "47" smd rect
			(at 5.75 9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 278 "LVDA25")
			(pinfunction "DQ25")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 5.75 8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 294 "LVDA26")
			(pinfunction "DQ26")
			(pintype "bidirectional")
		)
		(pad "49" smd rect
			(at 5.75 8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "50" smd rect
			(at 5.75 7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 284 "LVDA27")
			(pinfunction "DQ27")
			(pintype "bidirectional")
		)
		(pad "51" smd rect
			(at 5.75 7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 295 "LVDA28")
			(pinfunction "DQ28")
			(pintype "bidirectional")
		)
		(pad "52" smd rect
			(at 5.75 6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 5.75 6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 286 "LVDA29")
			(pinfunction "DQ29")
			(pintype "bidirectional")
		)
		(pad "54" smd rect
			(at 5.75 5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 283 "LVDA30")
			(pinfunction "DQ30")
			(pintype "bidirectional")
		)
		(pad "55" smd rect
			(at 5.75 5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "56" smd rect
			(at 5.75 4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "LVDA31")
			(pinfunction "DQ31")
			(pintype "bidirectional")
		)
		(pad "57" smd rect
			(at 5.75 4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "unconnected-(U401-NC-Pad57)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "58" smd rect
			(at 5.75 3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "59" smd rect
			(at 5.75 3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 145 "_UUBE")
			(pinfunction "DQM3")
			(pintype "input")
		)
		(pad "60" smd rect
			(at 5.75 2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 144 "EMA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "61" smd rect
			(at 5.75 2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "EMA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "62" smd rect
			(at 5.75 1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "EMA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "63" smd rect
			(at 5.75 1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "EMA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "64" smd rect
			(at 5.75 0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "EMA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 5.75 0)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "EMA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "66" smd rect
			(at 5.75 -0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "EMA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "67" smd rect
			(at 5.75 -1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "EMCLKE")
			(pinfunction "CKE")
			(pintype "input")
		)
		(pad "68" smd rect
			(at 5.75 -1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 343 "RAMCLKA")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "69" smd rect
			(at 5.75 -2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "EMA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "70" smd rect
			(at 5.75 -2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "unconnected-(U401-NC-Pad70)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "71" smd rect
			(at 5.75 -3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 154 "_LMBE")
			(pinfunction "DQM1")
			(pintype "input")
		)
		(pad "72" smd rect
			(at 5.75 -3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "73" smd rect
			(at 5.75 -4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "unconnected-(U401-NC-Pad73)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "74" smd rect
			(at 5.75 -4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 279 "LVDA15")
			(pinfunction "DQ8")
			(pintype "bidirectional")
		)
		(pad "75" smd rect
			(at 5.75 -5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "76" smd rect
			(at 5.75 -5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 275 "LVDA14")
			(pinfunction "DQ9")
			(pintype "bidirectional")
		)
		(pad "77" smd rect
			(at 5.75 -6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 273 "LVDA13")
			(pinfunction "DQ10")
			(pintype "bidirectional")
		)
		(pad "78" smd rect
			(at 5.75 -6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "79" smd rect
			(at 5.75 -7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 272 "LVDA12")
			(pinfunction "DQ11")
			(pintype "bidirectional")
		)
		(pad "80" smd rect
			(at 5.75 -7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 269 "LVDA11")
			(pinfunction "DQ12")
			(pintype "bidirectional")
		)
		(pad "81" smd rect
			(at 5.75 -8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "82" smd rect
			(at 5.75 -8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 271 "LVDA10")
			(pinfunction "DQ13")
			(pintype "bidirectional")
		)
		(pad "83" smd rect
			(at 5.75 -9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 268 "LVDA9")
			(pinfunction "DQ14")
			(pintype "bidirectional")
		)
		(pad "84" smd rect
			(at 5.75 -9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "85" smd rect
			(at 5.75 -10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 267 "LVDA8")
			(pinfunction "DQ15")
			(pintype "bidirectional")
		)
		(pad "86" smd rect
			(at 5.75 -10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 141.455 48.7 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R107"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "/Card Connector/U409_CRESET")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.84 61.33 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C410"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 86.51 88.385 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C209"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121.05 73.61 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R117"
			(at 0.03 1.52 0)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 0.01 2.99 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 244 "Net-(U111-IO1_140_GBIN3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 238 "BCLKA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 131.28 54.505 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C136"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.57 76.925 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C212"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.57 87.035 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C210"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm_Pad"
		(layer "F.Cu")
		(at 65.01 42.58)
		(descr "Mounting Hole 3.5mm")
		(tags "mounting hole 3.5mm")
		(property "Reference" "H1"
			(at 0 -4.5 0)
			(layer "F.Fab")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 57.77 47.545 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R102"
			(at -3.645 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k7"
			(at -7.355 0.03 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "/CPU/_CDIS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 149.27 64.495113 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C135"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 177.915 60.8075 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U108"
			(at 0 -4.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.2 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "LVA27")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "LVA24")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "LVA21")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "LVA20")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 186 "LVA18")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "LVA19")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "LVA17")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 187 "LVA16")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "A16")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "A17")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "A19")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "A18")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "A20")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "A21")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "A24")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "A27")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 81.69 44.47 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C138"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.895 74.63 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C412"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 63.08 115.14)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J100"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "_BG ASSERT"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "_BG")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 104.715 112.2021 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U106"
			(at 0 -4.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at -5.1879 -0.005 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "LVA13")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 179 "LVA12")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "LVA15")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "LVA0")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "LVA14")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "LVA3")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "LVA2")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "LVA1")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "A1")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "A2")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "A3")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "A14")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "A0")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "A15")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "A12")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "A13")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:Mug"
		(layer "F.Cu")
		(at 173.98 43.52)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "AmigaPCI:Mug"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 168.02 60.8075 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U107"
			(at 0 -4.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.2 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "LVA23")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "LVA25")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 200 "LVA30")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "LVA28")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "LVA26")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "LVA22")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "LVA31")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "LVA29")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "A29")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "A31")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "A22")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "A26")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "A28")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "A30")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "A25")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "A23")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.015 51.26)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R400"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -0.025 -2.93 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Fast Memory/U109_SS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 112.77 93.14 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U104"
			(at 0 -4.199999 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.199999 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 295 "LVDA28")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 294 "LVDA26")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 293 "LVDA24")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "LVDA31")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 283 "LVDA30")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 292 "LVDA21")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "LVDA29")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "LVDA27")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "D27")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "D29")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "D21")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "D30")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "D31")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "D24")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "D26")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "D28")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.935 86.83 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C418"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-144_20x20mm_P0.5mm"
		(layer "F.Cu")
		(at 134.49 82.12 135)
		(descr "LQFP, 144 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=425), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U111"
			(at 0 -12.35 135)
			(layer "F.SilkS")
		)
		(property "Value" "ICE40HX4K-TQ144"
			(at 0 12.35 135)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC FPGA 107 I/O 144TQFP"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Lattice Semiconductor"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "TQFP-144 Lattice Semiconductor"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "ICE40HX4K-TQ144"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "Unavailable"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -10.6625 -8.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 330 "LVDB29")
			(pinfunction "IO3_2A")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -10.6625 -8.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 329 "LVDB22")
			(pinfunction "IO3_2B")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -10.662501 -7.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 332 "LVDB20")
			(pinfunction "IO3_3A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -10.6625 -7.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 336 "LVDB23")
			(pinfunction "IO3_3B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -10.6625 -6.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -10.6625 -6.249999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_3")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -10.6625 -5.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 326 "LVDB19")
			(pinfunction "IO3_4A")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -10.6625 -5.250001 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 322 "LVDB25")
			(pinfunction "IO3_4B")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -10.6625 -4.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 328 "LVDB14")
			(pinfunction "IO3_5A")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -10.6625 -4.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 321 "LVDB15")
			(pinfunction "IO3_5B")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -10.6625 -3.749999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 324 "LVDB17")
			(pinfunction "IO3_8A")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -10.6625 -3.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 296 "LVDB13")
			(pinfunction "IO3_8B")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -10.6625 -2.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -10.6625 -2.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__2")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -10.6625 -1.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 314 "LVDB18")
			(pinfunction "IO3_10A")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -10.662501 -1.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 316 "LVDB12")
			(pinfunction "IO3_10B")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -10.6625 -0.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 311 "LVDB16")
			(pinfunction "IO3_12A")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -10.6625 -0.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 317 "LVDB10")
			(pinfunction "IO3_12B")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -10.6625 0.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 310 "LVDB11")
			(pinfunction "IO3_13A")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -10.6625 0.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 344 "unconnected-(U111-IO3_13B_GBIN7-Pad20)")
			(pinfunction "IO3_13B_GBIN7")
			(pintype "input+no_connect")
		)
		(pad "21" smd roundrect
			(at -10.662501 1.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 239 "Net-(U111-IO3_14A_GBIN6)")
			(pinfunction "IO3_14A_GBIN6")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -10.6625 1.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 312 "LVDB9")
			(pinfunction "IO3_14B")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -10.6625 2.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 308 "LVDB8")
			(pinfunction "IO3_17A")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at -10.6625 2.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 313 "LVDB7")
			(pinfunction "IO3_17B")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at -10.6625 3.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 318 "LVDB5")
			(pinfunction "IO3_18A")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at -10.6625 3.749999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "LVDB6")
			(pinfunction "IO3_18B")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at -10.6625 4.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at -10.6625 4.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 307 "LVDB1")
			(pinfunction "IO3_23A")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -10.6625 5.250001 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 320 "LVDB4")
			(pinfunction "IO3_23B")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -10.6625 5.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_3__1")
			(pintype "power_in")
		)
		(pad "31" smd roundrect
			(at -10.6625 6.249999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 297 "LVDB2")
			(pinfunction "IO3_24A")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at -10.6625 6.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "LVDB3")
			(pinfunction "IO3_24B")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -10.6625 7.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 319 "LVDB0")
			(pinfunction "IO3_25A")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -10.662501 7.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "_RESET")
			(pinfunction "IO3_25B")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -10.6625 8.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "36" smd roundrect
			(at -10.6625 8.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "37" smd roundrect
			(at -8.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "LVA0")
			(pinfunction "IO2_56")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at -8.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "LVA1")
			(pinfunction "IO2_57")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at -7.75 10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "A0_OUT")
			(pinfunction "IO2_61")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at -7.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__1")
			(pintype "power_in")
		)
		(pad "41" smd roundrect
			(at -6.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 255 "A1_OUT")
			(pinfunction "IO2_63")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at -6.249999 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "PORTSIZE")
			(pinfunction "IO2_64")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at -5.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "_TEA")
			(pinfunction "IO2_71")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at -5.250001 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "_TCI")
			(pinfunction "IO2_72")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at -4.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 95 "_TS")
			(pinfunction "IO2_73")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at -4.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_2")
			(pintype "power_in")
		)
		(pad "47" smd roundrect
			(at -3.749999 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "_TACK")
			(pinfunction "IO2_79")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at -3.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 235 "_LBEN")
			(pinfunction "IO2_80")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at -2.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 241 "Net-(U111-IO2_81_GBIN5)")
			(pinfunction "IO2_81_GBIN5")
			(pintype "input")
		)
		(pad "50" smd roundrect
			(at -2.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "51" smd roundrect
			(at -1.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "52" smd roundrect
			(at -1.25 10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 243 "Net-(U111-IO2_82_GBIN4)")
			(pinfunction "IO2_82_GBIN4")
			(pintype "input")
		)
		(pad "53" smd roundrect
			(at -0.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U111-GNDPLL0)")
			(pinfunction "GNDPLL0")
			(pintype "power_in")
		)
		(pad "54" smd roundrect
			(at -0.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U111-VCCPLL0)")
			(pinfunction "VCCPLL0")
			(pintype "power_in")
		)
		(pad "55" smd roundrect
			(at 0.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "_TBI")
			(pinfunction "IO2_91")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at 0.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 345 "Net-(U111-IO2_94)")
			(pinfunction "IO2_94")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at 1.25 10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_2__1")
			(pintype "power_in")
		)
		(pad "58" smd roundrect
			(at 1.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "59" smd roundrect
			(at 2.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__3")
			(pintype "power_in")
		)
		(pad "60" smd roundrect
			(at 2.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 340 "unconnected-(U111-IO2_95-Pad60)")
			(pinfunction "IO2_95")
			(pintype "bidirectional+no_connect")
		)
		(pad "61" smd roundrect
			(at 3.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 338 "unconnected-(U111-IO2_96-Pad61)")
			(pinfunction "IO2_96")
			(pintype "bidirectional+no_connect")
		)
		(pad "62" smd roundrect
			(at 3.749999 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 339 "unconnected-(U111-IO2_102-Pad62)")
			(pinfunction "IO2_102")
			(pintype "bidirectional+no_connect")
		)
		(pad "63" smd roundrect
			(at 4.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 341 "unconnected-(U111-IO2_103_CBSEL0-Pad63)")
			(pinfunction "IO2_103_CBSEL0")
			(pintype "bidirectional+no_connect")
		)
		(pad "64" smd roundrect
			(at 4.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 300 "_TBI-CPU")
			(pinfunction "IO2_104_CBSEL1")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at 5.250001 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 287 "CDONE")
			(pinfunction "CDONE")
			(pintype "input")
		)
		(pad "66" smd roundrect
			(at 5.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "/Card Connector/U409_CRESET")
			(pinfunction "CRESET_B")
			(pintype "input")
		)
		(pad "67" smd roundrect
			(at 6.249999 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/Card Connector/U409_SDI")
			(pinfunction "IOB_105_SDO")
			(pintype "bidirectional")
		)
		(pad "68" smd roundrect
			(at 6.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "/Card Connector/U409_SDO")
			(pinfunction "IOB_106_SDI")
			(pintype "bidirectional")
		)
		(pad "69" smd roundrect
			(at 7.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__4")
			(pintype "power_in")
		)
		(pad "70" smd roundrect
			(at 7.75 10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/Card Connector/U409_SCK")
			(pinfunction "IOB_107_SCK")
			(pintype "bidirectional")
		)
		(pad "71" smd roundrect
			(at 8.25 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "/Card Connector/U409_SS")
			(pinfunction "IOB_108_SS")
			(pintype "bidirectional")
		)
		(pad "72" smd roundrect
			(at 8.75 10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC_SPI")
			(pintype "power_in")
		)
		(pad "73" smd roundrect
			(at 10.6625 8.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 266 "LVDA3")
			(pinfunction "IO1_109")
			(pintype "bidirectional")
		)
		(pad "74" smd roundrect
			(at 10.6625 8.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 264 "LVDA0")
			(pinfunction "IO1_110")
			(pintype "bidirectional")
		)
		(pad "75" smd roundrect
			(at 10.662501 7.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 260 "LVDA1")
			(pinfunction "IO1_111")
			(pintype "bidirectional")
		)
		(pad "76" smd roundrect
			(at 10.6625 7.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 265 "LVDA4")
			(pinfunction "IO1_112")
			(pintype "bidirectional")
		)
		(pad "77" smd roundrect
			(at 10.6625 6.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "78" smd roundrect
			(at 10.6625 6.249999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 261 "LVDA2")
			(pinfunction "IO1_114")
			(pintype "bidirectional")
		)
		(pad "79" smd roundrect
			(at 10.6625 5.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 262 "LVDA5")
			(pinfunction "IO1_115")
			(pintype "bidirectional")
		)
		(pad "80" smd roundrect
			(at 10.6625 5.250001 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 259 "LVDA6")
			(pinfunction "IO1_116")
			(pintype "bidirectional")
		)
		(pad "81" smd roundrect
			(at 10.6625 4.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 257 "LVDA7")
			(pinfunction "IO1_117")
			(pintype "bidirectional")
		)
		(pad "82" smd roundrect
			(at 10.6625 4.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 267 "LVDA8")
			(pinfunction "IO1_118")
			(pintype "bidirectional")
		)
		(pad "83" smd roundrect
			(at 10.6625 3.749999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 268 "LVDA9")
			(pinfunction "IO1_119")
			(pintype "bidirectional")
		)
		(pad "84" smd roundrect
			(at 10.6625 3.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 271 "LVDA10")
			(pinfunction "IO1_120")
			(pintype "bidirectional")
		)
		(pad "85" smd roundrect
			(at 10.6625 2.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 269 "LVDA11")
			(pinfunction "IO1_128")
			(pintype "bidirectional")
		)
		(pad "86" smd roundrect
			(at 10.6625 2.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__5")
			(pintype "power_in")
		)
		(pad "87" smd roundrect
			(at 10.6625 1.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 272 "LVDA12")
			(pinfunction "IO1_136")
			(pintype "bidirectional")
		)
		(pad "88" smd roundrect
			(at 10.662501 1.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 270 "LVDA16")
			(pinfunction "IO1_137")
			(pintype "bidirectional")
		)
		(pad "89" smd roundrect
			(at 10.6625 0.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_1")
			(pintype "power_in")
		)
		(pad "90" smd roundrect
			(at 10.6625 0.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 273 "LVDA13")
			(pinfunction "IO1_138")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at 10.6625 -0.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 274 "LVDA18")
			(pinfunction "IO1_139")
			(pintype "bidirectional")
		)
		(pad "92" smd roundrect
			(at 10.6625 -0.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__2")
			(pintype "power_in")
		)
		(pad "93" smd roundrect
			(at 10.662501 -1.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 244 "Net-(U111-IO1_140_GBIN3)")
			(pinfunction "IO1_140_GBIN3")
			(pintype "input")
		)
		(pad "94" smd roundrect
			(at 10.6625 -1.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 245 "Net-(U111-IO1_141_GBIN2)")
			(pinfunction "IO1_141_GBIN2")
			(pintype "input")
		)
		(pad "95" smd roundrect
			(at 10.6625 -2.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "LVDA22")
			(pinfunction "IO1_144")
			(pintype "bidirectional")
		)
		(pad "96" smd roundrect
			(at 10.6625 -2.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "_BG-3V")
			(pinfunction "IO1_146")
			(pintype "bidirectional")
		)
		(pad "97" smd roundrect
			(at 10.6625 -3.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "IO1_147")
			(pintype "bidirectional")
		)
		(pad "98" smd roundrect
			(at 10.6625 -3.749999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 275 "LVDA14")
			(pinfunction "IO1_148")
			(pintype "bidirectional")
		)
		(pad "99" smd roundrect
			(at 10.6625 -4.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 279 "LVDA15")
			(pinfunction "IO1_152")
			(pintype "bidirectional")
		)
		(pad "100" smd roundrect
			(at 10.6625 -4.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_1__1")
			(pintype "power_in")
		)
		(pad "101" smd roundrect
			(at 10.6625 -5.250001 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "_TCI-CPU")
			(pinfunction "IO1_160")
			(pintype "bidirectional")
		)
		(pad "102" smd roundrect
			(at 10.6625 -5.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pinfunction "IO1_161")
			(pintype "bidirectional")
		)
		(pad "103" smd roundrect
			(at 10.6625 -6.249999 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__6")
			(pintype "power_in")
		)
		(pad "104" smd roundrect
			(at 10.6625 -6.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 282 "LVDA17")
			(pinfunction "IO1_164")
			(pintype "bidirectional")
		)
		(pad "105" smd roundrect
			(at 10.6625 -7.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 277 "LVDA23")
			(pinfunction "IO1_165")
			(pintype "bidirectional")
		)
		(pad "106" smd roundrect
			(at 10.662501 -7.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 280 "LVDA19")
			(pinfunction "IO1_166")
			(pintype "bidirectional")
		)
		(pad "107" smd roundrect
			(at 10.6625 -8.25 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 278 "LVDA25")
			(pinfunction "IO1_167")
			(pintype "bidirectional")
		)
		(pad "108" smd roundrect
			(at 10.6625 -8.75 135)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VPP_2V5")
			(pintype "power_in")
		)
		(pad "109" smd roundrect
			(at 8.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 288 "unconnected-(U111-VPP_FAST-Pad109)")
			(pinfunction "VPP_FAST")
			(pintype "power_in+no_connect")
		)
		(pad "110" smd roundrect
			(at 8.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 276 "LVDA20")
			(pinfunction "IO0_168")
			(pintype "bidirectional")
		)
		(pad "111" smd roundrect
			(at 7.75 -10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__3")
			(pintype "power_in")
		)
		(pad "112" smd roundrect
			(at 7.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "LVDA27")
			(pinfunction "IO0_169")
			(pintype "bidirectional")
		)
		(pad "113" smd roundrect
			(at 6.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "LVDA29")
			(pinfunction "IO0_170")
			(pintype "bidirectional")
		)
		(pad "114" smd roundrect
			(at 6.249999 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 292 "LVDA21")
			(pinfunction "IO0_171")
			(pintype "bidirectional")
		)
		(pad "115" smd roundrect
			(at 5.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 283 "LVDA30")
			(pinfunction "IO0_172")
			(pintype "bidirectional")
		)
		(pad "116" smd roundrect
			(at 5.250001 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "LVDA31")
			(pinfunction "IO0_173")
			(pintype "bidirectional")
		)
		(pad "117" smd roundrect
			(at 4.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 293 "LVDA24")
			(pinfunction "IO0_174")
			(pintype "bidirectional")
		)
		(pad "118" smd roundrect
			(at 4.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 294 "LVDA26")
			(pinfunction "IO0_177")
			(pintype "bidirectional")
		)
		(pad "119" smd roundrect
			(at 3.749999 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 295 "LVDA28")
			(pinfunction "IO0_178")
			(pintype "bidirectional")
		)
		(pad "120" smd roundrect
			(at 3.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "SIZ1-3V")
			(pinfunction "IO0_179")
			(pintype "bidirectional")
		)
		(pad "121" smd roundrect
			(at 2.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 227 "SIZ0-3V")
			(pinfunction "IO0_181")
			(pintype "bidirectional")
		)
		(pad "122" smd roundrect
			(at 2.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "_TEA-CPU")
			(pinfunction "IO0_190")
			(pintype "bidirectional")
		)
		(pad "123" smd roundrect
			(at 1.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_0")
			(pintype "power_in")
		)
		(pad "124" smd roundrect
			(at 1.25 -10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 246 "_TA-CPU")
			(pinfunction "IO0_191")
			(pintype "bidirectional")
		)
		(pad "125" smd roundrect
			(at 0.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 231 "_TS-3V")
			(pinfunction "IO0_192")
			(pintype "bidirectional")
		)
		(pad "126" smd roundrect
			(at 0.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U111-VCCPLL1)")
			(pinfunction "VCCPLL1")
			(pintype "power_in")
		)
		(pad "127" smd roundrect
			(at -0.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U111-GNDPLL1)")
			(pinfunction "GNDPLL1")
			(pintype "power_in")
		)
		(pad "128" smd roundrect
			(at -0.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 251 "unconnected-(U111-IO0_197_GBIN1-Pad128)")
			(pinfunction "IO0_197_GBIN1")
			(pintype "input+no_connect")
		)
		(pad "129" smd roundrect
			(at -1.25 -10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 237 "/Card Connector/CLK40")
			(pinfunction "IO0_198_GBIN0")
			(pintype "input")
		)
		(pad "130" smd roundrect
			(at -1.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "_BB-3V")
			(pinfunction "IO0_206")
			(pintype "bidirectional")
		)
		(pad "131" smd roundrect
			(at -2.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_0__1")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at -2.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__7")
			(pintype "power_in")
		)
		(pad "133" smd roundrect
			(at -3.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "134" smd roundrect
			(at -3.749999 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 256 "_DMA")
			(pinfunction "IO0_212")
			(pintype "bidirectional")
		)
		(pad "135" smd roundrect
			(at -4.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 258 "_BUFEN")
			(pinfunction "IO0_213")
			(pintype "bidirectional")
		)
		(pad "136" smd roundrect
			(at -4.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 254 "BUFDIR")
			(pinfunction "IO0_214")
			(pintype "bidirectional")
		)
		(pad "137" smd roundrect
			(at -5.250001 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 327 "LVDB28")
			(pinfunction "IO0_215")
			(pintype "bidirectional")
		)
		(pad "138" smd roundrect
			(at -5.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 323 "LVDB24")
			(pinfunction "IO0_216")
			(pintype "bidirectional")
		)
		(pad "139" smd roundrect
			(at -6.249999 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 334 "LVDB26")
			(pinfunction "IO0_217")
			(pintype "bidirectional")
		)
		(pad "140" smd roundrect
			(at -6.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__8")
			(pintype "power_in")
		)
		(pad "141" smd roundrect
			(at -7.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 333 "LVDB21")
			(pinfunction "IO0_219")
			(pintype "bidirectional")
		)
		(pad "142" smd roundrect
			(at -7.75 -10.662501 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 335 "LVDB30")
			(pinfunction "IO0_220")
			(pintype "bidirectional")
		)
		(pad "143" smd roundrect
			(at -8.25 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 331 "LVDB31")
			(pinfunction "IO0_221")
			(pintype "bidirectional")
		)
		(pad "144" smd roundrect
			(at -8.75 -10.6625 135)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 325 "LVDB27")
			(pinfunction "IO0_222")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-144_20x20mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.995 106.83 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C425"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 184.9 44.47 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C113"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.57 82.035 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C211"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.81 54.1 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C409"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-100_14x14mm_P0.5mm"
		(layer "F.Cu")
		(at 173.05 82.05 -135)
		(descr "LQFP, 100 Pin (https://www.nxp.com/docs/en/package-information/SOT407-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U400"
			(at 0 -9.42 45)
			(layer "F.SilkS")
		)
		(property "Value" "ICE40HX1K-VQ100"
			(at 0 9.42 45)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "3.4"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "LATTICE SEMICONDUCTOR"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" "QFP-100"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.675 -6 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "EMCLKE")
			(pinfunction "IOL_1A")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -7.675 -5.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 346 "unconnected-(U400-IOL_1B-Pad2)")
			(pinfunction "IOL_1B")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -7.675 -4.999999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "LVA0")
			(pinfunction "IOL_2A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -7.675 -4.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "LVA1")
			(pinfunction "IOL_2B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -7.675 -4.000001 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -7.675 -3.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_3")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -7.675 -3 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 289 "BANK1")
			(pinfunction "IOL_3A")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -7.675 -2.499999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 290 "BANK0")
			(pinfunction "IOL_3B")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -7.675 -2 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 129 "_EM0CS")
			(pinfunction "IOL_5A")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -7.675 -1.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 124 "_EMRAS")
			(pinfunction "IOL_5B")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -7.675 -1 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -7.675 -0.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 123 "_EMCAS")
			(pinfunction "IOL_6A")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -7.675001 0 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "_EMWE")
			(pinfunction "IOL_6B_GBIN7")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -7.675 0.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_3__1")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -7.675 1 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 187 "LVA16")
			(pinfunction "IOL_7A_GBIN6")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -7.675 1.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "LVA17")
			(pinfunction "IOL_7B")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -7.675 2 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at -7.675 2.499999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "LVA19")
			(pinfunction "IOL_8A")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -7.675 3 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 186 "LVA18")
			(pinfunction "IOL_8B")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -7.675 3.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "LVA20")
			(pinfunction "IOL_10A")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -7.675 4.000001 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "LVA21")
			(pinfunction "IOL_10B")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -7.675 4.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_3__2")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at -7.675 4.999999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__2")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at -7.675 5.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "LVA24")
			(pinfunction "IOL_12A")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at -7.675 6 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "LVA27")
			(pinfunction "IOL_12B")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at -6 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "LVA29")
			(pinfunction "IOB_26")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at -5.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "LVA31")
			(pinfunction "IOB_27")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at -4.999999 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "LVA22")
			(pinfunction "IOB_28")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -4.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "LVA26")
			(pinfunction "IOB_29")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -4.000001 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "LVA28")
			(pinfunction "IOB_30")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at -3.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_2")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at -3 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__3")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at -2.499999 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 200 "LVA30")
			(pinfunction "IOB_35_GBIN5")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -2 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "LVA25")
			(pinfunction "IOB_36_GBIN4")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -1.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__1")
			(pintype "power_in")
		)
		(pad "36" smd roundrect
			(at -1 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "LVA23")
			(pinfunction "IOB_34")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at -0.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "_UUBE")
			(pinfunction "IOB_37")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 0 7.675001 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_2__1")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at 0.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__4")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 1 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "_UMBE")
			(pinfunction "IOB_41")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 1.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "_LMBE")
			(pinfunction "IOB_42_CBSEL0")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 2 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 160 "_LLBE")
			(pinfunction "IOB_43_CBSEL1")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 2.499999 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 287 "CDONE")
			(pinfunction "CDONE")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 3 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/Fast Memory/U109_CRESET")
			(pinfunction "CRESET_B")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 3.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/Fast Memory/U109_SDI")
			(pinfunction "IOB_44_SDO")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 4.000001 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "/Fast Memory/U109_SDO")
			(pinfunction "IOB_45_SDI")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 4.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__5")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at 4.999999 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Fast Memory/U109_SCK")
			(pinfunction "IOB_46_SCK")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at 5.5 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Fast Memory/U109_SS")
			(pinfunction "IOB_47_SS")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at 6 7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC_SPI")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at 7.675 6 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "IOR_52")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 7.675 5.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 240 "RAMCLKB")
			(pinfunction "IOR_53")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 7.675 4.999999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 242 "BCLKB")
			(pinfunction "IOR_54")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 7.675 4.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 235 "_LBEN")
			(pinfunction "IOR_55")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 7.675 4.000001 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__6")
			(pintype "power_in")
		)
		(pad "56" smd roundrect
			(at 7.675 3.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 246 "_TA-CPU")
			(pinfunction "IOR_56")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at 7.675 3 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 231 "_TS-3V")
			(pinfunction "IOR_57")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at 7.675 2.499999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_1")
			(pintype "power_in")
		)
		(pad "59" smd roundrect
			(at 7.675 2 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "SIZ1-3V")
			(pinfunction "IOR_58")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at 7.675 1.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 227 "SIZ0-3V")
			(pinfunction "IOR_59")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at 7.675 1 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__2")
			(pintype "power_in")
		)
		(pad "62" smd roundrect
			(at 7.675 0.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 342 "unconnected-(U400-IOR_60_GBIN3-Pad62)")
			(pinfunction "IOR_60_GBIN3")
			(pintype "bidirectional+no_connect")
		)
		(pad "63" smd roundrect
			(at 7.675001 0 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "_RESET")
			(pinfunction "IOR_61_GBIN2")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at 7.675 -0.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "LVA13")
			(pinfunction "IOR_63")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at 7.675 -1 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "LVA4")
			(pinfunction "IOR_64")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 7.675 -1.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "LVA9")
			(pinfunction "IOR_65")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at 7.675 -2 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_1__1")
			(pintype "power_in")
		)
		(pad "68" smd roundrect
			(at 7.675 -2.499999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "LVA5")
			(pinfunction "IOR_67")
			(pintype "bidirectional")
		)
		(pad "69" smd roundrect
			(at 7.675 -3 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "LVA6")
			(pinfunction "IOR_68")
			(pintype "bidirectional")
		)
		(pad "70" smd roundrect
			(at 7.675 -3.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__7")
			(pintype "power_in")
		)
		(pad "71" smd roundrect
			(at 7.675 -4.000001 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "LVA7")
			(pinfunction "IOR_69")
			(pintype "bidirectional")
		)
		(pad "72" smd roundrect
			(at 7.675 -4.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "LVA8")
			(pinfunction "IOR_70")
			(pintype "bidirectional")
		)
		(pad "73" smd roundrect
			(at 7.675 -4.999999 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "LVA10")
			(pinfunction "IOR_71")
			(pintype "bidirectional")
		)
		(pad "74" smd roundrect
			(at 7.675 -5.5 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "LVA11")
			(pinfunction "IOR_72")
			(pintype "bidirectional")
		)
		(pad "75" smd roundrect
			(at 7.675 -6 225)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VPP_2V5")
			(pintype "power_in")
		)
		(pad "76" smd roundrect
			(at 6 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "unconnected-(U400-VPP_FAST-Pad76)")
			(pinfunction "VPP_FAST")
			(pintype "power_in+no_connect")
		)
		(pad "77" smd roundrect
			(at 5.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pinfunction "VCC__3")
			(pintype "power_in")
		)
		(pad "78" smd roundrect
			(at 4.999999 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "LVA2")
			(pinfunction "IOT_73")
			(pintype "bidirectional")
		)
		(pad "79" smd roundrect
			(at 4.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "LVA3")
			(pinfunction "IOT_74")
			(pintype "bidirectional")
		)
		(pad "80" smd roundrect
			(at 4.000001 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "LVA14")
			(pinfunction "IOT_75")
			(pintype "bidirectional")
		)
		(pad "81" smd roundrect
			(at 3.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "LVA15")
			(pinfunction "IOT_77")
			(pintype "bidirectional")
		)
		(pad "82" smd roundrect
			(at 3 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 179 "LVA12")
			(pinfunction "IOT_78")
			(pintype "bidirectional")
		)
		(pad "83" smd roundrect
			(at 2.499999 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "EMA2")
			(pinfunction "IOT_79")
			(pintype "bidirectional")
		)
		(pad "84" smd roundrect
			(at 2 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__8")
			(pintype "power_in")
		)
		(pad "85" smd roundrect
			(at 1.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "EMA1")
			(pinfunction "IOT_80")
			(pintype "bidirectional")
		)
		(pad "86" smd roundrect
			(at 1 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 114 "EMA0")
			(pinfunction "IOT_81")
			(pintype "bidirectional")
		)
		(pad "87" smd roundrect
			(at 0.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "EMA10")
			(pinfunction "IOT_82")
			(pintype "bidirectional")
		)
		(pad "88" smd roundrect
			(at 0 -7.675001 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_0")
			(pintype "power_in")
		)
		(pad "89" smd roundrect
			(at -0.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "EMA11")
			(pinfunction "IOT_84_GBIN1")
			(pintype "bidirectional")
		)
		(pad "90" smd roundrect
			(at -1 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 218 "_EM1CS")
			(pinfunction "IOT_85_GBIN0")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at -1.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "EMA12")
			(pinfunction "IOT_86")
			(pintype "bidirectional")
		)
		(pad "92" smd roundrect
			(at -2 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCIO_0__1")
			(pintype "power_in")
		)
		(pad "93" smd roundrect
			(at -2.499999 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "EMA9")
			(pinfunction "IOT_87")
			(pintype "bidirectional")
		)
		(pad "94" smd roundrect
			(at -3 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "EMA8")
			(pinfunction "IOT_88")
			(pintype "bidirectional")
		)
		(pad "95" smd roundrect
			(at -3.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 139 "EMA7")
			(pinfunction "IOT_89")
			(pintype "bidirectional")
		)
		(pad "96" smd roundrect
			(at -4.000001 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "EMA6")
			(pinfunction "IOT_90")
			(pintype "bidirectional")
		)
		(pad "97" smd roundrect
			(at -4.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "EMA5")
			(pinfunction "IOT_91")
			(pintype "bidirectional")
		)
		(pad "98" smd roundrect
			(at -4.999999 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND__9")
			(pintype "power_in")
		)
		(pad "99" smd roundrect
			(at -5.5 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "EMA4")
			(pinfunction "IOT_93")
			(pintype "bidirectional")
		)
		(pad "100" smd roundrect
			(at -6 -7.675 225)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "EMA3")
			(pinfunction "IOT_95")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-100_14x14mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 111.58 44.47 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C116"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 59.29 47.545 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R104"
			(at -3.645 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k7"
			(at -7.345 0.02 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "/CPU/TDO")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.155 74.97)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R115"
			(at 3.635 0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 7.625 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 241 "Net-(U111-IO2_81_GBIN5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 242 "BCLKB")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 151.9 54.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C400"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.57 65.685 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C200"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 86.7 112.16 90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U114"
			(at 0 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G125"
			(at 0 2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNum" "SN74LVC1G125DBVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 256 "_DMA")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 252 "AA0")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "A0")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 64.425 106.63)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R105"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2k7"
			(at 0 1.43 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 247 "_TS-CPU")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 112.9325 61.3 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U101"
			(at 0 -4.199999 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.199999 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 257 "LVDA7")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 259 "LVDA6")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 262 "LVDA5")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 261 "LVDA2")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 265 "LVDA4")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 260 "LVDA1")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 264 "LVDA0")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 266 "LVDA3")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "D3")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "D0")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "D1")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "D4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "D2")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "D5")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "D6")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "D7")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 75.05 88.385 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C207"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 114.68 112.2021 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U105"
			(at 0 -4.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at -5.1679 0 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "LVA4")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "LVA9")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "LVA5")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "LVA6")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "LVA7")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "LVA8")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "LVA10")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "LVA11")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "A11")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "A10")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "A8")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "A7")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "A6")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "A5")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "A9")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "A4")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 86.705 117.6275 90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U112"
			(at 0 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G125"
			(at 0 2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNum" "SN74LVC1G125DBVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "A0_OUT")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 252 "AA0")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 74.7925 114.88 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U203"
			(at 0 -4.199999 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.199999 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 250 "unconnected-(U203A-A0-Pad2)")
			(pinfunction "A0")
			(pintype "tri_state+no_connect")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 229 "unconnected-(U203A-A1-Pad3)")
			(pinfunction "A1")
			(pintype "tri_state+no_connect")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "_BG-3V")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 231 "_TS-3V")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "_BB-3V")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 227 "SIZ0-3V")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "SIZ1-3V")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "SIZ1")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "SIZ0")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "_BB")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 247 "_TS-CPU")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "R_W")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "_BG")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 248 "unconnected-(U203A-B1-Pad17)")
			(pinfunction "B1")
			(pintype "tri_state+no_connect")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 249 "unconnected-(U203A-B0-Pad18)")
			(pinfunction "B0")
			(pintype "tri_state+no_connect")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 56.25 47.545 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R103"
			(at -3.645 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k7"
			(at -7.355 0.03 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "/CPU/_MDIS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 123.463363 95.746637 -135)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R112"
			(at 0 -1.43 45)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 0 1.43 45)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 225)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 237 "/Card Connector/CLK40")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 225)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 236 "Net-(X100-OUT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.57 71.82 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C216"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.945 90.83 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C422"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 136.965 56.195 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U409F2"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "W25X20CLSN"
			(at 0 3.4 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25x20cl_revf%2020150806.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "/Card Connector/U409_SS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "/Card Connector/U409_SDO")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "~{WP}")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/Card Connector/U409_SDI")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/Card Connector/U409_SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "~{HOLD}")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 68.165 117.8 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C214"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 155.81 81.19 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C117"
			(at 1 -3.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 1 3.75 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 112.7825 82.34 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U103"
			(at 0 -4.199999 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.199999 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 276 "LVDA20")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "LVDA22")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 278 "LVDA25")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 280 "LVDA19")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 277 "LVDA23")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 282 "LVDA17")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 279 "LVDA15")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 275 "LVDA14")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "D14")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "D15")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "D17")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "D23")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "D19")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "D25")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "D22")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "D20")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 80.21 88.345 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C208"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 127.845 51.14)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R106"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 -2.81 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "/Card Connector/U409_SS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 164.68 43.79 -90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "CN400"
			(at 0.02 -2.91 90)
			(layer "F.SilkS")
		)
		(property "Value" "SPI"
			(at 0 15.03 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Fast Memory/U109_SDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Fast Memory/U109_SCK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/Fast Memory/U109_SDO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Fast Memory/U109_SS")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Fast Memory/U109_CRESET")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm_Pad"
		(layer "F.Cu")
		(at 195.01 42.58)
		(descr "Mounting Hole 3.5mm")
		(tags "mounting hole 3.5mm")
		(property "Reference" "H2"
			(at 0 -4.5 0)
			(layer "F.Fab")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.28 43.79 -90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "CN111"
			(at 0.02 -2.91 90)
			(layer "F.SilkS")
		)
		(property "Value" "SPI"
			(at 0 15.03 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/Card Connector/U409_SDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/Card Connector/U409_SCK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "/Card Connector/U409_SDO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "/Card Connector/U409_SS")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "/Card Connector/U409_CRESET")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm"
		(layer "F.Cu")
		(at 121.063274 99.191421 135)
		(descr "Miniature Crystal Clock Oscillator ECS 2520MV series, https://www.ecsxtal.com/store/pdf/ECS-2520MV.pdf")
		(tags "Miniature Crystal Clock Oscillator ECS 2520MV series SMD SMT HCMOS")
		(property "Reference" "X100"
			(at 2.280204 -0.029595 -135)
			(layer "F.SilkS")
		)
		(property "Value" "40MHz"
			(at 0 0 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/B400/XO32.pdf"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*SMD*EuroQuartz*XO32*3.2x2.5mm*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.725 -0.925 135)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.725 0.925 135)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at 0.725 0.925 135)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 236 "Net-(X100-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at 0.725 -0.925 135)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 93.165 117.6275 90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U113"
			(at 0 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G125"
			(at 0 2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNum" "SN74LVC1G125DBVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 255 "A1_OUT")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 253 "AA1")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 112.8075 71.345 180)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U102"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC245"
			(at 0 4.2 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "R_W-3V")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 274 "LVDA18")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 273 "LVDA13")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 270 "LVDA16")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 272 "LVDA12")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 269 "LVDA11")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 271 "LVDA10")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 268 "LVDA9")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 267 "LVDA8")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "D8")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "D9")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "D10")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "D11")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "D12")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "D16")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "D13")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "D18")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "_CPUBG")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 106.64 96.84 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C104"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:PGA179"
		(layer "F.Cu")
		(at 78.85 76.88 90)
		(property "Reference" "U100"
			(at 0 26.67 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MC68040"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "AmigaPCI:PGA179"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(clearance 0.15)
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 21.59 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.2)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 73 "A31")
			(pinfunction "A31")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at 19.05 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 16.51 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 13.97 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 11.43 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 8.89 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 6.35 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 3.81 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 1.27 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "D11")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at -1.27 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at -3.81 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -6.35 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "D14")
			(pinfunction "D14")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at -8.89 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "D15")
			(pinfunction "D15")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at -11.43 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "D17")
			(pinfunction "D17")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at -13.97 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "D19")
			(pinfunction "D19")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at -16.51 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "D20")
			(pinfunction "D20")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at -19.05 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "D21")
			(pinfunction "D21")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at -21.59 21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "D24")
			(pinfunction "D24")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 21.59 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "A29")
			(pinfunction "A29")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 19.05 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "21" thru_hole circle
			(at 16.51 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 13.97 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" thru_hole circle
			(at 11.43 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "24" thru_hole circle
			(at 8.89 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "25" thru_hole circle
			(at 6.35 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "D8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 3.81 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "27" thru_hole circle
			(at 1.27 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "28" thru_hole circle
			(at -1.27 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" thru_hole circle
			(at -3.81 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "D16")
			(pinfunction "D16")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at -6.35 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "D18")
			(pinfunction "D18")
			(pintype "bidirectional")
		)
		(pad "31" thru_hole circle
			(at -8.89 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "32" thru_hole circle
			(at -11.43 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "33" thru_hole circle
			(at -13.97 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" thru_hole circle
			(at -16.51 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "D22")
			(pinfunction "D22")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at -19.05 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "36" thru_hole circle
			(at -21.59 19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "D26")
			(pinfunction "D26")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole circle
			(at 21.59 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "A27")
			(pinfunction "A27")
			(pintype "bidirectional")
		)
		(pad "38" thru_hole circle
			(at 19.05 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "39" thru_hole circle
			(at 16.51 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "40" thru_hole circle
			(at 13.97 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "41" thru_hole circle
			(at 11.43 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "42" thru_hole circle
			(at 8.89 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" thru_hole circle
			(at 6.35 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "44" thru_hole circle
			(at 3.81 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "45" thru_hole circle
			(at 1.27 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" thru_hole circle
			(at -1.27 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "47" thru_hole circle
			(at -3.81 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "48" thru_hole circle
			(at -6.35 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "49" thru_hole circle
			(at -8.89 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "50" thru_hole circle
			(at -11.43 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "51" thru_hole circle
			(at -13.97 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "D23")
			(pinfunction "D23")
			(pintype "bidirectional")
		)
		(pad "52" thru_hole circle
			(at -16.51 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "D25")
			(pinfunction "D25")
			(pintype "bidirectional")
		)
		(pad "53" thru_hole circle
			(at -19.05 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "54" thru_hole circle
			(at -21.59 16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "D28")
			(pinfunction "D28")
			(pintype "bidirectional")
		)
		(pad "55" thru_hole circle
			(at 21.59 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "A24")
			(pinfunction "A24")
			(pintype "bidirectional")
		)
		(pad "56" thru_hole circle
			(at 19.05 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 16.51 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "A30")
			(pinfunction "A30")
			(pintype "bidirectional")
		)
		(pad "58" thru_hole circle
			(at -16.51 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "D27")
			(pinfunction "D27")
			(pintype "bidirectional")
		)
		(pad "59" thru_hole circle
			(at -19.05 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -21.59 13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "D31")
			(pinfunction "D31")
			(pintype "bidirectional")
		)
		(pad "61" thru_hole circle
			(at 21.59 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "A22")
			(pinfunction "A22")
			(pintype "bidirectional")
		)
		(pad "62" thru_hole circle
			(at 19.05 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "A26")
			(pinfunction "A26")
			(pintype "bidirectional")
		)
		(pad "63" thru_hole circle
			(at 16.51 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "A28")
			(pinfunction "A28")
			(pintype "bidirectional")
		)
		(pad "64" thru_hole circle
			(at -16.51 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "D29")
			(pinfunction "D29")
			(pintype "bidirectional")
		)
		(pad "65" thru_hole circle
			(at -19.05 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "D30")
			(pinfunction "D30")
			(pintype "bidirectional")
		)
		(pad "66" thru_hole circle
			(at -21.59 11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "A8")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "67" thru_hole circle
			(at 21.59 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "A21")
			(pinfunction "A21")
			(pintype "bidirectional")
		)
		(pad "68" thru_hole circle
			(at 19.05 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "69" thru_hole circle
			(at 16.51 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "A25")
			(pinfunction "A25")
			(pintype "bidirectional")
		)
		(pad "70" thru_hole circle
			(at -16.51 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "A9")
			(pinfunction "A9")
			(pintype "bidirectional")
		)
		(pad "71" thru_hole circle
			(at -19.05 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "72" thru_hole circle
			(at -21.59 8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "A7")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "73" thru_hole circle
			(at 21.59 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "A20")
			(pinfunction "A20")
			(pintype "bidirectional")
		)
		(pad "74" thru_hole circle
			(at 19.05 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "75" thru_hole circle
			(at 16.51 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "A23")
			(pinfunction "A23")
			(pintype "bidirectional")
		)
		(pad "76" thru_hole circle
			(at -16.51 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "A6")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "77" thru_hole circle
			(at -19.05 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "78" thru_hole circle
			(at -21.59 6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "A5")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "79" thru_hole circle
			(at 21.59 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "A18")
			(pinfunction "A18")
			(pintype "bidirectional")
		)
		(pad "80" thru_hole circle
			(at 19.05 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "81" thru_hole circle
			(at 16.51 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "82" thru_hole circle
			(at -16.51 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "83" thru_hole circle
			(at -19.05 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "84" thru_hole circle
			(at -21.59 3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "A4")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "85" thru_hole circle
			(at 21.59 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "A17")
			(pinfunction "A17")
			(pintype "bidirectional")
		)
		(pad "86" thru_hole circle
			(at 19.05 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "A19")
			(pinfunction "A19")
			(pintype "bidirectional")
		)
		(pad "87" thru_hole circle
			(at 16.51 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "88" thru_hole circle
			(at -16.51 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "89" thru_hole circle
			(at -19.05 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "A2")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "90" thru_hole circle
			(at -21.59 1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "A3")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "91" thru_hole circle
			(at 21.59 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "A15")
			(pinfunction "A15")
			(pintype "bidirectional")
		)
		(pad "92" thru_hole circle
			(at 19.05 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "A16")
			(pinfunction "A16")
			(pintype "bidirectional")
		)
		(pad "93" thru_hole circle
			(at 16.51 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "94" thru_hole circle
			(at -16.51 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "95" thru_hole circle
			(at -19.05 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "TM2")
			(pinfunction "TM2")
			(pintype "input")
		)
		(pad "96" thru_hole circle
			(at -21.59 -1.27 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A1")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "97" thru_hole circle
			(at 21.59 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "A14")
			(pinfunction "A14")
			(pintype "bidirectional")
		)
		(pad "98" thru_hole circle
			(at 19.05 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "99" thru_hole circle
			(at 16.51 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "100" thru_hole circle
			(at -16.51 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "101" thru_hole circle
			(at -19.05 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "102" thru_hole circle
			(at -21.59 -3.81 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "A0")
			(pinfunction "A0")
			(pintype "bidirectional")
		)
		(pad "103" thru_hole circle
			(at 21.59 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "A13")
			(pinfunction "A13")
			(pintype "bidirectional")
		)
		(pad "104" thru_hole circle
			(at 19.05 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "105" thru_hole circle
			(at 16.51 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "106" thru_hole circle
			(at -16.51 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "107" thru_hole circle
			(at -19.05 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "108" thru_hole circle
			(at -21.59 -6.35 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "TM1")
			(pinfunction "TM1")
			(pintype "output")
		)
		(pad "109" thru_hole circle
			(at 21.59 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "A12")
			(pinfunction "A12")
			(pintype "bidirectional")
		)
		(pad "110" thru_hole circle
			(at 19.05 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "111" thru_hole circle
			(at 16.51 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "A11")
			(pinfunction "A11")
			(pintype "bidirectional")
		)
		(pad "112" thru_hole circle
			(at -16.51 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "R_W")
			(pinfunction "R_W")
			(pintype "bidirectional")
		)
		(pad "113" thru_hole circle
			(at -19.05 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "114" thru_hole circle
			(at -21.59 -8.89 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "TM0")
			(pinfunction "TM0")
			(pintype "output")
		)
		(pad "115" thru_hole circle
			(at 21.59 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "A10")
			(pinfunction "A10")
			(pintype "bidirectional")
		)
		(pad "116" thru_hole circle
			(at 19.05 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "TT1")
			(pinfunction "TT1")
			(pintype "bidirectional")
		)
		(pad "117" thru_hole circle
			(at 16.51 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "TT0")
			(pinfunction "TT0")
			(pintype "bidirectional")
		)
		(pad "118" thru_hole circle
			(at -16.51 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "SIZ1")
			(pinfunction "SIZ1")
			(pintype "bidirectional")
		)
		(pad "119" thru_hole circle
			(at -19.05 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "SIZ0")
			(pinfunction "SIZ0")
			(pintype "bidirectional")
		)
		(pad "120" thru_hole circle
			(at -21.59 -11.43 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "unconnected-(U100A-TLN1-Pad120)")
			(pinfunction "TLN1")
			(pintype "output+no_connect")
		)
		(pad "121" thru_hole circle
			(at 21.59 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "UPA1")
			(pinfunction "UPA1")
			(pintype "output")
		)
		(pad "122" thru_hole circle
			(at 19.05 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "123" thru_hole circle
			(at 16.51 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "UPA0")
			(pinfunction "UPA0")
			(pintype "output")
		)
		(pad "124" thru_hole circle
			(at -16.51 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 208 "unconnected-(U100A-_MI-Pad124)")
			(pinfunction "_MI")
			(pintype "output+no_connect")
		)
		(pad "125" thru_hole circle
			(at -19.05 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "126" thru_hole circle
			(at -21.59 -13.97 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 205 "unconnected-(U100A-TLN0-Pad126)")
			(pinfunction "TLN0")
			(pintype "output+no_connect")
		)
		(pad "127" thru_hole circle
			(at 21.59 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 213 "unconnected-(U100A-_CIOUT-Pad127)")
			(pinfunction "_CIOUT")
			(pintype "output+no_connect")
		)
		(pad "128" thru_hole circle
			(at 19.05 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "129" thru_hole circle
			(at 16.51 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "_RSTOUT")
			(pinfunction "_RSTO")
			(pintype "output")
		)
		(pad "130" thru_hole circle
			(at 13.97 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "131" thru_hole circle
			(at 11.43 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "132" thru_hole circle
			(at 8.89 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "133" thru_hole circle
			(at 6.35 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 238 "BCLKA")
			(pinfunction "BCLK")
			(pintype "input")
		)
		(pad "134" thru_hole circle
			(at 3.81 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "135" thru_hole circle
			(at 1.27 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "PCLK")
			(pinfunction "PCLK")
			(pintype "input")
		)
		(pad "136" thru_hole circle
			(at -1.27 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "137" thru_hole circle
			(at -3.81 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "138" thru_hole circle
			(at -6.35 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "139" thru_hole circle
			(at -8.89 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "140" thru_hole circle
			(at -11.43 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "unconnected-(U100A-PST2-Pad140)")
			(pinfunction "PST2")
			(pintype "output+no_connect")
		)
		(pad "141" thru_hole circle
			(at -13.97 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(U100A-_TIP-Pad141)")
			(pinfunction "_TIP")
			(pintype "output+no_connect")
		)
		(pad "142" thru_hole circle
			(at -16.51 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 247 "_TS-CPU")
			(pinfunction "_TS")
			(pintype "bidirectional")
		)
		(pad "143" thru_hole circle
			(at -19.05 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "144" thru_hole circle
			(at -21.59 -16.51 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "unconnected-(U100A-_LOCKE-Pad144)")
			(pinfunction "_LOCKE")
			(pintype "output+no_connect")
		)
		(pad "145" thru_hole circle
			(at 21.59 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 214 "unconnected-(U100A-_IPEND-Pad145)")
			(pinfunction "_IPEND")
			(pintype "output+no_connect")
		)
		(pad "146" thru_hole circle
			(at 19.05 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "147" thru_hole circle
			(at 16.51 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "unconnected-(U100A-TDI-Pad147)")
			(pinfunction "TDI")
			(pintype "input+no_connect")
		)
		(pad "148" thru_hole circle
			(at 13.97 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "unconnected-(U100A-TCK-Pad148)")
			(pinfunction "TCK")
			(pintype "input+no_connect")
		)
		(pad "149" thru_hole circle
			(at 11.43 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "unconnected-(U100A-TMS-Pad149)")
			(pinfunction "TMS")
			(pintype "input+no_connect")
		)
		(pad "150" thru_hole circle
			(at 8.89 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/CPU/_MDIS")
			(pinfunction "_MDIS")
			(pintype "input")
		)
		(pad "151" thru_hole circle
			(at 6.35 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "_CPURST")
			(pinfunction "_RSTI")
			(pintype "input")
		)
		(pad "152" thru_hole circle
			(at 3.81 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "153" thru_hole circle
			(at 1.27 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "154" thru_hole circle
			(at -1.27 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "155" thru_hole circle
			(at -3.81 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "_TBI-CPU")
			(pinfunction "_TBI")
			(pintype "input")
		)
		(pad "156" thru_hole circle
			(at -6.35 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/CPU/SC1")
			(pinfunction "SC1")
			(pintype "bidirectional")
		)
		(pad "157" thru_hole circle
			(at -8.89 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 299 "_TEA-CPU")
			(pinfunction "_TEA")
			(pintype "input")
		)
		(pad "158" thru_hole circle
			(at -11.43 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "unconnected-(U100A-PST1-Pad158)")
			(pinfunction "PST1")
			(pintype "output+no_connect")
		)
		(pad "159" thru_hole circle
			(at -13.97 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "160" thru_hole circle
			(at -16.51 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "161" thru_hole circle
			(at -19.05 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "162" thru_hole circle
			(at -21.59 -19.05 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "_LOCK")
			(pinfunction "_LOCK")
			(pintype "output")
		)
		(pad "163" thru_hole circle
			(at 19.05 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/CPU/TDO")
			(pinfunction "TDO")
			(pintype "output")
		)
		(pad "164" thru_hole circle
			(at 16.51 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "unconnected-(U100A-_TRST-Pad164)")
			(pinfunction "_TRST")
			(pintype "input+no_connect")
		)
		(pad "165" thru_hole circle
			(at 13.97 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "166" thru_hole circle
			(at 11.43 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/CPU/_CDIS")
			(pinfunction "_CDIS")
			(pintype "input")
		)
		(pad "167" thru_hole circle
			(at 8.89 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "_IPL2")
			(pinfunction "_IPL2")
			(pintype "input")
		)
		(pad "168" thru_hole circle
			(at 6.35 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "_IPL1")
			(pinfunction "_IPL1")
			(pintype "input")
		)
		(pad "169" thru_hole circle
			(at 3.81 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "_IPL0")
			(pinfunction "_IPL0")
			(pintype "input")
		)
		(pad "170" thru_hole circle
			(at 1.27 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 209 "unconnected-(U100A-DLE-Pad170)")
			(pinfunction "DLE")
			(pintype "input+no_connect")
		)
		(pad "171" thru_hole circle
			(at -1.27 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "_TCI-CPU")
			(pinfunction "_TCI")
			(pintype "input")
		)
		(pad "172" thru_hole circle
			(at -3.81 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "_AVEC")
			(pintype "input")
		)
		(pad "173" thru_hole circle
			(at -6.35 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/CPU/SC0")
			(pinfunction "SC0")
			(pintype "bidirectional")
		)
		(pad "174" thru_hole circle
			(at -8.89 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "_BG")
			(pinfunction "_BG")
			(pintype "output")
		)
		(pad "175" thru_hole circle
			(at -11.43 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 246 "_TA-CPU")
			(pinfunction "_TA")
			(pintype "bidirectional")
		)
		(pad "176" thru_hole circle
			(at -13.97 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 204 "unconnected-(U100A-PST0-Pad176)")
			(pinfunction "PST0")
			(pintype "output+no_connect")
		)
		(pad "177" thru_hole circle
			(at -16.51 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "unconnected-(U100A-PST3-Pad177)")
			(pinfunction "PST3")
			(pintype "output+no_connect")
		)
		(pad "178" thru_hole circle
			(at -19.05 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "_BB")
			(pinfunction "_BB")
			(pintype "bidirectional")
		)
		(pad "179" thru_hole circle
			(at -21.59 -21.59 90)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "_BR")
			(pinfunction "_BR")
			(pintype "input")
		)
	)
	(footprint "AmigaPCI:TSOP-II-86"
		(layer "F.Cu")
		(at 196.1 97.33)
		(descr "54-lead TSOP typ II package")
		(tags "TSOPII TSOP2")
		(property "Reference" "U402"
			(at 0 -12.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "SDRAM(16Mx32)"
			(at 0 12.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "AmigaPCI:TSOP-II-86"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/42-45R-S-32160F.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16M x 32 bit Synchronous DRAM (SDRAM), TSOP II 86pin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(clearance 0.1)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5.75 -10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -5.75 -10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 266 "LVDA3")
			(pinfunction "DQ0")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -5.75 -9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -5.75 -9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 264 "LVDA0")
			(pinfunction "DQ1")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -5.75 -8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 260 "LVDA1")
			(pinfunction "DQ2")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -5.75 -8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -5.75 -7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 265 "LVDA4")
			(pinfunction "DQ3")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -5.75 -7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 261 "LVDA2")
			(pinfunction "DQ4")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -5.75 -6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -5.75 -6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 262 "LVDA5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -5.75 -5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 259 "LVDA6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -5.75 -5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -5.75 -4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 257 "LVDA7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -5.75 -4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "unconnected-(U402-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd rect
			(at -5.75 -3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -5.75 -3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "_LLBE")
			(pinfunction "DQM0")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -5.75 -2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "_EMWE")
			(pinfunction "_WE")
			(pintype "input")
		)
		(pad "18" smd rect
			(at -5.75 -2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "_EMCAS")
			(pinfunction "_CAS")
			(pintype "input")
		)
		(pad "19" smd rect
			(at -5.75 -1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "_EMRAS")
			(pinfunction "_RAS")
			(pintype "input")
		)
		(pad "20" smd rect
			(at -5.75 -1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "_EM1CS")
			(pinfunction "_CS")
			(pintype "input")
		)
		(pad "21" smd rect
			(at -5.75 -0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "EMA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "22" smd rect
			(at -5.75 0)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 290 "BANK0")
			(pinfunction "BA0")
			(pintype "input")
		)
		(pad "23" smd rect
			(at -5.75 0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 289 "BANK1")
			(pinfunction "BA1")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -5.75 1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "EMA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "25" smd rect
			(at -5.75 1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "EMA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -5.75 2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "EMA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" smd rect
			(at -5.75 2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "EMA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" smd rect
			(at -5.75 3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "_UMBE")
			(pinfunction "DQM2")
			(pintype "input")
		)
		(pad "29" smd rect
			(at -5.75 3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "30" smd rect
			(at -5.75 4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 221 "unconnected-(U402-NC-Pad30)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "31" smd rect
			(at -5.75 4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 270 "LVDA16")
			(pinfunction "DQ16")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -5.75 5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at -5.75 5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 282 "LVDA17")
			(pinfunction "DQ17")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at -5.75 6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 274 "LVDA18")
			(pinfunction "DQ18")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at -5.75 6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at -5.75 7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 280 "LVDA19")
			(pinfunction "DQ19")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at -5.75 7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 276 "LVDA20")
			(pinfunction "DQ20")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at -5.75 8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at -5.75 8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 292 "LVDA21")
			(pinfunction "DQ21")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at -5.75 9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "LVDA22")
			(pinfunction "DQ22")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at -5.75 9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at -5.75 10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 277 "LVDA23")
			(pinfunction "DQ23")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at -5.75 10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 5.75 10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "45" smd rect
			(at 5.75 10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 293 "LVDA24")
			(pinfunction "DQ24")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 5.75 9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "47" smd rect
			(at 5.75 9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 278 "LVDA25")
			(pinfunction "DQ25")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 5.75 8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 294 "LVDA26")
			(pinfunction "DQ26")
			(pintype "bidirectional")
		)
		(pad "49" smd rect
			(at 5.75 8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "50" smd rect
			(at 5.75 7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 284 "LVDA27")
			(pinfunction "DQ27")
			(pintype "bidirectional")
		)
		(pad "51" smd rect
			(at 5.75 7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 295 "LVDA28")
			(pinfunction "DQ28")
			(pintype "bidirectional")
		)
		(pad "52" smd rect
			(at 5.75 6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 5.75 6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 286 "LVDA29")
			(pinfunction "DQ29")
			(pintype "bidirectional")
		)
		(pad "54" smd rect
			(at 5.75 5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 283 "LVDA30")
			(pinfunction "DQ30")
			(pintype "bidirectional")
		)
		(pad "55" smd rect
			(at 5.75 5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "56" smd rect
			(at 5.75 4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "LVDA31")
			(pinfunction "DQ31")
			(pintype "bidirectional")
		)
		(pad "57" smd rect
			(at 5.75 4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 222 "unconnected-(U402-NC-Pad57)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "58" smd rect
			(at 5.75 3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "59" smd rect
			(at 5.75 3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 145 "_UUBE")
			(pinfunction "DQM3")
			(pintype "input")
		)
		(pad "60" smd rect
			(at 5.75 2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 144 "EMA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "61" smd rect
			(at 5.75 2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "EMA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "62" smd rect
			(at 5.75 1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "EMA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "63" smd rect
			(at 5.75 1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "EMA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "64" smd rect
			(at 5.75 0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "EMA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 5.75 0)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "EMA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "66" smd rect
			(at 5.75 -0.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "EMA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "67" smd rect
			(at 5.75 -1)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "EMCLKE")
			(pinfunction "CKE")
			(pintype "input")
		)
		(pad "68" smd rect
			(at 5.75 -1.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 343 "RAMCLKA")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "69" smd rect
			(at 5.75 -2)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "EMA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "70" smd rect
			(at 5.75 -2.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "unconnected-(U402-NC-Pad70)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "71" smd rect
			(at 5.75 -3)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 154 "_LMBE")
			(pinfunction "DQM1")
			(pintype "input")
		)
		(pad "72" smd rect
			(at 5.75 -3.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "73" smd rect
			(at 5.75 -4)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 220 "unconnected-(U402-NC-Pad73)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "74" smd rect
			(at 5.75 -4.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 279 "LVDA15")
			(pinfunction "DQ8")
			(pintype "bidirectional")
		)
		(pad "75" smd rect
			(at 5.75 -5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "76" smd rect
			(at 5.75 -5.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 275 "LVDA14")
			(pinfunction "DQ9")
			(pintype "bidirectional")
		)
		(pad "77" smd rect
			(at 5.75 -6)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 273 "LVDA13")
			(pinfunction "DQ10")
			(pintype "bidirectional")
		)
		(pad "78" smd rect
			(at 5.75 -6.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "79" smd rect
			(at 5.75 -7)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 272 "LVDA12")
			(pinfunction "DQ11")
			(pintype "bidirectional")
		)
		(pad "80" smd rect
			(at 5.75 -7.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 269 "LVDA11")
			(pinfunction "DQ12")
			(pintype "bidirectional")
		)
		(pad "81" smd rect
			(at 5.75 -8)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "82" smd rect
			(at 5.75 -8.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 271 "LVDA10")
			(pinfunction "DQ13")
			(pintype "bidirectional")
		)
		(pad "83" smd rect
			(at 5.75 -9)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 268 "LVDA9")
			(pinfunction "DQ14")
			(pintype "bidirectional")
		)
		(pad "84" smd rect
			(at 5.75 -9.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "85" smd rect
			(at 5.75 -10)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 267 "LVDA8")
			(pinfunction "DQ15")
			(pintype "bidirectional")
		)
		(pad "86" smd rect
			(at 5.75 -10.5)
			(size 1.51 0.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 82.21 111.785 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C140"
			(at 0 1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 163.905 48.73 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R401"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/Fast Memory/U109_CRESET")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 146.5 92.37 -45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R114"
			(at 3.764123 -0.035355 -45)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 7.594327 0 -45)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 315)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 239 "Net-(U111-IO3_14A_GBIN6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 315)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "BCLKC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 82.21 115.74 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C139"
			(at 0 -1.49 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121.045 75.13 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R118"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "22R"
			(at 3.615 -1.42 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 245 "Net-(U111-IO1_141_GBIN2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 291 "PCLK")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:48-BSSOP"
		(layer "F.Cu")
		(at 164.1275 110.2545 -90)
		(property "Reference" "U109"
			(at 0 -9.3525 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC16T245DLR"
			(at 7.5655 -0.1125 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Footprint" "AmigaPCI:48-BSSOP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "SN74LVC16T245DLR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DL48 DL48-M DL48-L")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.66725 -7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "BUFDIR")
			(pinfunction "1DIR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -4.66725 -6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "LVDB0")
			(pinfunction "1B1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.66725 -6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "LVDB3")
			(pinfunction "1B2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.66725 -5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -4.66725 -4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 297 "LVDB2")
			(pinfunction "1B3")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.66725 -4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "LVDB4")
			(pinfunction "1B4")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.66725 -3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -4.66725 -2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 307 "LVDB1")
			(pinfunction "1B5")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -4.66725 -2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 306 "LVDB6")
			(pinfunction "1B6")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -4.66725 -1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -4.66725 -0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 318 "LVDB5")
			(pinfunction "1B7")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -4.66725 -0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 313 "LVDB7")
			(pinfunction "1B8")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -4.66725 0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 308 "LVDB8")
			(pinfunction "2B1")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -4.66725 0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 312 "LVDB9")
			(pinfunction "2B2")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -4.66725 1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -4.66725 2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 310 "LVDB11")
			(pinfunction "2B3")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -4.66725 2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 317 "LVDB10")
			(pinfunction "2B4")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -4.66725 3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -4.66725 4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "LVDB16")
			(pinfunction "2B5")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -4.66725 4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 316 "LVDB12")
			(pinfunction "2B6")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at -4.66725 5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd rect
			(at -4.66725 6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 314 "LVDB18")
			(pinfunction "2B7")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -4.66725 6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 296 "LVDB13")
			(pinfunction "2B8")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -4.66725 7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "BUFDIR")
			(pinfunction "2DIR")
			(pintype "input")
		)
		(pad "25" smd rect
			(at 4.66725 7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "_BUFEN")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "26" smd rect
			(at 4.66725 6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "DA13")
			(pinfunction "2A8")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 4.66725 6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "DA18")
			(pinfunction "2A7")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 4.66725 5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at 4.66725 4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 263 "DA12")
			(pinfunction "2A6")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 4.66725 4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "DA16")
			(pinfunction "2A5")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 4.66725 3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at 4.66725 2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "DA10")
			(pinfunction "2A4")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 4.66725 2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "DA11")
			(pinfunction "2A3")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 4.66725 1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" smd rect
			(at 4.66725 0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "DA9")
			(pinfunction "2A2")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 4.66725 0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 122 "DA8")
			(pinfunction "2A1")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 4.66725 -0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "DA7")
			(pinfunction "1A8")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 4.66725 -0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "DA5")
			(pinfunction "1A7")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 4.66725 -1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd rect
			(at 4.66725 -2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "DA6")
			(pinfunction "1A6")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 4.66725 -2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 140 "DA1")
			(pinfunction "1A5")
			(pintype "bidirectional")
		)
		(pad "42" smd rect
			(at 4.66725 -3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "43" smd rect
			(at 4.66725 -4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "DA4")
			(pinfunction "1A4")
			(pintype "bidirectional")
		)
		(pad "44" smd rect
			(at 4.66725 -4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "DA2")
			(pinfunction "1A3")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 4.66725 -5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd rect
			(at 4.66725 -6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "DA3")
			(pinfunction "1A2")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 4.66725 -6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 142 "DA0")
			(pinfunction "1A1")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 4.66725 -7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "_BUFEN")
			(pinfunction "1OE")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-48_7.5x15.9mm_P0.635mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 93.14 112.16 90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U115"
			(at 0 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LVC1G125"
			(at 0 2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g125.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNum" "SN74LVC1G125DBVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 256 "_DMA")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 253 "AA1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "A1")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 157.45 56.195 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U400F1"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "W25X20CLSN"
			(at 0 3.4 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25x20cl_revf%2020150806.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Fast Memory/U109_SS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "/Fast Memory/U109_SDO")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "~{WP}")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/Fast Memory/U109_SDI")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Fast Memory/U109_SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "~{HOLD}")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:48-BSSOP"
		(layer "F.Cu")
		(at 137.79 110.2545 -90)
		(property "Reference" "U110"
			(at 0 -9.55 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC16T245DLR"
			(at 7.6355 -0.01 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Footprint" "AmigaPCI:48-BSSOP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "SN74LVC16T245DLR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DL48 DL48-M DL48-L")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.66725 -7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "BUFDIR")
			(pinfunction "1DIR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -4.66725 -6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "LVDB17")
			(pinfunction "1B1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.66725 -6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 321 "LVDB15")
			(pinfunction "1B2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.66725 -5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -4.66725 -4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 328 "LVDB14")
			(pinfunction "1B3")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.66725 -4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 322 "LVDB25")
			(pinfunction "1B4")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.66725 -3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -4.66725 -2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 326 "LVDB19")
			(pinfunction "1B5")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -4.66725 -2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 336 "LVDB23")
			(pinfunction "1B6")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -4.66725 -1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -4.66725 -0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 332 "LVDB20")
			(pinfunction "1B7")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -4.66725 -0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 329 "LVDB22")
			(pinfunction "1B8")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -4.66725 0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 330 "LVDB29")
			(pinfunction "2B1")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -4.66725 0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 325 "LVDB27")
			(pinfunction "2B2")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -4.66725 1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -4.66725 2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 331 "LVDB31")
			(pinfunction "2B3")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -4.66725 2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 335 "LVDB30")
			(pinfunction "2B4")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -4.66725 3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -4.66725 4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 333 "LVDB21")
			(pinfunction "2B5")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -4.66725 4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 334 "LVDB26")
			(pinfunction "2B6")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at -4.66725 5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd rect
			(at -4.66725 6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 323 "LVDB24")
			(pinfunction "2B7")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -4.66725 6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 327 "LVDB28")
			(pinfunction "2B8")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -4.66725 7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "BUFDIR")
			(pinfunction "2DIR")
			(pintype "input")
		)
		(pad "25" smd rect
			(at 4.66725 7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "_BUFEN")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "26" smd rect
			(at 4.66725 6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "DA28")
			(pinfunction "2A8")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 4.66725 6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 126 "DA24")
			(pinfunction "2A7")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 4.66725 5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at 4.66725 4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "DA26")
			(pinfunction "2A6")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 4.66725 4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 125 "DA21")
			(pinfunction "2A5")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 4.66725 3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at 4.66725 2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "DA30")
			(pinfunction "2A4")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 4.66725 2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 130 "DA31")
			(pinfunction "2A3")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 4.66725 1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" smd rect
			(at 4.66725 0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "DA27")
			(pinfunction "2A2")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 4.66725 0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 166 "DA29")
			(pinfunction "2A1")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 4.66725 -0.3175 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "DA22")
			(pinfunction "1A8")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 4.66725 -0.9525 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "DA20")
			(pinfunction "1A7")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 4.66725 -1.5875 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd rect
			(at 4.66725 -2.2225 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "DA23")
			(pinfunction "1A6")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 4.66725 -2.8575 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "DA19")
			(pinfunction "1A5")
			(pintype "bidirectional")
		)
		(pad "42" smd rect
			(at 4.66725 -3.4925 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "43" smd rect
			(at 4.66725 -4.1275 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "DA25")
			(pinfunction "1A4")
			(pintype "bidirectional")
		)
		(pad "44" smd rect
			(at 4.66725 -4.7625 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "DA14")
			(pinfunction "1A3")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 4.66725 -5.3975 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd rect
			(at 4.66725 -6.0325 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 153 "DA15")
			(pinfunction "1A2")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 4.66725 -6.6675 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "DA17")
			(pinfunction "1A1")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 4.66725 -7.3025 270)
			(size 2.0447 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "_BUFEN")
			(pinfunction "1OE")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-48_7.5x15.9mm_P0.635mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 82.65 65.685 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C201"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 66.98 88.4 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C206"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 73.25 125.415 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R119"
			(at 3.655 -0.12 90)
			(layer "B.SilkS")
		)
		(property "Value" "22R"
			(at -0.005 1.65 90)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 298 "Net-(CN100-Pin_c16)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 93 "SIZ0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 124.521992 82.221992 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C123"
			(at -3.700986 0.091924 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 130.141992 88.288008 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C131"
			(at -3.645854 0.014142 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 45)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U111-VCCPLL1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U111-GNDPLL1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 179.138008 81.098008 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C403"
			(at 3.616133 0.007071 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 128.83 77.47 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C122"
			(at -3.57796 0.028284 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 165.09 62.325 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C107"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 166.07 106.965 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C120"
			(at -3.685 -0.01 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 112.09 110.11 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C105"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 109.295 64.1 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C101"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 205.565 89.33)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C413"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 135.88 106.925 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C118"
			(at -3.765 -0.02 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 139.138008 76.481992 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C134"
			(at -3.723636 0.035355 -135)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 3.389859 0.106066 -135)
			(layer "B.SilkS")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U111-VCCPLL0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U111-GNDPLL0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 144.038008 81.678008 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C124"
			(at -3.849478 0.014142 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 125.601992 81.141992 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C126"
			(at -3.700986 0.091924 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 175 64.15 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C108"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 92.05 117.53 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C142"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 176.961992 83.251992 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C406"
			(at -3.794346 0.13435 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 160.64 106.955 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C112"
			(at -3.685 -0.01 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AmigaPCI:DIN41612_R_3x40_Male_Vertical_THT"
		(layer "B.Cu")
		(at 89.01 124.08 -90)
		(descr "DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
		(tags "DIN 41612 IEC 60603 R")
		(property "Reference" "CN100"
			(at 2.54 9.13 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "DIN41612_03x40"
			(at 2.54 -87.87 90)
			(layer "B.Fab")
		)
		(property "Footprint" "AmigaPCI:DIN41612_R_3x40_Male_Vertical_THT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "DIN41612 connector, three row, 03x40"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIN41612*2x*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(clearance 0.1)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 2.24 -104.69 270)
			(size 2.85 2.85)
			(drill 2.85)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.24 5.63 270)
			(size 2.85 2.85)
			(drill 2.85)
			(layers "*.Cu" "*.Mask")
		)
		(pad "a1" thru_hole roundrect
			(at 0 0 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.16129)
			(net 16 "PORTSIZE")
			(pinfunction "Pin_a1")
			(pintype "passive")
		)
		(pad "a2" thru_hole circle
			(at 0 -2.54 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "A12")
			(pinfunction "Pin_a2")
			(pintype "passive")
		)
		(pad "a3" thru_hole circle
			(at 0 -5.08 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "A14")
			(pinfunction "Pin_a3")
			(pintype "passive")
		)
		(pad "a4" thru_hole circle
			(at 0 -7.62 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "AA1")
			(pinfunction "Pin_a4")
			(pintype "passive")
		)
		(pad "a5" thru_hole circle
			(at 0 -10.16 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "A4")
			(pinfunction "Pin_a5")
			(pintype "passive")
		)
		(pad "a6" thru_hole circle
			(at 0 -12.7 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+1V2")
			(pinfunction "Pin_a6")
			(pintype "passive")
		)
		(pad "a7" thru_hole circle
			(at 0 -15.24 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_a7")
			(pintype "passive")
		)
		(pad "a8" thru_hole circle
			(at 0 -17.78 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "A6")
			(pinfunction "Pin_a8")
			(pintype "passive")
		)
		(pad "a9" thru_hole circle
			(at 0 -20.32 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "A8")
			(pinfunction "Pin_a9")
			(pintype "passive")
		)
		(pad "a10" thru_hole circle
			(at 0 -22.86 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "A11")
			(pinfunction "Pin_a10")
			(pintype "passive")
		)
		(pad "a11" thru_hole circle
			(at 0 -25.4 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "_BR")
			(pinfunction "Pin_a11")
			(pintype "passive")
		)
		(pad "a12" thru_hole circle
			(at 0 -27.94 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "TM0")
			(pinfunction "Pin_a12")
			(pintype "passive")
		)
		(pad "a13" thru_hole circle
			(at 0 -30.48 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "TM2")
			(pinfunction "Pin_a13")
			(pintype "passive")
		)
		(pad "a14" thru_hole circle
			(at 0 -33.02 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "DA26")
			(pinfunction "Pin_a14")
			(pintype "passive")
		)
		(pad "a15" thru_hole circle
			(at 0 -35.56 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "DA31")
			(pinfunction "Pin_a15")
			(pintype "passive")
		)
		(pad "a16" thru_hole circle
			(at 0 -38.1 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "DA29")
			(pinfunction "Pin_a16")
			(pintype "passive")
		)
		(pad "a17" thru_hole circle
			(at 0 -40.64 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 347 "Net-(CN100-Pin_a17)")
			(pinfunction "Pin_a17")
			(pintype "passive")
		)
		(pad "a18" thru_hole circle
			(at 0 -43.18 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 164 "DA20")
			(pinfunction "Pin_a18")
			(pintype "passive")
		)
		(pad "a19" thru_hole circle
			(at 0 -45.72 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 155 "DA25")
			(pinfunction "Pin_a19")
			(pintype "passive")
		)
		(pad "a20" thru_hole circle
			(at 0 -48.26 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "DA17")
			(pinfunction "Pin_a20")
			(pintype "passive")
		)
		(pad "a21" thru_hole circle
			(at 0 -50.8 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_a21")
			(pintype "passive")
		)
		(pad "a22" thru_hole circle
			(at 0 -53.34 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_a22")
			(pintype "passive")
		)
		(pad "a23" thru_hole circle
			(at 0 -55.88 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "_TBI")
			(pinfunction "Pin_a23")
			(pintype "passive")
		)
		(pad "a24" thru_hole circle
			(at 0 -58.42 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_a24")
			(pintype "passive")
		)
		(pad "a25" thru_hole circle
			(at 0 -60.96 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_a25")
			(pintype "passive")
		)
		(pad "a26" thru_hole circle
			(at 0 -63.5 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_a26")
			(pintype "passive")
		)
		(pad "a27" thru_hole circle
			(at 0 -66.04 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "DA8")
			(pinfunction "Pin_a27")
			(pintype "passive")
		)
		(pad "a28" thru_hole circle
			(at 0 -68.58 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "BCLKC")
			(pinfunction "Pin_a28")
			(pintype "passive")
		)
		(pad "a29" thru_hole circle
			(at 0 -71.12 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_a29")
			(pintype "passive")
		)
		(pad "a30" thru_hole circle
			(at 0 -73.66 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_a30")
			(pintype "passive")
		)
		(pad "a31" thru_hole circle
			(at 0 -76.2 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 225 "DA2")
			(pinfunction "Pin_a31")
			(pintype "passive")
		)
		(pad "a32" thru_hole circle
			(at 0 -78.74 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "DA0")
			(pinfunction "Pin_a32")
			(pintype "passive")
		)
		(pad "a33" thru_hole circle
			(at 0 -81.28 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_a33")
			(pintype "passive")
		)
		(pad "a34" thru_hole circle
			(at 0 -83.82 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_a34")
			(pintype "passive")
		)
		(pad "a35" thru_hole circle
			(at 0 -86.36 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "A22")
			(pinfunction "Pin_a35")
			(pintype "passive")
		)
		(pad "a36" thru_hole circle
			(at 0 -88.9 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "A24")
			(pinfunction "Pin_a36")
			(pintype "passive")
		)
		(pad "a37" thru_hole circle
			(at 0 -91.44 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_a37")
			(pintype "passive")
		)
		(pad "a38" thru_hole circle
			(at 0 -93.98 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_a38")
			(pintype "passive")
		)
		(pad "a39" thru_hole circle
			(at 0 -96.52 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "A23")
			(pinfunction "Pin_a39")
			(pintype "passive")
		)
		(pad "a40" thru_hole circle
			(at 0 -99.06 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "A18")
			(pinfunction "Pin_a40")
			(pintype "passive")
		)
		(pad "b1" thru_hole circle
			(at 2.54 0 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "_BB")
			(pinfunction "Pin_b1")
			(pintype "passive")
		)
		(pad "b2" thru_hole circle
			(at 2.54 -2.54 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "A13")
			(pinfunction "Pin_b2")
			(pintype "passive")
		)
		(pad "b3" thru_hole circle
			(at 2.54 -5.08 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "AA0")
			(pinfunction "Pin_b3")
			(pintype "passive")
		)
		(pad "b4" thru_hole circle
			(at 2.54 -7.62 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "A2")
			(pinfunction "Pin_b4")
			(pintype "passive")
		)
		(pad "b5" thru_hole circle
			(at 2.54 -10.16 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_b5")
			(pintype "passive")
		)
		(pad "b6" thru_hole circle
			(at 2.54 -12.7 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_b6")
			(pintype "passive")
		)
		(pad "b7" thru_hole circle
			(at 2.54 -15.24 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_b7")
			(pintype "passive")
		)
		(pad "b8" thru_hole circle
			(at 2.54 -17.78 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "A5")
			(pinfunction "Pin_b8")
			(pintype "passive")
		)
		(pad "b9" thru_hole circle
			(at 2.54 -20.32 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "A7")
			(pinfunction "Pin_b9")
			(pintype "passive")
		)
		(pad "b10" thru_hole circle
			(at 2.54 -22.86 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "A10")
			(pinfunction "Pin_b10")
			(pintype "passive")
		)
		(pad "b11" thru_hole circle
			(at 2.54 -25.4 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "_LOCK")
			(pinfunction "Pin_b11")
			(pintype "passive")
		)
		(pad "b12" thru_hole circle
			(at 2.54 -27.94 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "Net-(CN100-Pin_b12)")
			(pinfunction "Pin_b12")
			(pintype "passive")
		)
		(pad "b13" thru_hole circle
			(at 2.54 -30.48 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "DA28")
			(pinfunction "Pin_b13")
			(pintype "passive")
		)
		(pad "b14" thru_hole circle
			(at 2.54 -33.02 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "DA24")
			(pinfunction "Pin_b14")
			(pintype "passive")
		)
		(pad "b15" thru_hole circle
			(at 2.54 -35.56 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "DA30")
			(pinfunction "Pin_b15")
			(pintype "passive")
		)
		(pad "b16" thru_hole circle
			(at 2.54 -38.1 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "DA27")
			(pinfunction "Pin_b16")
			(pintype "passive")
		)
		(pad "b17" thru_hole circle
			(at 2.54 -40.64 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "_TS")
			(pinfunction "Pin_b17")
			(pintype "passive")
		)
		(pad "b18" thru_hole circle
			(at 2.54 -43.18 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "DA22")
			(pinfunction "Pin_b18")
			(pintype "passive")
		)
		(pad "b19" thru_hole circle
			(at 2.54 -45.72 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "DA19")
			(pinfunction "Pin_b19")
			(pintype "passive")
		)
		(pad "b20" thru_hole circle
			(at 2.54 -48.26 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "DA15")
			(pinfunction "Pin_b20")
			(pintype "passive")
		)
		(pad "b21" thru_hole circle
			(at 2.54 -50.8 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "_TACK")
			(pinfunction "Pin_b21")
			(pintype "passive")
		)
		(pad "b22" thru_hole circle
			(at 2.54 -53.34 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "CDONE")
			(pinfunction "Pin_b22")
			(pintype "passive")
		)
		(pad "b23" thru_hole circle
			(at 2.54 -55.88 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 216 "_INT6")
			(pinfunction "Pin_b23")
			(pintype "passive")
		)
		(pad "b24" thru_hole circle
			(at 2.54 -58.42 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 159 "DA18")
			(pinfunction "Pin_b24")
			(pintype "passive")
		)
		(pad "b25" thru_hole circle
			(at 2.54 -60.96 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "DA16")
			(pinfunction "Pin_b25")
			(pintype "passive")
		)
		(pad "b26" thru_hole circle
			(at 2.54 -63.5 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "DA11")
			(pinfunction "Pin_b26")
			(pintype "passive")
		)
		(pad "b27" thru_hole circle
			(at 2.54 -66.04 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "DA9")
			(pinfunction "Pin_b27")
			(pintype "passive")
		)
		(pad "b28" thru_hole circle
			(at 2.54 -68.58 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "_RESET")
			(pinfunction "Pin_b28")
			(pintype "passive")
		)
		(pad "b29" thru_hole circle
			(at 2.54 -71.12 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "_IPL2")
			(pinfunction "Pin_b29")
			(pintype "passive")
		)
		(pad "b30" thru_hole circle
			(at 2.54 -73.66 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 230 "DA6")
			(pinfunction "Pin_b30")
			(pintype "passive")
		)
		(pad "b31" thru_hole circle
			(at 2.54 -76.2 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 152 "DA4")
			(pinfunction "Pin_b31")
			(pintype "passive")
		)
		(pad "b32" thru_hole circle
			(at 2.54 -78.74 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "DA3")
			(pinfunction "Pin_b32")
			(pintype "passive")
		)
		(pad "b33" thru_hole circle
			(at 2.54 -81.28 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "TT1")
			(pinfunction "Pin_b33")
			(pintype "passive")
		)
		(pad "b34" thru_hole circle
			(at 2.54 -83.82 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "UPA1")
			(pinfunction "Pin_b34")
			(pintype "passive")
		)
		(pad "b35" thru_hole circle
			(at 2.54 -86.36 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "A26")
			(pinfunction "Pin_b35")
			(pintype "passive")
		)
		(pad "b36" thru_hole circle
			(at 2.54 -88.9 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "A30")
			(pinfunction "Pin_b36")
			(pintype "passive")
		)
		(pad "b37" thru_hole circle
			(at 2.54 -91.44 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "A31")
			(pinfunction "Pin_b37")
			(pintype "passive")
		)
		(pad "b38" thru_hole circle
			(at 2.54 -93.98 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "A25")
			(pinfunction "Pin_b38")
			(pintype "passive")
		)
		(pad "b39" thru_hole circle
			(at 2.54 -96.52 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "A20")
			(pinfunction "Pin_b39")
			(pintype "passive")
		)
		(pad "b40" thru_hole circle
			(at 2.54 -99.06 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "A17")
			(pinfunction "Pin_b40")
			(pintype "passive")
		)
		(pad "c1" thru_hole circle
			(at 5.08 0 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c1")
			(pintype "passive")
		)
		(pad "c2" thru_hole circle
			(at 5.08 -2.54 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c2")
			(pintype "passive")
		)
		(pad "c3" thru_hole circle
			(at 5.08 -5.08 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "A15")
			(pinfunction "Pin_c3")
			(pintype "passive")
		)
		(pad "c4" thru_hole circle
			(at 5.08 -7.62 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "A3")
			(pinfunction "Pin_c4")
			(pintype "passive")
		)
		(pad "c5" thru_hole circle
			(at 5.08 -10.16 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_c5")
			(pintype "passive")
		)
		(pad "c6" thru_hole circle
			(at 5.08 -12.7 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 233 "_INT2")
			(pinfunction "Pin_c6")
			(pintype "passive")
		)
		(pad "c7" thru_hole circle
			(at 5.08 -15.24 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "_CPUCONF")
			(pinfunction "Pin_c7")
			(pintype "passive")
		)
		(pad "c8" thru_hole circle
			(at 5.08 -17.78 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "A9")
			(pinfunction "Pin_c8")
			(pintype "passive")
		)
		(pad "c9" thru_hole circle
			(at 5.08 -20.32 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c9")
			(pintype "passive")
		)
		(pad "c10" thru_hole circle
			(at 5.08 -22.86 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c10")
			(pintype "passive")
		)
		(pad "c11" thru_hole circle
			(at 5.08 -25.4 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "_CPURST")
			(pinfunction "Pin_c11")
			(pintype "passive")
		)
		(pad "c12" thru_hole circle
			(at 5.08 -27.94 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "TM1")
			(pinfunction "Pin_c12")
			(pintype "passive")
		)
		(pad "c13" thru_hole circle
			(at 5.08 -30.48 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_c13")
			(pintype "passive")
		)
		(pad "c14" thru_hole circle
			(at 5.08 -33.02 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "Pin_c14")
			(pintype "passive")
		)
		(pad "c15" thru_hole circle
			(at 5.08 -35.56 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "DA21")
			(pinfunction "Pin_c15")
			(pintype "passive")
		)
		(pad "c16" thru_hole circle
			(at 5.08 -38.1 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 298 "Net-(CN100-Pin_c16)")
			(pinfunction "Pin_c16")
			(pintype "passive")
		)
		(pad "c17" thru_hole circle
			(at 5.08 -40.64 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c17")
			(pintype "passive")
		)
		(pad "c18" thru_hole circle
			(at 5.08 -43.18 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_c18")
			(pintype "passive")
		)
		(pad "c19" thru_hole circle
			(at 5.08 -45.72 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "DA23")
			(pinfunction "Pin_c19")
			(pintype "passive")
		)
		(pad "c20" thru_hole circle
			(at 5.08 -48.26 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "DA14")
			(pinfunction "Pin_c20")
			(pintype "passive")
		)
		(pad "c21" thru_hole circle
			(at 5.08 -50.8 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "_TEA")
			(pinfunction "Pin_c21")
			(pintype "passive")
		)
		(pad "c22" thru_hole circle
			(at 5.08 -53.34 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "_BG")
			(pinfunction "Pin_c22")
			(pintype "passive")
		)
		(pad "c23" thru_hole circle
			(at 5.08 -55.88 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "_TCI")
			(pinfunction "Pin_c23")
			(pintype "passive")
		)
		(pad "c24" thru_hole circle
			(at 5.08 -58.42 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 224 "DA13")
			(pinfunction "Pin_c24")
			(pintype "passive")
		)
		(pad "c25" thru_hole circle
			(at 5.08 -60.96 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 263 "DA12")
			(pinfunction "Pin_c25")
			(pintype "passive")
		)
		(pad "c26" thru_hole circle
			(at 5.08 -63.5 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 234 "DA10")
			(pinfunction "Pin_c26")
			(pintype "passive")
		)
		(pad "c27" thru_hole circle
			(at 5.08 -66.04 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "_IPL0")
			(pinfunction "Pin_c27")
			(pintype "passive")
		)
		(pad "c28" thru_hole circle
			(at 5.08 -68.58 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "_IPL1")
			(pinfunction "Pin_c28")
			(pintype "passive")
		)
		(pad "c29" thru_hole circle
			(at 5.08 -71.12 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "DA7")
			(pinfunction "Pin_c29")
			(pintype "passive")
		)
		(pad "c30" thru_hole circle
			(at 5.08 -73.66 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 158 "DA5")
			(pinfunction "Pin_c30")
			(pintype "passive")
		)
		(pad "c31" thru_hole circle
			(at 5.08 -76.2 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "DA1")
			(pinfunction "Pin_c31")
			(pintype "passive")
		)
		(pad "c32" thru_hole circle
			(at 5.08 -78.74 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "TT0")
			(pinfunction "Pin_c32")
			(pintype "passive")
		)
		(pad "c33" thru_hole circle
			(at 5.08 -81.28 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "UPA0")
			(pinfunction "Pin_c33")
			(pintype "passive")
		)
		(pad "c34" thru_hole circle
			(at 5.08 -83.82 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "_RSTOUT")
			(pinfunction "Pin_c34")
			(pintype "passive")
		)
		(pad "c35" thru_hole circle
			(at 5.08 -86.36 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "A28")
			(pinfunction "Pin_c35")
			(pintype "passive")
		)
		(pad "c36" thru_hole circle
			(at 5.08 -88.9 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "A29")
			(pinfunction "Pin_c36")
			(pintype "passive")
		)
		(pad "c37" thru_hole circle
			(at 5.08 -91.44 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "A27")
			(pinfunction "Pin_c37")
			(pintype "passive")
		)
		(pad "c38" thru_hole circle
			(at 5.08 -93.98 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "A21")
			(pinfunction "Pin_c38")
			(pintype "passive")
		)
		(pad "c39" thru_hole circle
			(at 5.08 -96.52 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "A19")
			(pinfunction "Pin_c39")
			(pintype "passive")
		)
		(pad "c40" thru_hole circle
			(at 5.08 -99.06 270)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "A16")
			(pinfunction "Pin_c40")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/AmigaPCI-Footprints/5650910-5.stp"
			(offset
				(xyz 2.5 -49.5 11.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 141.29 106.935 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C110"
			(at -3.765 -0.02 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 171.51 86.54 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C414"
			(at -3.648671 0.070711 -135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 -135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 67.7 80.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R100"
			(at -3.575 -0.01 0)
			(layer "B.SilkS")
		)
		(property "Value" "2k7"
			(at -7.095 0.01 0)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/CPU/SC0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 193.9 68.63)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C411"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 109.14 87.81 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C103"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 92.2 107.285 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C141"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 172.591992 87.628008 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C402"
			(at -3.648671 0.070711 -135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 -135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 153.525 71.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R113"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "22R"
			(at 0 -1.43 0)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 345 "Net-(U111-IO2_94)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 343 "RAMCLKA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 131.236637 89.393363 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C127"
			(at 3.80899 0.028284 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 45)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 135.1 92.63 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C129"
			(at -3.528463 -0.077782 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 45)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 167.111992 81.978008 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C416"
			(at -3.630275 0.021213 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 45)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 73.485 89.16 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R111"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "22R"
			(at 0 -1.43 0)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 309 "Net-(CN100-Pin_b12)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 89 "R_W")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 178.048008 82.168008 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C415"
			(at 3.616133 -0.035355 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 142.948008 82.778008 135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C125"
			(at -3.849478 0.014142 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 135)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 205.445 70.13)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C408"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 145.121992 80.601992 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C128"
			(at 3.61757 -0.113137 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 99.64 110.13 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C106"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 139.75 106.935 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C119"
			(at -3.765 -0.02 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 171.858008 78.068008 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C404"
			(at -3.75192 0.148492 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 205.415 57.13)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C407"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 168.2 83.06 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C401"
			(at -3.630275 0.021213 -135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 -135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 136.184008 73.619992 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C130"
			(at 3.679795 -0.124451 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 45)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 134.32 106.915 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C109"
			(at -3.765 -0.02 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 140.248008 77.571992 45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C133"
			(at -3.723636 0.035355 -135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 -135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U111-VCCPLL0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 45)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U111-GNDPLL0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 70.98 125.415 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R120"
			(at 3.655 -0.12 90)
			(layer "B.SilkS")
		)
		(property "Value" "22R"
			(at 0 -1.43 90)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 347 "Net-(CN100-Pin_a17)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 91 "SIZ1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 127.971992 86.098008 45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R108"
			(at 3.645854 0.098995 -135)
			(layer "B.SilkS")
		)
		(property "Value" "100R"
			(at -3.828265 -0.021213 -135)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 45)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U111-VCCPLL1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 45)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 109.17 74.02 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 67.715 73.09)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C204"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 67.715 83.25)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C205"
			(at 3.525 0.01 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 138.043363 75.386637 -135)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R109"
			(at 3.679795 -0.124451 45)
			(layer "B.SilkS")
		)
		(property "Value" "100R"
			(at -3.650986 -0.176777 45)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 225)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 225)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U111-VCCPLL0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 67.715 65.44)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C203"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 205.575 102.33)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C417"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 129.061992 87.198008 -135)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C132"
			(at -3.716565 0.014142 45)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 3.566635 0.014142 45)
			(layer "B.SilkS")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Card Connector")
		(sheetfile "CardConnector.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U111-VCCPLL1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 225)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U111-GNDPLL1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 167.62 106.97 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C111"
			(at -3.685 -0.01 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 172.928008 76.988008 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C405"
			(at -3.75192 0.148492 135)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 135)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Fast Memory")
		(sheetfile "FastMem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 315)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 67.705 81.72 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R101"
			(at -3.49 0.02 0)
			(layer "B.SilkS")
		)
		(property "Value" "2k7"
			(at -7.07 0 0)
			(layer "B.SilkS")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "CPU")
		(sheetfile "CPU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 103 "/CPU/SC1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 162.18 106.955 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C121"
			(at -3.685 -0.01 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Shifting")
		(sheetfile "level_shift.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 52.494607 38.638571)
		(mid 52.783332 37.935538)
		(end 53.484607 37.642571)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210.99 37.642107)
		(mid 211.696072 37.932499)
		(end 211.99 38.637107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 53.484607 37.642571)
		(end 210.99 37.642107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 52.492036 133.118722)
		(end 52.494607 38.638571)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 53.493036 134.112722)
		(mid 52.786669 133.823038)
		(end 52.492036 133.118722)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.99 134.11)
		(end 53.493036 134.112722)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 211.99 133.11)
		(mid 211.697107 133.817107)
		(end 210.99 134.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.99 38.637107)
		(end 211.99 133.11)
		(layer "Edge.Cuts")
	)
	(gr_text "CONNECTOR THIS SIDE!"
		(at 160.52 119.76 0)
		(layer "B.SilkS")
	)
	(gr_text "RST\nSS\nDO\nCLK\nDI\nGND"
		(at 141.82 41.53 90)
		(layer "F.SilkS")
	)
	(gr_text "AmigaPCI LOCAL BUS CARD 68040 Rev 4.1\nhttps://github.com/jasonsbeer/AmigaPCI"
		(at 205.13 53.31 270)
		(layer "F.SilkS")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 71.2 76.03 0)
		(layer "F.SilkS")
	)
	(gr_text "RST\nSS\nDO\nCLK\nDI\nGND"
		(at 165.24 41.55 90)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 100.86 49.96 90)
		(layer "F.SilkS")
	)
	(gr_text "THE BRAIN"
		(at 64.65 129.46 0)
		(layer "F.SilkS")
	)
	(gr_text "U401"
		(at 196.25 65.13 0)
		(layer "F.Fab")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 76.51 44.34) (xy 76.51 40.88)
		)
		(height 6.5)
		(gr_text "3.5 mm"
			(at 84.35 42.62 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 65.04 42.58) (xy 195.04 42.58)
		)
		(height -8.04)
		(gr_text "130.0 mm"
			(at 130.04 33.39 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 75.01 42.59) (xy 75.01 124.09)
		)
		(height 6.87)
		(gr_text "81.5 mm"
			(at 66.99 83.34 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 65.05 42.56) (xy 89.04 42.56)
		)
		(height 95.97)
		(gr_text "24.0 mm"
			(at 77.045 137.38 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.5 37.64) (xy 52.51 134.11) (xy 211.99 134.1) (xy 211.99 37.64)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.49 37.64) (xy 52.5 134.11) (xy 211.99 134.15) (xy 211.99 37.69)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+1V2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.31 82.26) (xy 134.46 70.01) (xy 146.01 82.45) (xy 134.02 94.19)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.48 37.64) (xy 52.49 134.11) (xy 211.99 134.15) (xy 211.99 37.69)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+1V2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.55 82.42) (xy 173.01 90.09) (xy 181 81.98) (xy 173.53 74.4)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.48 37.64) (xy 52.49 134.11) (xy 211.99 134.15) (xy 211.99 37.69)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.49 37.64) (xy 52.5 134.11) (xy 211.99 134.1) (xy 211.99 37.64)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.477516 37.64) (xy 52.487516 134.11) (xy 211.987516 134.15) (xy 211.987516 37.69)
			)
		)
	)
)
