(footprint "C_1206_3216_Feedthrough" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 60515DB2)
  (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
  (tags "capacitor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.82) (layer "F.SilkS"))
  (fp_text value "C_1206_3216_Feedthrough" (at 0 1.82) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
  (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "3" smd roundrect (at 0 -1.016) (size 0.94 0.94) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at 0 1.016) (size 0.94 0.94) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
