(footprint "DSUB-25_Stack_Female_Bottom_Male_Top" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
  (tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -21.844) (layer "F.SilkS"))
  (fp_text value "DSUB-25_Stack_Female_Bottom_Male_Top" (at 0.017 7.976) (layer "F.Fab"))
  (fp_text user "MALE TOP/FEMALE BOTTOM" (at 0 -3.81) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 0.017 3.391) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 16.637 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 13.867 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at 11.097 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at 8.327 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at 5.557 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at 2.787 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole circle (at 0.017 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole circle (at -2.753 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole circle (at -5.523 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole circle (at -8.293 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "11" thru_hole circle (at -11.063 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "12" thru_hole circle (at -13.833 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "13" thru_hole circle (at -16.603 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "14" thru_hole circle (at 15.252 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "15" thru_hole circle (at 12.482 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "16" thru_hole circle (at 9.712 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "17" thru_hole circle (at 6.942 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "18" thru_hole circle (at 4.172 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole circle (at 1.402 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "20" thru_hole circle (at -1.368 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "21" thru_hole circle (at -4.138 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "22" thru_hole circle (at -6.908 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "23" thru_hole circle (at -9.678 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "24" thru_hole circle (at -12.448 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "25" thru_hole circle (at -15.218 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "26" thru_hole rect (at -16.603 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "27" thru_hole circle (at -13.833 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "28" thru_hole circle (at -11.049 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "29" thru_hole circle (at -8.293 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "30" thru_hole circle (at -5.523 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "31" thru_hole circle (at -2.753 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "32" thru_hole circle (at 0.017 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "33" thru_hole circle (at 2.794 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "34" thru_hole circle (at 5.557 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "35" thru_hole circle (at 8.327 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "36" thru_hole circle (at 11.097 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "37" thru_hole circle (at 13.843 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "38" thru_hole circle (at 16.637 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "39" thru_hole circle (at -15.24 -14.98) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "40" thru_hole circle (at -12.448 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "41" thru_hole circle (at -9.652 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "42" thru_hole circle (at -6.908 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "43" thru_hole circle (at -4.138 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "44" thru_hole circle (at -1.368 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "45" thru_hole circle (at 1.397 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "46" thru_hole circle (at 4.172 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "47" thru_hole circle (at 6.942 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "48" thru_hole circle (at 9.712 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "49" thru_hole circle (at 12.482 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "50" thru_hole circle (at 15.252 -14.986) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "51" thru_hole circle (at -23.533 -16.4) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "51" thru_hole circle (at -23.533 -8.5) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "51" thru_hole circle (at 23.567 -16.4) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "51" thru_hole circle (at 23.567 -8.5) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
