(footprint "DSUB-9_Male_Stack" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
  (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
  (attr through_hole)
  (fp_text reference "REF**" (at -0.048 -21.082) (layer "F.SilkS"))
  (fp_text value "DSUB-9_Male_Stack" (at 0 8.636) (layer "F.Fab"))
  (fp_text user "MALE TOP/MALE BOTTOM" (at 0 -3.556) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at -0.048 3.272) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -5.588 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at -2.818 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at -0.048 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at 2.722 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at 5.492 -11.02) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at -4.203 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole circle (at -1.433 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole circle (at 1.337 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole circle (at 4.107 -8.18) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole rect (at -5.588 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "11" thru_hole circle (at -2.818 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "12" thru_hole circle (at -0.048 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "13" thru_hole circle (at 2.722 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "14" thru_hole circle (at 5.492 -17.82) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "15" thru_hole circle (at -4.203 -14.98) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "16" thru_hole circle (at -1.433 -14.98) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "17" thru_hole circle (at 1.337 -14.98) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "18" thru_hole circle (at 4.107 -14.98) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole circle (at -12.548 -16.4) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole circle (at -12.548 -8.5) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole circle (at 12.452 -16.4) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole circle (at 12.452 -8.5) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
  (model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
