(footprint "FanHeader_1x03_P2.54mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (property "Sheetfile" "power.kicad_sch")
  (property "Sheetname" "Power")
  (attr through_hole)
  (fp_text reference "J9003" (at 2.44348 2.42824 90) (layer "F.SilkS"))
  (fp_text value "Case Fan" (at -3.44302 2.52476 90) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 0 2.54 -90) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
