(footprint "PCI-5V" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -6.14569 37.52615 90) (layer "F.SilkS"))
  (fp_text value "PCI-5V" (at 6.11251 31.26976 90) (layer "F.Fab"))
  (pad "" np_thru_hole oval (at 0 -40.01 90) (size 2 2.44) (drill oval 2 2.44) (layers "F&B.Cu" "*.Mask"))
  (pad "" np_thru_hole oval (at 0 24.76 90) (size 2 2.44) (drill oval 2 2.44) (layers "F&B.Cu" "*.Mask"))
  (pad "A1" thru_hole roundrect (at 3.81 -38.11) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25))
  (pad "A2" thru_hole roundrect (at 1.27 -36.84) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A3" thru_hole roundrect (at 3.81 -35.57) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A4" thru_hole roundrect (at 1.27 -34.3) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A5" thru_hole roundrect (at 3.81 -33.03) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A6" thru_hole roundrect (at 1.27 -31.76) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A7" thru_hole roundrect (at 3.81 -30.49) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A8" thru_hole roundrect (at 1.27 -29.22) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A9" thru_hole roundrect (at 3.81 -27.95) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A10" thru_hole roundrect (at 1.27 -26.68) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A11" thru_hole roundrect (at 3.81 -25.41) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A12" thru_hole roundrect (at 1.27 -24.13) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A13" thru_hole roundrect (at 3.81 -22.86) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A14" thru_hole roundrect (at 1.27 -21.59) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A15" thru_hole roundrect (at 3.81 -20.32) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A16" thru_hole roundrect (at 1.27 -19.05) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A17" thru_hole roundrect (at 3.81 -17.78) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A18" thru_hole roundrect (at 1.27 -16.51) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A19" thru_hole roundrect (at 3.81 -15.24) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A20" thru_hole roundrect (at 1.27 -13.97) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A21" thru_hole roundrect (at 3.81 -12.7) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A22" thru_hole roundrect (at 1.27 -11.43) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A23" thru_hole roundrect (at 3.81 -10.16) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A24" thru_hole roundrect (at 1.27 -8.89) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A25" thru_hole roundrect (at 3.81 -7.62) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A26" thru_hole roundrect (at 1.27 -6.35) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A27" thru_hole roundrect (at 3.81 -5.08) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A28" thru_hole roundrect (at 1.27 -3.81) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A29" thru_hole roundrect (at 3.81 -2.54) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A30" thru_hole roundrect (at 1.27 -1.27) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A31" thru_hole roundrect (at 3.81 0) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A32" thru_hole roundrect (at 1.27 1.27) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A33" thru_hole roundrect (at 3.81 2.54) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A34" thru_hole roundrect (at 1.27 3.81) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A35" thru_hole roundrect (at 3.81 5.08) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A36" thru_hole roundrect (at 1.27 6.35) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A37" thru_hole roundrect (at 3.81 7.62) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A38" thru_hole roundrect (at 1.27 8.89) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A39" thru_hole roundrect (at 3.81 10.16) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A40" thru_hole roundrect (at 1.27 11.43) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A41" thru_hole roundrect (at 3.81 12.7) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A42" thru_hole roundrect (at 1.27 13.97) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A43" thru_hole roundrect (at 3.81 15.24) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A44" thru_hole roundrect (at 1.27 16.51) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A45" thru_hole roundrect (at 3.81 17.78) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A46" thru_hole roundrect (at 1.27 19.05) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A47" thru_hole roundrect (at 3.81 20.32) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A48" thru_hole roundrect (at 1.27 21.59) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A49" thru_hole roundrect (at 3.81 22.86) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A52" thru_hole roundrect (at 1.27 26.67) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A53" thru_hole roundrect (at 3.81 27.94) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A54" thru_hole roundrect (at 1.27 29.21) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A55" thru_hole roundrect (at 3.81 30.48) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A56" thru_hole roundrect (at 1.27 31.75) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A57" thru_hole roundrect (at 3.81 33.02) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A58" thru_hole roundrect (at 1.27 34.29) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A59" thru_hole roundrect (at 3.81 35.56) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A60" thru_hole roundrect (at 1.27 36.83) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A61" thru_hole roundrect (at 3.81 38.1) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "A62" thru_hole roundrect (at 1.27 39.37) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B1" thru_hole roundrect (at -1.27 -38.11) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B2" thru_hole roundrect (at -3.81 -36.84) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B3" thru_hole roundrect (at -1.27 -35.57) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B4" thru_hole roundrect (at -3.81 -34.3) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B5" thru_hole roundrect (at -1.27 -33.03) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B6" thru_hole roundrect (at -3.81 -31.76) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B7" thru_hole roundrect (at -1.27 -30.49) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B8" thru_hole roundrect (at -3.81 -29.22) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B9" thru_hole roundrect (at -1.27 -27.95) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B10" thru_hole roundrect (at -3.81 -26.68) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B11" thru_hole roundrect (at -1.27 -25.41) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B12" thru_hole roundrect (at -3.81 -24.13) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B13" thru_hole roundrect (at -1.27 -22.86) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B14" thru_hole roundrect (at -3.81 -21.59) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B15" thru_hole roundrect (at -1.27 -20.32) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B16" thru_hole roundrect (at -3.81 -19.05) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B17" thru_hole roundrect (at -1.27 -17.78) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B18" thru_hole roundrect (at -3.81 -16.51) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B19" thru_hole roundrect (at -1.27 -15.24) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B20" thru_hole roundrect (at -3.81 -13.97) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B21" thru_hole roundrect (at -1.27 -12.7) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B22" thru_hole roundrect (at -3.81 -11.43) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B23" thru_hole roundrect (at -1.27 -10.16) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B24" thru_hole roundrect (at -3.81 -8.89) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B25" thru_hole roundrect (at -1.27 -7.62) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B26" thru_hole roundrect (at -3.81 -6.35) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B27" thru_hole roundrect (at -1.27 -5.08) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B28" thru_hole roundrect (at -3.81 -3.81) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B29" thru_hole roundrect (at -1.27 -2.54) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B30" thru_hole roundrect (at -3.81 -1.27) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B31" thru_hole roundrect (at -1.27 0) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B32" thru_hole roundrect (at -3.81 1.27) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B33" thru_hole roundrect (at -1.27 2.54) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B34" thru_hole roundrect (at -3.81 3.81) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B35" thru_hole roundrect (at -1.27 5.08) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B36" thru_hole roundrect (at -3.81 6.35) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B37" thru_hole roundrect (at -1.27 7.62) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B38" thru_hole roundrect (at -3.81 8.89) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B39" thru_hole roundrect (at -1.27 10.16) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B40" thru_hole roundrect (at -3.81 11.43) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B41" thru_hole roundrect (at -1.27 12.7) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B42" thru_hole roundrect (at -3.81 13.97) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B43" thru_hole roundrect (at -1.27 15.24) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B44" thru_hole roundrect (at -3.81 16.51) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B45" thru_hole roundrect (at -1.27 17.78) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B46" thru_hole roundrect (at -3.81 19.05) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B47" thru_hole roundrect (at -1.27 20.32) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B48" thru_hole roundrect (at -3.81 21.59) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B49" thru_hole roundrect (at -1.27 22.86) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B52" thru_hole roundrect (at -3.81 26.67) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B53" thru_hole roundrect (at -1.27 27.94) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B54" thru_hole roundrect (at -3.81 29.21) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B55" thru_hole roundrect (at -1.27 30.48) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B56" thru_hole roundrect (at -3.81 31.75) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B57" thru_hole roundrect (at -1.27 33.02) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B58" thru_hole roundrect (at -3.81 34.29) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B59" thru_hole roundrect (at -1.27 35.56) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B60" thru_hole roundrect (at -3.81 36.83) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B61" thru_hole roundrect (at -1.27 38.1) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (pad "B62" thru_hole roundrect (at -3.81 39.37) (size 1.68 1.68) (drill 1.02) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
    (chamfer_ratio 0.2929) (chamfer top_left top_right bottom_left bottom_right))
  (model "${KIPRJMOD}/A2900-Footprints/5145154-4.step"
    (offset (xyz 0 -0.6 14))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
