(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "74LVC245" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U405" (at 0 18.9398 0))
    (property "Value" "74LVC245" (at 0 16.4029 0))
    (property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm" (at 0 0 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245" (at 0 0 0))
    (property "ki_locked" "" (at 0 0 0))
    (property "ki_keywords" "TTL BUS 3State" (at 0 0 0))
    (property "ki_description" "Octal BUS Transceivers, 3-State outputs" (at 0 0 0))
    (property "ki_fp_filters" "DIP?20*" (at 0 0 0))
    (symbol "74LVC245_1_0"
      (pin input line (at -12.7 -10.16 0) (length 5.08)
        (name "A->B")
        (number "1")
      )
      (pin tri_state line (at 12.7 -5.08 180) (length 5.08)
        (name "B7")
        (number "11")
      )
      (pin tri_state line (at 12.7 -2.54 180) (length 5.08)
        (name "B6")
        (number "12")
      )
      (pin tri_state line (at 12.7 0 180) (length 5.08)
        (name "B5")
        (number "13")
      )
      (pin tri_state line (at 12.7 2.54 180) (length 5.08)
        (name "B4")
        (number "14")
      )
      (pin tri_state line (at 12.7 5.08 180) (length 5.08)
        (name "B3")
        (number "15")
      )
      (pin tri_state line (at 12.7 7.62 180) (length 5.08)
        (name "B2")
        (number "16")
      )
      (pin tri_state line (at 12.7 10.16 180) (length 5.08)
        (name "B1")
        (number "17")
      )
      (pin tri_state line (at 12.7 12.7 180) (length 5.08)
        (name "B0")
        (number "18")
      )
      (pin input inverted (at -12.7 -12.7 0) (length 5.08)
        (name "CE")
        (number "19")
      )
      (pin tri_state line (at -12.7 12.7 0) (length 5.08)
        (name "A0")
        (number "2")
      )
      (pin tri_state line (at -12.7 10.16 0) (length 5.08)
        (name "A1")
        (number "3")
      )
      (pin tri_state line (at -12.7 7.62 0) (length 5.08)
        (name "A2")
        (number "4")
      )
      (pin tri_state line (at -12.7 5.08 0) (length 5.08)
        (name "A3")
        (number "5")
      )
      (pin tri_state line (at -12.7 2.54 0) (length 5.08)
        (name "A4")
        (number "6")
      )
      (pin tri_state line (at -12.7 0 0) (length 5.08)
        (name "A5")
        (number "7")
      )
      (pin tri_state line (at -12.7 -2.54 0) (length 5.08)
        (name "A6")
        (number "8")
      )
      (pin tri_state line (at -12.7 -5.08 0) (length 5.08)
        (name "A7")
        (number "9")
      )
    )
    (symbol "74LVC245_1_1")
    (symbol "74LVC245_2_0"
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND")
        (number "10")
      )
      (pin power_in line (at 0 12.7 270) (length 5.08)
        (name "VCC")
        (number "20")
      )
    )
    (symbol "74LVC245_2_1")
  )
)
