(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "+AUD"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR094"
			(at 0 -3.81 0)
		)
		(property "Value" "+AUD"
			(at 0.381 4.3942 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "power-flag"
			(at 0 0 0)
		)
		(symbol "+AUD_0_1")
		(symbol "+AUD_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0) hide
				(name "+AUD")
				(number "1")
			)
		)
	)
	(symbol "+AV"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#+AV02"
			(at 0 -3.81 0)
		)
		(property "Value" "+AV"
			(at 0.381 4.3942 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "power-flag"
			(at 0 0 0)
		)
		(symbol "+AV_0_1")
		(symbol "+AV_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0) hide
				(name "+AV")
				(number "1")
			)
		)
	)
	(symbol "+VID"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR062"
			(at 0 -3.81 0)
		)
		(property "Value" "+VID"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "power-flag"
			(at 0 0 0)
		)
		(symbol "+VID_0_1")
		(symbol "+VID_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0) hide
				(name "+VID")
				(number "1")
			)
		)
	)
	(symbol "-AV"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#-AV02"
			(at 0 -3.81 0)
		)
		(property "Value" "-AV"
			(at 0.381 4.3942 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "power-flag"
			(at 0 0 0)
		)
		(symbol "-AV_0_1")
		(symbol "-AV_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0) hide
				(name "-AV")
				(number "1")
			)
		)
	)
	(symbol "74CBT16233"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 1.27 0)
		)
		(property "Value" "74CBT16233"
			(at 15.24 -1.27 0)
		)
		(property "Footprint" "Package_SO:SSOP-56_7.5x18.5mm_P0.635mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74cbt16233.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1686702107606&ref_url=https%253A%252F%252Fwww.ti.com%252Fgeneral%252Fdocs%252Fsuppproductinfo.tsp%253FdistId%253D10%2526gotoUrl%253Dhttps%253A%252F%252Fwww.ti.com%252Flit%252Fgpn%252Fsn74cbt16233"
			(at -1.27 0 0)
		)
		(property "Description" "16 x 1:2 FET Multiplexer/Demultiplexer, Low-Voltage"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "mux demux low-voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm* TSSOP*4.4x5mm*P0.65mm* TVSOP*4.4x3.6mm*P0.4mm* SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "74CBT16233_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1A")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "1B2")
				(number "55")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "1B1")
				(number "56")
			)
		)
		(symbol "74CBT16233_2_1"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "2B1")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "2B2")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "2A")
				(number "54")
			)
		)
		(symbol "74CBT16233_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "3A")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "3B2")
				(number "52")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "3B1")
				(number "53")
			)
		)
		(symbol "74CBT16233_4_1"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "4B1")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "4A")
				(number "51")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "4B2")
				(number "6")
			)
		)
		(symbol "74CBT16233_5_1"
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "5B2")
				(number "49")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "5B1")
				(number "50")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "5A")
				(number "7")
			)
		)
		(symbol "74CBT16233_6_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "6A")
				(number "48")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "6B1")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "6B2")
				(number "9")
			)
		)
		(symbol "74CBT16233_7_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "7A")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "7B2")
				(number "46")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "7B1")
				(number "47")
			)
		)
		(symbol "74CBT16233_8_0"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "8B1")
				(number "11")
			)
		)
		(symbol "74CBT16233_8_1"
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "8B2")
				(number "12")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "8A")
				(number "45")
			)
		)
		(symbol "74CBT16233_9_0"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "9A")
				(number "15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "9B2")
				(number "41")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "9B1")
				(number "42")
			)
		)
		(symbol "74CBT16233_9_1")
		(symbol "74CBT16233_10_0"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "10B1")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "10B2")
				(number "17")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "10A")
				(number "40")
			)
		)
		(symbol "74CBT16233_10_1")
		(symbol "74CBT16233_11_0"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "11A")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "11B2")
				(number "38")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "11B1")
				(number "39")
			)
		)
		(symbol "74CBT16233_11_1")
		(symbol "74CBT16233_12_0"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "12B1")
				(number "19")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "12B2")
				(number "20")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "12A")
				(number "37")
			)
		)
		(symbol "74CBT16233_12_1")
		(symbol "74CBT16233_13_0"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "13A")
				(number "21")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "13B2")
				(number "35")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "13B1")
				(number "36")
			)
		)
		(symbol "74CBT16233_13_1")
		(symbol "74CBT16233_14_0"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "14B1")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "14B2")
				(number "23")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "14A")
				(number "34")
			)
		)
		(symbol "74CBT16233_14_1")
		(symbol "74CBT16233_15_0"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "15A")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "15B2")
				(number "32")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "15B1")
				(number "33")
			)
		)
		(symbol "74CBT16233_15_1")
		(symbol "74CBT16233_16_0"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "16B1")
				(number "25")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "16B2")
				(number "26")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "16A")
				(number "31")
			)
		)
		(symbol "74CBT16233_16_1")
		(symbol "74CBT16233_17_0"
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "SEL2")
				(number "29")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "SEL1")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "44")
			)
		)
		(symbol "74CBT16233_17_1"
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "TEST1")
				(number "27")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "TEST2")
				(number "28")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "43")
			)
		)
	)
	(symbol "74FCT646"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U702"
			(at 0 18.2372 0)
		)
		(property "Value" "74FCT646"
			(at 0 15.875 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Digikey" "296-33244-5-ND"
			(at 0 17.8816 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "74FCT646_1_0"
			(pin input line
				(at -12.7 1.27 0)
				(length 2.54)
				(name "CPAB")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 -8.89 0)
				(length 2.54)
				(name "A7")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -11.43 0)
				(length 2.54)
				(name "A8")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -11.43 180)
				(length 2.54)
				(name "B8")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -8.89 180)
				(length 2.54)
				(name "B7")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -6.35 180)
				(length 2.54)
				(name "B6")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -3.81 180)
				(length 2.54)
				(name "B5")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 2.54)
				(name "B4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 6.35 180)
				(length 2.54)
				(name "B3")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 8.89 180)
				(length 2.54)
				(name "B2")
				(number "19")
			)
			(pin input line
				(at 1.27 -16.51 90)
				(length 2.54)
				(name "SAB")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 11.43 180)
				(length 2.54)
				(name "B1")
				(number "20")
			)
			(pin input inverted
				(at -1.27 -16.51 90)
				(length 2.54)
				(name "G")
				(number "21")
			)
			(pin input line
				(at 3.81 -16.51 90)
				(length 2.54)
				(name "SBA")
				(number "22")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 2.54)
				(name "CPBA")
				(number "23")
			)
			(pin input line
				(at -3.81 -16.51 90)
				(length 2.54)
				(name "DIR")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 11.43 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 8.89 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 6.35 0)
				(length 2.54)
				(name "A3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 3.81 0)
				(length 2.54)
				(name "A4")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -3.81 0)
				(length 2.54)
				(name "A5")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -6.35 0)
				(length 2.54)
				(name "A6")
				(number "9")
			)
		)
		(symbol "74FCT646_1_1")
		(symbol "74FCT646_2_0"
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vcc")
				(number "24")
			)
		)
		(symbol "74FCT646_2_1")
	)
	(symbol "74LVC1G157"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "74LVC1G157"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74LVC1G157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single 2 to 1 line Multiplexer"
			(at 0 0 0)
		)
		(property "ki_keywords" "MUX MUX2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "74LVC1G157_1_0"
			(pin input line
				(at -12.7 1.27 0)
				(length 5.08)
				(name "I1")
				(number "1")
			)
			(pin power_in line
				(at 0 -11.43 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -12.7 3.81 0)
				(length 5.08)
				(name "I0")
				(number "3")
			)
			(pin output line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "Y")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "S")
				(number "6")
			)
		)
		(symbol "74LVC1G157_1_1")
	)
	(symbol "74LVC245"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U405"
			(at 0 18.9398 0)
		)
		(property "Value" "74LVC245"
			(at 0 16.4029 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245"
			(at 0 0 0)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TTL BUS 3State"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LVC245_1_0"
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A->B")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "B7")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "B6")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "B5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B4")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B2")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B1")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "B0")
				(number "18")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CE")
				(number "19")
			)
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
		)
		(symbol "74LVC245_1_1")
		(symbol "74LVC245_2_0"
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
		)
		(symbol "74LVC245_2_1")
	)
	(symbol "AP2156SG-13"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part Number" "AP2156SG-13"
			(at 0 7.62 0)
		)
		(symbol "AP2156SG-13_0_0"
			(pin input line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "EN1")
				(number "1")
			)
			(pin output line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "FLG1")
				(number "2")
			)
			(pin output line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "FLG2")
				(number "3")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "EN2")
				(number "4")
			)
			(pin power_out line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
			(pin power_in line
				(at 1.27 -8.89 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -1.27 -8.89 90)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin power_out line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "OUT1")
				(number "8")
			)
		)
		(symbol "AP2156SG-13_0_1")
	)
	(symbol "AT27C1024"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "AT27C1024"
			(at 0 21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm_Socket"
			(at -10.414 12.7 0)
		)
		(property "Datasheet" ""
			(at -10.414 12.7 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "AT27C1024_1_1"
			(pin input line
				(at 12.7 0 180)
				(length 5.08)
				(name "O8")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O7")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O6")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "O5")
				(number "14")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "O4")
				(number "15")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "O3")
				(number "16")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "O2")
				(number "17")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "O1")
				(number "18")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "O0")
				(number "19")
			)
			(pin input line
				(at 12.7 -29.21 180)
				(length 5.08)
				(name "_CE")
				(number "2")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "_OE")
				(number "20")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "A1")
				(number "22")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "A2")
				(number "23")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "A3")
				(number "24")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "A4")
				(number "25")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "A5")
				(number "26")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A6")
				(number "27")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A7")
				(number "28")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A8")
				(number "29")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "O15")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A9")
				(number "31")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A10")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A11")
				(number "33")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A12")
				(number "34")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A13")
				(number "35")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A14")
				(number "36")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A15")
				(number "37")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "")
				(number "38")
			)
			(pin no_connect line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "")
				(number "39")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "O14")
				(number "4")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O13")
				(number "5")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O12")
				(number "6")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O11")
				(number "7")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O10")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O9")
				(number "9")
			)
		)
		(symbol "AT27C1024_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "30")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vcc")
				(number "40")
			)
		)
	)
	(symbol "AT27C4096"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "AT27C4096"
			(at 0 21.59 0)
		)
		(property "Footprint" ""
			(at -10.414 12.7 0)
		)
		(property "Datasheet" ""
			(at -10.414 12.7 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "AT27C4096_1_1"
			(pin input line
				(at 12.7 0 180)
				(length 5.08)
				(name "O8")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O7")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O6")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "O5")
				(number "14")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "O4")
				(number "15")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "O3")
				(number "16")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "O2")
				(number "17")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "O1")
				(number "18")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "O0")
				(number "19")
			)
			(pin input line
				(at 12.7 -29.21 180)
				(length 5.08)
				(name "_CE")
				(number "2")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "_OE")
				(number "20")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "A1")
				(number "22")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "A2")
				(number "23")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "A3")
				(number "24")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "A4")
				(number "25")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "A5")
				(number "26")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A6")
				(number "27")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A7")
				(number "28")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A8")
				(number "29")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "O15")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A9")
				(number "31")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A10")
				(number "32")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A11")
				(number "33")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A12")
				(number "34")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A13")
				(number "35")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A14")
				(number "36")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A15")
				(number "37")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "A16")
				(number "38")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "A17")
				(number "39")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "O14")
				(number "4")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O13")
				(number "5")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O12")
				(number "6")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O11")
				(number "7")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O10")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O9")
				(number "9")
			)
		)
		(symbol "AT27C4096_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "30")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vcc")
				(number "40")
			)
		)
	)
	(symbol "AT27C4096-PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 24.13 0)
		)
		(property "Value" "AT27C4096"
			(at 0 21.59 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44_SMD-Socket"
			(at -10.414 12.7 0)
		)
		(property "Datasheet" ""
			(at -10.414 12.7 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "AT27C4096-PLCC_1_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A14")
				(number "40")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A15")
				(number "41")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "A16")
				(number "42")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "A17")
				(number "43")
			)
		)
		(symbol "AT27C4096-PLCC_1_1"
			(pin no_connect line
				(at -5.08 -38.1 90)
				(length 5.08)
				(name "NC")
				(number "1")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "O9")
				(number "10")
			)
			(pin input line
				(at 12.7 0 180)
				(length 5.08)
				(name "O8")
				(number "11")
			)
			(pin no_connect line
				(at 0 -38.1 90)
				(length 5.08)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "O7")
				(number "14")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "O6")
				(number "15")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "O5")
				(number "16")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "O4")
				(number "17")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "O3")
				(number "18")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "O2")
				(number "19")
			)
			(pin no_connect line
				(at -2.54 -38.1 90)
				(length 5.08)
				(name "Vpp")
				(number "2")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "O1")
				(number "20")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "O0")
				(number "21")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "_OE")
				(number "22")
			)
			(pin no_connect line
				(at 2.54 -38.1 90)
				(length 5.08)
				(name "NC")
				(number "23")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "A0")
				(number "24")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "A1")
				(number "25")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "A2")
				(number "26")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "A3")
				(number "27")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "A4")
				(number "28")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "A5")
				(number "29")
			)
			(pin input line
				(at 12.7 -27.94 180)
				(length 5.08)
				(name "_CE")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A6")
				(number "30")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "A7")
				(number "31")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A8")
				(number "32")
			)
			(pin no_connect line
				(at 5.08 -38.1 90)
				(length 5.08)
				(name "NC")
				(number "33")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A9")
				(number "35")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A10")
				(number "36")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A11")
				(number "37")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A12")
				(number "38")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A13")
				(number "39")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "O15")
				(number "4")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "O14")
				(number "5")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "O13")
				(number "6")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "O12")
				(number "7")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "O11")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "O10")
				(number "9")
			)
		)
		(symbol "AT27C4096-PLCC_2_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 5.08)
				(name "Vcc")
				(number "44")
			)
		)
		(symbol "AT27C4096-PLCC_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 5.08)
				(name "GND")
				(number "34")
			)
		)
	)
	(symbol "ATX-24-Amiga"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 0 16.9418 0)
		)
		(property "Value" "ATX-24"
			(at 0 14.6304 0)
		)
		(property "Footprint" "Connector_Molex:Molex_Mini-Fit_Jr_5566-24A_2x12_P4.20mm_Vertical"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.intel.com/content/dam/www/public/us/en/documents/guides/power-supply-design-guide-june.pdf#page=33"
			(at 60.96 -13.97 0)
		)
		(property "Description" "ATX Power supply 24pins"
			(at 0 0 0)
		)
		(property "Part" "39281243"
			(at 0 0 0)
		)
		(property "ki_keywords" "ATX PSU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Mini?Fit*2x12*Vertical* *Mini?Fit*2x12*Horizontal*"
			(at 0 0 0)
		)
		(symbol "ATX-24-Amiga_0_0"
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "+3.3V")
				(number "1")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54) hide
				(name "+3.3V")
				(number "13")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54) hide
				(name "+3.3V")
				(number "2")
			)
		)
		(symbol "ATX-24-Amiga_0_1")
		(symbol "ATX-24-Amiga_1_0"
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54) hide
				(name "+3.3V")
				(number "12")
			)
		)
		(symbol "ATX-24-Amiga_1_1"
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+12V")
				(number "10")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54) hide
				(name "+12V")
				(number "11")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "-12V")
				(number "14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "15")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PS_ON#")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54) hide
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54) hide
				(name "+5V")
				(number "21")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54) hide
				(name "+5V")
				(number "22")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54) hide
				(name "+5V")
				(number "23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "+5V")
				(number "4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54) hide
				(name "+5V")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PWR_OK")
				(number "8")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "+5VSB")
				(number "9")
			)
		)
	)
	(symbol "AUDIO GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR046"
			(at 0 -6.35 0)
		)
		(property "Value" "AUDIO GND"
			(at 0.127 -4.3942 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"AUDIO\" , reference supply ground"
			(at 0 0 0)
		)
		(property "ki_keywords" "power-flag"
			(at 0 0 0)
		)
		(symbol "AUDIO GND_0_1")
		(symbol "AUDIO GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0) hide
				(name "AUDIO")
				(number "1")
			)
		)
	)
	(symbol "Agnus Multiadapter"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "Agnus_MULTI"
			(at 0 0 0)
		)
		(property "Footprint" "Package_LCC:PLCC-84_THT-Socket"
			(at 0 -3.048 0)
		)
		(property "Datasheet" ""
			(at -2.54 39.37 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "Agnus Multiadapter_1_1"
			(pin bidirectional line
				(at -17.78 52.07 0)
				(length 2.54)
				(name "DRD13")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 29.21 0)
				(length 2.54)
				(name "DRD4")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 26.67 0)
				(length 2.54)
				(name "DRD3")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 24.13 0)
				(length 2.54)
				(name "DRD2")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 21.59 0)
				(length 2.54)
				(name "DRD1")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 19.05 0)
				(length 2.54)
				(name "DRD0")
				(number "14")
			)
			(pin input line
				(at -17.78 -54.61 0)
				(length 2.54)
				(name "_RESET")
				(number "16")
			)
			(pin output line
				(at -17.78 -59.69 0)
				(length 2.54)
				(name "_INTR")
				(number "17")
			)
			(pin input line
				(at -17.78 -57.15 0)
				(length 2.54)
				(name "DMAL")
				(number "18")
			)
			(pin input line
				(at 0 62.23 270)
				(length 2.54)
				(name "_BLS")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 49.53 0)
				(length 2.54)
				(name "DRD12")
				(number "2")
			)
			(pin output line
				(at 2.54 62.23 270)
				(length 2.54)
				(name "_DBR")
				(number "20")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "_WE")
				(number "21")
			)
			(pin input line
				(at -17.78 -46.99 0)
				(length 2.54)
				(name "R/W")
				(number "22")
			)
			(pin input line
				(at -2.54 62.23 270)
				(length 2.54)
				(name "_REGEN")
				(number "23")
			)
			(pin input line
				(at -17.78 -49.53 0)
				(length 2.54)
				(name "_AS")
				(number "24")
			)
			(pin input line
				(at -5.08 62.23 270)
				(length 2.54)
				(name "_RAMEN")
				(number "25")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RGA8")
				(number "26")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RGA7")
				(number "27")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "RGA6")
				(number "28")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "RGA5")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 46.99 0)
				(length 2.54)
				(name "DRD11")
				(number "3")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "RGA4")
				(number "30")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "RGA3")
				(number "31")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "RGA2")
				(number "32")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "RGA1")
				(number "33")
			)
			(pin output line
				(at -17.78 -67.31 0)
				(length 2.54)
				(name "28MHz")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "A20/XCLK")
				(number "35")
			)
			(pin output line
				(at 17.78 -45.72 180)
				(length 2.54)
				(name "_CDAC/_XCLKEN")
				(number "36")
			)
			(pin output line
				(at 17.78 -41.91 180)
				(length 2.54)
				(name "7MHz/_CDAC")
				(number "37")
			)
			(pin output line
				(at 17.78 52.07 180)
				(length 2.54)
				(name "CCKQ/7MHz")
				(number "38")
			)
			(pin output line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "CCK/CCKQ")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 44.45 0)
				(length 2.54)
				(name "DRD10")
				(number "4")
			)
			(pin output line
				(at 17.78 44.45 180)
				(length 2.54)
				(name "14M_or_Vbb/CCK")
				(number "40")
			)
			(pin input line
				(at 17.78 -67.31 180)
				(length 2.54)
				(name "GND/PAL-NTSC")
				(number "41")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DRA0/GND")
				(number "42")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DRA1/DRA0")
				(number "43")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DRA2/DRA1")
				(number "44")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DRA3/DRA2")
				(number "45")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "DRA4/DRA3")
				(number "46")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DRA5/DRA4")
				(number "47")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DRA6/DRA5")
				(number "48")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DRA7/DRA6")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 41.91 0)
				(length 2.54)
				(name "DRD9")
				(number "5")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DRA8/DRA7")
				(number "50")
			)
			(pin input line
				(at -17.78 -41.91 0)
				(length 2.54)
				(name "_LDS/DRA8")
				(number "51")
			)
			(pin input line
				(at -17.78 -44.45 0)
				(length 2.54)
				(name "_UDS/_LDS")
				(number "52")
			)
			(pin output line
				(at 17.78 39.37 180)
				(length 2.54)
				(name "_CASL/_UDS")
				(number "53")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "_CASU/_CASL")
				(number "54")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DRA9/_CASU")
				(number "55")
			)
			(pin output line
				(at 17.78 26.67 180)
				(length 2.54)
				(name "_RAS1")
				(number "56")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "_RAS0")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "A19")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 39.37 0)
				(length 2.54)
				(name "DRD8")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "A1")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "A2")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "A3")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "A4")
				(number "63")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "A5")
				(number "64")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "A6")
				(number "65")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "A7")
				(number "66")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "A8")
				(number "67")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "A9")
				(number "68")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "A10")
				(number "69")
			)
			(pin bidirectional line
				(at -17.78 36.83 0)
				(length 2.54)
				(name "DRD7")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "A11")
				(number "70")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "A12")
				(number "71")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "A13")
				(number "72")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "A14")
				(number "73")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "A15")
				(number "74")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A16")
				(number "75")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "A17")
				(number "76")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "A18")
				(number "77")
			)
			(pin input line
				(at 17.78 -54.61 180)
				(length 2.54)
				(name "_LPEN")
				(number "78")
			)
			(pin bidirectional line
				(at 17.78 -59.69 180)
				(length 2.54)
				(name "_VSYNC")
				(number "79")
			)
			(pin bidirectional line
				(at -17.78 34.29 0)
				(length 2.54)
				(name "DRD6")
				(number "8")
			)
			(pin output line
				(at 17.78 -62.23 180)
				(length 2.54)
				(name "_CSYNC")
				(number "80")
			)
			(pin bidirectional line
				(at 17.78 -57.15 180)
				(length 2.54)
				(name "_HSYNC")
				(number "81")
			)
			(pin bidirectional line
				(at -17.78 57.15 0)
				(length 2.54)
				(name "DRD15")
				(number "83")
			)
			(pin bidirectional line
				(at -17.78 54.61 0)
				(length 2.54)
				(name "DRD14")
				(number "84")
			)
			(pin bidirectional line
				(at -17.78 31.75 0)
				(length 2.54)
				(name "DRD5")
				(number "9")
			)
		)
		(symbol "Agnus Multiadapter_2_1"
			(pin power_in line
				(at 0 8.89 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -3.81 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at 3.81 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "82")
			)
		)
	)
	(symbol "Amiga Internal Floppy Conn"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at -1.27 25.8318 0)
		)
		(property "Value" "INTERNAL FLOPPY"
			(at -1.27 23.5204 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??_*"
			(at 0 0 0)
		)
		(symbol "Amiga Internal Floppy Conn_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
		)
	)
	(symbol "Amiga-2000-Video-Slot"
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at -3.937 0 90)
		)
		(property "Value" "Video-Slot"
			(at -4.318 -36.83 90)
		)
		(property "Footprint" "AmigaPCI:2x18_P2.54mm_Horizontal"
			(at -1.27 0 0)
		)
		(property "Datasheet" ""
			(at 1.27 10.16 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Amiga-2000-Video-Slot_0_1")
		(symbol "Amiga-2000-Video-Slot_1_1"
			(pin unspecified line
				(at 0 43.18 0)
				(length 0)
				(name "1")
				(number "1")
			)
			(pin unspecified line
				(at 2.54 20.32 0)
				(length 0)
				(name "10")
				(number "10")
			)
			(pin unspecified line
				(at 0 17.78 0)
				(length 0)
				(name "11")
				(number "11")
			)
			(pin unspecified line
				(at 2.54 15.24 0)
				(length 0)
				(name "12")
				(number "12")
			)
			(pin unspecified line
				(at 0 12.7 0)
				(length 0)
				(name "13")
				(number "13")
			)
			(pin unspecified line
				(at 2.54 10.16 0)
				(length 0)
				(name "14")
				(number "14")
			)
			(pin unspecified line
				(at 0 7.62 0)
				(length 0)
				(name "15")
				(number "15")
			)
			(pin unspecified line
				(at 2.54 5.08 0)
				(length 0)
				(name "16")
				(number "16")
			)
			(pin unspecified line
				(at 0 2.54 0)
				(length 0)
				(name "17")
				(number "17")
			)
			(pin unspecified line
				(at 2.54 0 0)
				(length 0)
				(name "18")
				(number "18")
			)
			(pin unspecified line
				(at 0 -2.54 0)
				(length 0)
				(name "19")
				(number "19")
			)
			(pin unspecified line
				(at 2.54 40.64 0)
				(length 0)
				(name "2")
				(number "2")
			)
			(pin unspecified line
				(at 2.54 -5.08 0)
				(length 0)
				(name "20")
				(number "20")
			)
			(pin unspecified line
				(at 0 -7.62 0)
				(length 0)
				(name "21")
				(number "21")
			)
			(pin unspecified line
				(at 2.54 -10.16 0)
				(length 0)
				(name "22")
				(number "22")
			)
			(pin unspecified line
				(at 0 -12.7 0)
				(length 0)
				(name "23")
				(number "23")
			)
			(pin unspecified line
				(at 2.54 -15.24 0)
				(length 0)
				(name "24")
				(number "24")
			)
			(pin unspecified line
				(at 0 -17.78 0)
				(length 0)
				(name "25")
				(number "25")
			)
			(pin unspecified line
				(at 2.54 -20.32 0)
				(length 0)
				(name "26")
				(number "26")
			)
			(pin unspecified line
				(at 0 -22.86 0)
				(length 0)
				(name "27")
				(number "27")
			)
			(pin unspecified line
				(at 2.54 -25.4 0)
				(length 0)
				(name "28")
				(number "28")
			)
			(pin unspecified line
				(at 0 -27.94 0)
				(length 0)
				(name "29")
				(number "29")
			)
			(pin unspecified line
				(at 0 38.1 0)
				(length 0)
				(name "3")
				(number "3")
			)
			(pin unspecified line
				(at 2.54 -30.48 0)
				(length 0)
				(name "30")
				(number "30")
			)
			(pin unspecified line
				(at 0 -33.02 0)
				(length 0)
				(name "31")
				(number "31")
			)
			(pin unspecified line
				(at 2.54 -35.56 0)
				(length 0)
				(name "32")
				(number "32")
			)
			(pin unspecified line
				(at 0 -38.1 0)
				(length 0)
				(name "33")
				(number "33")
			)
			(pin unspecified line
				(at 2.54 -40.64 0)
				(length 0)
				(name "34")
				(number "34")
			)
			(pin unspecified line
				(at 0 -43.18 0)
				(length 0)
				(name "35")
				(number "35")
			)
			(pin unspecified line
				(at 2.54 -45.72 0)
				(length 0)
				(name "36")
				(number "36")
			)
			(pin unspecified line
				(at 2.54 35.56 0)
				(length 0)
				(name "4")
				(number "4")
			)
			(pin unspecified line
				(at 0 33.02 0)
				(length 0)
				(name "5")
				(number "5")
			)
			(pin unspecified line
				(at 2.54 30.48 0)
				(length 0)
				(name "6")
				(number "6")
			)
			(pin unspecified line
				(at 0 27.94 0)
				(length 0)
				(name "7")
				(number "7")
			)
			(pin unspecified line
				(at 2.54 25.4 0)
				(length 0)
				(name "8")
				(number "8")
			)
			(pin unspecified line
				(at 0 22.86 0)
				(length 0)
				(name "9")
				(number "9")
			)
		)
	)
	(symbol "AudioJack3-Connector"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at -7.112 0.635 0)
		)
		(property "Value" "AudioJack"
			(at -7.112 -1.6764 0)
		)
		(property "Footprint" "AmigaPCI:Jack_3.5mm_CUI_SJ1-3533NG_Horizontal_CircularHoles"
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part" "SJ1-3533NG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3-Connector_0_1")
		(symbol "AudioJack3-Connector_1_1"
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
	)
	(symbol "CPU-SLOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 0 0 0)
		)
		(property "Value" "CPU SLOT"
			(at 0 0 0)
		)
		(property "Footprint" "A2900:PCIe-x16"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CPU-SLOT_0_0"
			(pin unspecified line
				(at 8.89 152.4 180)
				(length 3.81)
				(name "")
				(number "A1")
			)
			(pin unspecified line
				(at 8.89 118.11 180)
				(length 3.81)
				(name "")
				(number "A10")
			)
			(pin unspecified line
				(at 8.89 114.3 180)
				(length 3.81)
				(name "")
				(number "A11")
			)
			(pin unspecified line
				(at 8.89 110.49 180)
				(length 3.81)
				(name "")
				(number "A12")
			)
			(pin unspecified line
				(at 8.89 106.68 180)
				(length 3.81)
				(name "")
				(number "A13")
			)
			(pin unspecified line
				(at 8.89 102.87 180)
				(length 3.81)
				(name "")
				(number "A14")
			)
			(pin unspecified line
				(at 8.89 99.06 180)
				(length 3.81)
				(name "")
				(number "A15")
			)
			(pin unspecified line
				(at 8.89 95.25 180)
				(length 3.81)
				(name "")
				(number "A16")
			)
			(pin unspecified line
				(at 8.89 91.44 180)
				(length 3.81)
				(name "")
				(number "A17")
			)
			(pin unspecified line
				(at 8.89 87.63 180)
				(length 3.81)
				(name "")
				(number "A18")
			)
			(pin unspecified line
				(at 8.89 83.82 180)
				(length 3.81)
				(name "")
				(number "A19")
			)
			(pin unspecified line
				(at 8.89 148.59 180)
				(length 3.81)
				(name "")
				(number "A2")
			)
			(pin unspecified line
				(at 8.89 80.01 180)
				(length 3.81)
				(name "")
				(number "A20")
			)
			(pin unspecified line
				(at 8.89 76.2 180)
				(length 3.81)
				(name "")
				(number "A21")
			)
			(pin unspecified line
				(at 8.89 72.39 180)
				(length 3.81)
				(name "")
				(number "A22")
			)
			(pin unspecified line
				(at 8.89 68.58 180)
				(length 3.81)
				(name "")
				(number "A23")
			)
			(pin unspecified line
				(at 8.89 64.77 180)
				(length 3.81)
				(name "")
				(number "A24")
			)
			(pin unspecified line
				(at 8.89 60.96 180)
				(length 3.81)
				(name "")
				(number "A25")
			)
			(pin unspecified line
				(at 8.89 57.15 180)
				(length 3.81)
				(name "")
				(number "A26")
			)
			(pin unspecified line
				(at 8.89 53.34 180)
				(length 3.81)
				(name "")
				(number "A27")
			)
			(pin unspecified line
				(at 8.89 49.53 180)
				(length 3.81)
				(name "")
				(number "A28")
			)
			(pin unspecified line
				(at 8.89 45.72 180)
				(length 3.81)
				(name "")
				(number "A29")
			)
			(pin unspecified line
				(at 8.89 144.78 180)
				(length 3.81)
				(name "")
				(number "A3")
			)
			(pin unspecified line
				(at 8.89 41.91 180)
				(length 3.81)
				(name "")
				(number "A30")
			)
			(pin unspecified line
				(at 8.89 38.1 180)
				(length 3.81)
				(name "")
				(number "A31")
			)
			(pin unspecified line
				(at 8.89 34.29 180)
				(length 3.81)
				(name "")
				(number "A32")
			)
			(pin unspecified line
				(at 8.89 30.48 180)
				(length 3.81)
				(name "")
				(number "A33")
			)
			(pin unspecified line
				(at 8.89 26.67 180)
				(length 3.81)
				(name "")
				(number "A34")
			)
			(pin unspecified line
				(at 8.89 22.86 180)
				(length 3.81)
				(name "")
				(number "A35")
			)
			(pin unspecified line
				(at 8.89 19.05 180)
				(length 3.81)
				(name "")
				(number "A36")
			)
			(pin unspecified line
				(at 8.89 15.24 180)
				(length 3.81)
				(name "")
				(number "A37")
			)
			(pin unspecified line
				(at 8.89 11.43 180)
				(length 3.81)
				(name "")
				(number "A38")
			)
			(pin unspecified line
				(at 8.89 7.62 180)
				(length 3.81)
				(name "")
				(number "A39")
			)
			(pin unspecified line
				(at 8.89 140.97 180)
				(length 3.81)
				(name "")
				(number "A4")
			)
			(pin unspecified line
				(at 8.89 3.81 180)
				(length 3.81)
				(name "")
				(number "A40")
			)
			(pin unspecified line
				(at 8.89 0 180)
				(length 3.81)
				(name "")
				(number "A41")
			)
			(pin unspecified line
				(at 8.89 -3.81 180)
				(length 3.81)
				(name "")
				(number "A42")
			)
			(pin unspecified line
				(at 8.89 -7.62 180)
				(length 3.81)
				(name "")
				(number "A43")
			)
			(pin unspecified line
				(at 8.89 -11.43 180)
				(length 3.81)
				(name "")
				(number "A44")
			)
			(pin unspecified line
				(at 8.89 -15.24 180)
				(length 3.81)
				(name "")
				(number "A45")
			)
			(pin unspecified line
				(at 8.89 -19.05 180)
				(length 3.81)
				(name "")
				(number "A46")
			)
			(pin unspecified line
				(at 8.89 -22.86 180)
				(length 3.81)
				(name "")
				(number "A47")
			)
			(pin unspecified line
				(at 8.89 -26.67 180)
				(length 3.81)
				(name "")
				(number "A48")
			)
			(pin unspecified line
				(at 8.89 -30.48 180)
				(length 3.81)
				(name "")
				(number "A49")
			)
			(pin unspecified line
				(at 8.89 137.16 180)
				(length 3.81)
				(name "")
				(number "A5")
			)
			(pin unspecified line
				(at 8.89 -34.29 180)
				(length 3.81)
				(name "")
				(number "A50")
			)
			(pin unspecified line
				(at 8.89 -38.1 180)
				(length 3.81)
				(name "")
				(number "A51")
			)
			(pin unspecified line
				(at 8.89 -41.91 180)
				(length 3.81)
				(name "")
				(number "A52")
			)
			(pin unspecified line
				(at 8.89 -45.72 180)
				(length 3.81)
				(name "")
				(number "A53")
			)
			(pin unspecified line
				(at 8.89 -49.53 180)
				(length 3.81)
				(name "")
				(number "A54")
			)
			(pin unspecified line
				(at 8.89 -53.34 180)
				(length 3.81)
				(name "")
				(number "A55")
			)
			(pin unspecified line
				(at 8.89 -57.15 180)
				(length 3.81)
				(name "")
				(number "A56")
			)
			(pin unspecified line
				(at 8.89 -60.96 180)
				(length 3.81)
				(name "")
				(number "A57")
			)
			(pin unspecified line
				(at 8.89 -64.77 180)
				(length 3.81)
				(name "")
				(number "A58")
			)
			(pin unspecified line
				(at 8.89 -68.58 180)
				(length 3.81)
				(name "")
				(number "A59")
			)
			(pin unspecified line
				(at 8.89 133.35 180)
				(length 3.81)
				(name "")
				(number "A6")
			)
			(pin unspecified line
				(at 8.89 -72.39 180)
				(length 3.81)
				(name "")
				(number "A60")
			)
			(pin unspecified line
				(at 8.89 -76.2 180)
				(length 3.81)
				(name "")
				(number "A61")
			)
			(pin unspecified line
				(at 8.89 -80.01 180)
				(length 3.81)
				(name "")
				(number "A62")
			)
			(pin unspecified line
				(at 8.89 -83.82 180)
				(length 3.81)
				(name "")
				(number "A63")
			)
			(pin unspecified line
				(at 8.89 -87.63 180)
				(length 3.81)
				(name "")
				(number "A64")
			)
			(pin unspecified line
				(at 8.89 -91.44 180)
				(length 3.81)
				(name "")
				(number "A65")
			)
			(pin unspecified line
				(at 8.89 -95.25 180)
				(length 3.81)
				(name "")
				(number "A66")
			)
			(pin unspecified line
				(at 8.89 -99.06 180)
				(length 3.81)
				(name "")
				(number "A67")
			)
			(pin unspecified line
				(at 8.89 -102.87 180)
				(length 3.81)
				(name "")
				(number "A68")
			)
			(pin unspecified line
				(at 8.89 -106.68 180)
				(length 3.81)
				(name "")
				(number "A69")
			)
			(pin unspecified line
				(at 8.89 129.54 180)
				(length 3.81)
				(name "")
				(number "A7")
			)
			(pin unspecified line
				(at 8.89 -110.49 180)
				(length 3.81)
				(name "")
				(number "A70")
			)
			(pin unspecified line
				(at 8.89 -114.3 180)
				(length 3.81)
				(name "")
				(number "A71")
			)
			(pin unspecified line
				(at 8.89 -118.11 180)
				(length 3.81)
				(name "")
				(number "A72")
			)
			(pin unspecified line
				(at 8.89 -121.92 180)
				(length 3.81)
				(name "")
				(number "A73")
			)
			(pin unspecified line
				(at 8.89 -125.73 180)
				(length 3.81)
				(name "")
				(number "A74")
			)
			(pin unspecified line
				(at 8.89 -129.54 180)
				(length 3.81)
				(name "")
				(number "A75")
			)
			(pin unspecified line
				(at 8.89 -133.35 180)
				(length 3.81)
				(name "")
				(number "A76")
			)
			(pin unspecified line
				(at 8.89 -137.16 180)
				(length 3.81)
				(name "")
				(number "A77")
			)
			(pin unspecified line
				(at 8.89 -140.97 180)
				(length 3.81)
				(name "")
				(number "A78")
			)
			(pin unspecified line
				(at 8.89 -144.78 180)
				(length 3.81)
				(name "")
				(number "A79")
			)
			(pin unspecified line
				(at 8.89 125.73 180)
				(length 3.81)
				(name "")
				(number "A8")
			)
			(pin unspecified line
				(at 8.89 -148.59 180)
				(length 3.81)
				(name "")
				(number "A80")
			)
			(pin unspecified line
				(at 8.89 -152.4 180)
				(length 3.81)
				(name "")
				(number "A81")
			)
			(pin unspecified line
				(at 8.89 -156.21 180)
				(length 3.81)
				(name "")
				(number "A82")
			)
			(pin unspecified line
				(at 8.89 121.92 180)
				(length 3.81)
				(name "")
				(number "A9")
			)
			(pin unspecified line
				(at -8.89 152.4 0)
				(length 3.81)
				(name "")
				(number "B1")
			)
			(pin unspecified line
				(at -8.89 118.11 0)
				(length 3.81)
				(name "")
				(number "B10")
			)
			(pin unspecified line
				(at -8.89 114.3 0)
				(length 3.81)
				(name "")
				(number "B11")
			)
			(pin unspecified line
				(at -8.89 110.49 0)
				(length 3.81)
				(name "")
				(number "B12")
			)
			(pin unspecified line
				(at -8.89 106.68 0)
				(length 3.81)
				(name "")
				(number "B13")
			)
			(pin unspecified line
				(at -8.89 102.87 0)
				(length 3.81)
				(name "")
				(number "B14")
			)
			(pin unspecified line
				(at -8.89 99.06 0)
				(length 3.81)
				(name "")
				(number "B15")
			)
			(pin unspecified line
				(at -8.89 95.25 0)
				(length 3.81)
				(name "")
				(number "B16")
			)
			(pin unspecified line
				(at -8.89 91.44 0)
				(length 3.81)
				(name "")
				(number "B17")
			)
			(pin unspecified line
				(at -8.89 87.63 0)
				(length 3.81)
				(name "")
				(number "B18")
			)
			(pin unspecified line
				(at -8.89 83.82 0)
				(length 3.81)
				(name "")
				(number "B19")
			)
			(pin unspecified line
				(at -8.89 148.59 0)
				(length 3.81)
				(name "")
				(number "B2")
			)
			(pin unspecified line
				(at -8.89 80.01 0)
				(length 3.81)
				(name "")
				(number "B20")
			)
			(pin unspecified line
				(at -8.89 76.2 0)
				(length 3.81)
				(name "")
				(number "B21")
			)
			(pin unspecified line
				(at -8.89 72.39 0)
				(length 3.81)
				(name "")
				(number "B22")
			)
			(pin unspecified line
				(at -8.89 68.58 0)
				(length 3.81)
				(name "")
				(number "B23")
			)
			(pin unspecified line
				(at -8.89 64.77 0)
				(length 3.81)
				(name "")
				(number "B24")
			)
			(pin unspecified line
				(at -8.89 60.96 0)
				(length 3.81)
				(name "")
				(number "B25")
			)
			(pin unspecified line
				(at -8.89 57.15 0)
				(length 3.81)
				(name "")
				(number "B26")
			)
			(pin unspecified line
				(at -8.89 53.34 0)
				(length 3.81)
				(name "")
				(number "B27")
			)
			(pin unspecified line
				(at -8.89 49.53 0)
				(length 3.81)
				(name "")
				(number "B28")
			)
			(pin unspecified line
				(at -8.89 45.72 0)
				(length 3.81)
				(name "")
				(number "B29")
			)
			(pin unspecified line
				(at -8.89 144.78 0)
				(length 3.81)
				(name "")
				(number "B3")
			)
			(pin unspecified line
				(at -8.89 41.91 0)
				(length 3.81)
				(name "")
				(number "B30")
			)
			(pin unspecified line
				(at -8.89 38.1 0)
				(length 3.81)
				(name "")
				(number "B31")
			)
			(pin unspecified line
				(at -8.89 34.29 0)
				(length 3.81)
				(name "")
				(number "B32")
			)
			(pin unspecified line
				(at -8.89 30.48 0)
				(length 3.81)
				(name "")
				(number "B33")
			)
			(pin unspecified line
				(at -8.89 26.67 0)
				(length 3.81)
				(name "")
				(number "B34")
			)
			(pin unspecified line
				(at -8.89 22.86 0)
				(length 3.81)
				(name "")
				(number "B35")
			)
			(pin unspecified line
				(at -8.89 19.05 0)
				(length 3.81)
				(name "")
				(number "B36")
			)
			(pin unspecified line
				(at -8.89 15.24 0)
				(length 3.81)
				(name "")
				(number "B37")
			)
			(pin unspecified line
				(at -8.89 11.43 0)
				(length 3.81)
				(name "")
				(number "B38")
			)
			(pin unspecified line
				(at -8.89 7.62 0)
				(length 3.81)
				(name "")
				(number "B39")
			)
			(pin unspecified line
				(at -8.89 140.97 0)
				(length 3.81)
				(name "")
				(number "B4")
			)
			(pin unspecified line
				(at -8.89 3.81 0)
				(length 3.81)
				(name "")
				(number "B40")
			)
			(pin unspecified line
				(at -8.89 0 0)
				(length 3.81)
				(name "")
				(number "B41")
			)
			(pin unspecified line
				(at -8.89 -3.81 0)
				(length 3.81)
				(name "")
				(number "B42")
			)
			(pin unspecified line
				(at -8.89 -7.62 0)
				(length 3.81)
				(name "")
				(number "B43")
			)
			(pin unspecified line
				(at -8.89 -11.43 0)
				(length 3.81)
				(name "")
				(number "B44")
			)
			(pin unspecified line
				(at -8.89 -15.24 0)
				(length 3.81)
				(name "")
				(number "B45")
			)
			(pin unspecified line
				(at -8.89 -19.05 0)
				(length 3.81)
				(name "")
				(number "B46")
			)
			(pin unspecified line
				(at -8.89 -22.86 0)
				(length 3.81)
				(name "")
				(number "B47")
			)
			(pin unspecified line
				(at -8.89 -26.67 0)
				(length 3.81)
				(name "")
				(number "B48")
			)
			(pin unspecified line
				(at -8.89 -30.48 0)
				(length 3.81)
				(name "")
				(number "B49")
			)
			(pin unspecified line
				(at -8.89 137.16 0)
				(length 3.81)
				(name "")
				(number "B5")
			)
			(pin unspecified line
				(at -8.89 -34.29 0)
				(length 3.81)
				(name "")
				(number "B50")
			)
			(pin unspecified line
				(at -8.89 -38.1 0)
				(length 3.81)
				(name "")
				(number "B51")
			)
			(pin unspecified line
				(at -8.89 -41.91 0)
				(length 3.81)
				(name "")
				(number "B52")
			)
			(pin unspecified line
				(at -8.89 -45.72 0)
				(length 3.81)
				(name "")
				(number "B53")
			)
			(pin unspecified line
				(at -8.89 -49.53 0)
				(length 3.81)
				(name "")
				(number "B54")
			)
			(pin unspecified line
				(at -8.89 -53.34 0)
				(length 3.81)
				(name "")
				(number "B55")
			)
			(pin unspecified line
				(at -8.89 -57.15 0)
				(length 3.81)
				(name "")
				(number "B56")
			)
			(pin unspecified line
				(at -8.89 -60.96 0)
				(length 3.81)
				(name "")
				(number "B57")
			)
			(pin unspecified line
				(at -8.89 -64.77 0)
				(length 3.81)
				(name "")
				(number "B58")
			)
			(pin unspecified line
				(at -8.89 -68.58 0)
				(length 3.81)
				(name "")
				(number "B59")
			)
			(pin unspecified line
				(at -8.89 133.35 0)
				(length 3.81)
				(name "")
				(number "B6")
			)
			(pin unspecified line
				(at -8.89 -72.39 0)
				(length 3.81)
				(name "")
				(number "B60")
			)
			(pin unspecified line
				(at -8.89 -76.2 0)
				(length 3.81)
				(name "")
				(number "B61")
			)
			(pin unspecified line
				(at -8.89 -80.01 0)
				(length 3.81)
				(name "")
				(number "B62")
			)
			(pin unspecified line
				(at -8.89 -83.82 0)
				(length 3.81)
				(name "")
				(number "B63")
			)
			(pin unspecified line
				(at -8.89 -87.63 0)
				(length 3.81)
				(name "")
				(number "B64")
			)
			(pin unspecified line
				(at -8.89 -91.44 0)
				(length 3.81)
				(name "")
				(number "B65")
			)
			(pin unspecified line
				(at -8.89 -95.25 0)
				(length 3.81)
				(name "")
				(number "B66")
			)
			(pin unspecified line
				(at -8.89 -99.06 0)
				(length 3.81)
				(name "")
				(number "B67")
			)
			(pin unspecified line
				(at -8.89 -102.87 0)
				(length 3.81)
				(name "")
				(number "B68")
			)
			(pin unspecified line
				(at -8.89 -106.68 0)
				(length 3.81)
				(name "")
				(number "B69")
			)
			(pin unspecified line
				(at -8.89 129.54 0)
				(length 3.81)
				(name "")
				(number "B7")
			)
			(pin unspecified line
				(at -8.89 -110.49 0)
				(length 3.81)
				(name "")
				(number "B70")
			)
			(pin unspecified line
				(at -8.89 -114.3 0)
				(length 3.81)
				(name "")
				(number "B71")
			)
			(pin unspecified line
				(at -8.89 -118.11 0)
				(length 3.81)
				(name "")
				(number "B72")
			)
			(pin unspecified line
				(at -8.89 -121.92 0)
				(length 3.81)
				(name "")
				(number "B73")
			)
			(pin unspecified line
				(at -8.89 -125.73 0)
				(length 3.81)
				(name "")
				(number "B74")
			)
			(pin unspecified line
				(at -8.89 -129.54 0)
				(length 3.81)
				(name "")
				(number "B75")
			)
			(pin unspecified line
				(at -8.89 -133.35 0)
				(length 3.81)
				(name "")
				(number "B76")
			)
			(pin unspecified line
				(at -8.89 -137.16 0)
				(length 3.81)
				(name "")
				(number "B77")
			)
			(pin unspecified line
				(at -8.89 -140.97 0)
				(length 3.81)
				(name "")
				(number "B78")
			)
			(pin unspecified line
				(at -8.89 -144.78 0)
				(length 3.81)
				(name "")
				(number "B79")
			)
			(pin unspecified line
				(at -8.89 125.73 0)
				(length 3.81)
				(name "")
				(number "B8")
			)
			(pin unspecified line
				(at -8.89 -148.59 0)
				(length 3.81)
				(name "")
				(number "B80")
			)
			(pin unspecified line
				(at -8.89 -152.4 0)
				(length 3.81)
				(name "")
				(number "B81")
			)
			(pin unspecified line
				(at -8.89 -156.21 0)
				(length 3.81)
				(name "")
				(number "B82")
			)
			(pin unspecified line
				(at -8.89 121.92 0)
				(length 3.81)
				(name "")
				(number "B9")
			)
		)
		(symbol "CPU-SLOT_0_1")
	)
	(symbol "CP_Small-Device"
		(pin_numbers hide)
		(pin_names
			(offset 0.254) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at -2.2352 -1.1684 0)
		)
		(property "Value" ""
			(at -2.2352 1.143 0)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP_*"
			(at 0 0 0)
		)
		(symbol "CP_Small-Device_0_1")
		(symbol "CP_Small-Device_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 1.8542)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 1.8542)
				(name "~")
				(number "2")
			)
		)
	)
	(symbol "C_Feedthrough_Small"
		(pin_names
			(offset 0.254) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "EMI"
			(at 0 2.54 0)
		)
		(property "Value" "C_Feedthrough_Small"
			(at 0 5.715 0)
		)
		(property "Footprint" "AmigaFootprints:C_1206_3216_Feedthrough"
			(at 0 0 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Feedthrough capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI filter feedthrough capacitor"
			(at 0 0 0)
		)
		(symbol "C_Feedthrough_Small_0_1")
		(symbol "C_Feedthrough_Small_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 0 -1.27 90)
				(length 0.9906)
				(name "3")
				(number "3")
			)
		)
	)
	(symbol "C_Pack04"
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CA"
			(at -6.604 0 90)
		)
		(property "Value" "C_Pack04"
			(at 6.096 0 90)
		)
		(property "Footprint" ""
			(at 8.001 0 90)
		)
		(property "Datasheet" "~"
			(at 1.016 0 0)
		)
		(property "Description" "4 Capacitor Pack"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* SOIC* R*Array*Concave* R*Array*Convex*"
			(at 0 0 0)
		)
		(symbol "C_Pack04_0_1")
		(symbol "C_Pack04_1_1"
			(pin passive line
				(at -4.064 -5.08 90)
				(length 2.54)
				(name "R1.1")
				(number "1")
			)
			(pin passive line
				(at -1.524 -5.08 90)
				(length 2.54)
				(name "R2.1")
				(number "2")
			)
			(pin passive line
				(at 1.016 -5.08 90)
				(length 2.54)
				(name "R3.1")
				(number "3")
			)
			(pin passive line
				(at 3.556 -5.08 90)
				(length 2.54)
				(name "R4.1")
				(number "4")
			)
			(pin passive line
				(at 3.556 5.08 270)
				(length 2.54)
				(name "R4.2")
				(number "5")
			)
			(pin passive line
				(at 1.016 5.08 270)
				(length 2.54)
				(name "R3.2")
				(number "6")
			)
			(pin passive line
				(at -1.524 5.08 270)
				(length 2.54)
				(name "R2.2")
				(number "7")
			)
			(pin passive line
				(at -4.064 5.08 270)
				(length 2.54)
				(name "R1.2")
				(number "8")
			)
		)
	)
	(symbol "Conn_02x20_IDE"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 1.27 27.94 0)
		)
		(property "Value" "IDE"
			(at 1.27 26.019 0)
		)
		(property "Footprint" "AmigaPCI:ATA_Header_2x20_P2.54mm"
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_IDE_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
		)
	)
	(symbol "DB15_Female_HighDensity"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN202"
			(at 0 22.0218 0)
		)
		(property "Value" "DB15_Female_HighDensity"
			(at 0 19.7104 0)
		)
		(property "Footprint" "AmigaFootprints:DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm"
			(at -24.13 10.16 0)
		)
		(property "Datasheet" " ~"
			(at -24.13 10.16 0)
		)
		(property "Description" "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector db15 VGA female D-SUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Female*"
			(at 0 0 0)
		)
		(symbol "DB15_Female_HighDensity_0_1")
		(symbol "DB15_Female_HighDensity_1_0"
			(pin passive line
				(at 3.81 -17.78 90)
				(length 5.08)
				(name "SHIELD")
				(number "16")
			)
		)
		(symbol "DB15_Female_HighDensity_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
		)
	)
	(symbol "DB25_Stack_FemaleAndMale"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 34.29 0)
		)
		(property "Value" "DB25_Stack_FemaleAndMale"
			(at 12.7 -35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" " ~"
			(at 0 0 0)
		)
		(property "Description" "25-pin female D-SUB connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "female D-SUB connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Female*"
			(at 0 0 0)
		)
		(symbol "DB25_Stack_FemaleAndMale_0_1")
		(symbol "DB25_Stack_FemaleAndMale_1_0"
			(text "Female_Bottom"
				(at 0 -38.1 0)
			)
		)
		(symbol "DB25_Stack_FemaleAndMale_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
		)
		(symbol "DB25_Stack_FemaleAndMale_2_0"
			(text "Male_Top"
				(at 5.08 -38.1 0)
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 5.02)
				(name "GND")
				(number "51")
			)
		)
		(symbol "DB25_Stack_FemaleAndMale_2_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "38")
				(number "38")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "39")
				(number "39")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "40")
				(number "40")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "41")
				(number "41")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "42")
				(number "42")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "43")
				(number "43")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "50")
				(number "50")
			)
		)
	)
	(symbol "DB9_Male_Stack"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9_Male_Stack"
			(at 5.08 -13.97 0)
		)
		(property "Footprint" "AmigaFootprints:DSUB-9_Male_Stack"
			(at 0 0 0)
		)
		(property "Datasheet" " ~"
			(at 0 0 0)
		)
		(property "Description" "9-pin male D-SUB connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector male D-SUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Male*"
			(at 0 0 0)
		)
		(symbol "DB9_Male_Stack_0_1")
		(symbol "DB9_Male_Stack_1_1"
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
		)
		(symbol "DB9_Male_Stack_2_0"
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "19")
			)
		)
		(symbol "DB9_Male_Stack_2_1"
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "18")
				(number "18")
			)
		)
	)
	(symbol "DIN41612_03x40"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 77.724 0)
		)
		(property "Value" "DIN41612_03x40"
			(at -0.254 2.032 0)
		)
		(property "Footprint" ""
			(at -1.27 41.91 0)
		)
		(property "Datasheet" "~"
			(at -1.27 41.91 0)
		)
		(property "Description" "DIN41612 connector, three row, 03x40"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_03x40_1_0"
			(pin passive line
				(at -6.35 74.93 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -6.35 6.35 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -6.35 -16.51 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -6.35 -24.13 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -6.35 -31.75 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -6.35 -46.99 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -6.35 -54.61 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -6.35 -62.23 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -6.35 67.31 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at 6.35 74.93 180)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at 6.35 67.31 180)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at 6.35 59.69 180)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at 6.35 52.07 180)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at 6.35 36.83 180)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at 6.35 29.21 180)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at 6.35 21.59 180)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at 6.35 6.35 180)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at 6.35 -8.89 180)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 6.35 -16.51 180)
				(length 3.81)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at 6.35 -31.75 180)
				(length 3.81)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at 6.35 -39.37 180)
				(length 3.81)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at 6.35 -46.99 180)
				(length 3.81)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at 6.35 -62.23 180)
				(length 3.81)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -6.35 52.07 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at 6.35 -69.85 180)
				(length 3.81)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -6.35 44.45 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -6.35 36.83 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -6.35 21.59 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -6.35 13.97 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -6.35 72.39 0)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at -6.35 3.81 0)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at -6.35 -11.43 0)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at -6.35 -19.05 0)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at -6.35 -26.67 0)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at -6.35 -34.29 0)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at -6.35 -49.53 0)
				(length 3.81)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at -6.35 -57.15 0)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at -6.35 -64.77 0)
				(length 3.81)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 6.35 72.39 180)
				(length 3.81)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 6.35 64.77 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 6.35 57.15 180)
				(length 3.81)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 6.35 34.29 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 6.35 26.67 180)
				(length 3.81)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 6.35 19.05 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 6.35 3.81 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 3.81)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 6.35 -11.43 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 6.35 -26.67 180)
				(length 3.81)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 6.35 -34.29 180)
				(length 3.81)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 6.35 -41.91 180)
				(length 3.81)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 6.35 -49.53 180)
				(length 3.81)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 6.35 -64.77 180)
				(length 3.81)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at -6.35 49.53 0)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 6.35 -72.39 180)
				(length 3.81)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at -6.35 41.91 0)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at -6.35 34.29 0)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at -6.35 19.05 0)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at -6.35 11.43 0)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at -6.35 69.85 0)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at -6.35 -13.97 0)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at -6.35 -21.59 0)
				(length 3.81)
				(name "Pin_c13")
				(number "c13")
			)
			(pin passive line
				(at -6.35 -29.21 0)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at -6.35 -44.45 0)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
			(pin passive line
				(at -6.35 -52.07 0)
				(length 3.81)
				(name "Pin_c17")
				(number "c17")
			)
			(pin passive line
				(at -6.35 -59.69 0)
				(length 3.81)
				(name "Pin_c18")
				(number "c18")
			)
			(pin passive line
				(at -6.35 -67.31 0)
				(length 3.81)
				(name "Pin_c19")
				(number "c19")
			)
			(pin passive line
				(at 6.35 69.85 180)
				(length 3.81)
				(name "Pin_c21")
				(number "c21")
			)
			(pin passive line
				(at 6.35 62.23 180)
				(length 3.81)
				(name "Pin_c22")
				(number "c22")
			)
			(pin passive line
				(at 6.35 54.61 180)
				(length 3.81)
				(name "Pin_c23")
				(number "c23")
			)
			(pin passive line
				(at 6.35 39.37 180)
				(length 3.81)
				(name "Pin_c25")
				(number "c25")
			)
			(pin passive line
				(at 6.35 31.75 180)
				(length 3.81)
				(name "Pin_c26")
				(number "c26")
			)
			(pin passive line
				(at 6.35 24.13 180)
				(length 3.81)
				(name "Pin_c27")
				(number "c27")
			)
			(pin passive line
				(at -6.35 54.61 0)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at 6.35 1.27 180)
				(length 3.81)
				(name "Pin_c30")
				(number "c30")
			)
			(pin passive line
				(at 6.35 -6.35 180)
				(length 3.81)
				(name "Pin_c31")
				(number "c31")
			)
			(pin passive line
				(at 6.35 -13.97 180)
				(length 3.81)
				(name "Pin_c32")
				(number "c32")
			)
			(pin passive line
				(at 6.35 -29.21 180)
				(length 3.81)
				(name "Pin_c34")
				(number "c34")
			)
			(pin passive line
				(at 6.35 -36.83 180)
				(length 3.81)
				(name "Pin_c35")
				(number "c35")
			)
			(pin passive line
				(at 6.35 -44.45 180)
				(length 3.81)
				(name "Pin_c36")
				(number "c36")
			)
			(pin passive line
				(at 6.35 -59.69 180)
				(length 3.81)
				(name "Pin_c38")
				(number "c38")
			)
			(pin passive line
				(at 6.35 -67.31 180)
				(length 3.81)
				(name "Pin_c39")
				(number "c39")
			)
			(pin passive line
				(at -6.35 46.99 0)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 6.35 -74.93 180)
				(length 3.81)
				(name "Pin_c40")
				(number "c40")
			)
			(pin passive line
				(at -6.35 39.37 0)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at -6.35 16.51 0)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at -6.35 8.89 0)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
		)
		(symbol "DIN41612_03x40_1_1"
			(pin passive line
				(at -6.35 -1.27 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -6.35 -8.89 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -6.35 -39.37 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -6.35 -69.85 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at 6.35 44.45 180)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at 6.35 13.97 180)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -6.35 59.69 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at 6.35 -24.13 180)
				(length 3.81)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at 6.35 -54.61 180)
				(length 3.81)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -6.35 29.21 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -6.35 -3.81 0)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at -6.35 -41.91 0)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at -6.35 64.77 0)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at -6.35 -72.39 0)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 6.35 49.53 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 6.35 41.91 180)
				(length 3.81)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 6.35 11.43 180)
				(length 3.81)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at -6.35 57.15 0)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 6.35 -19.05 180)
				(length 3.81)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 6.35 -57.15 180)
				(length 3.81)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at -6.35 26.67 0)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at -6.35 -6.35 0)
				(length 3.81)
				(name "Pin_c11")
				(number "c11")
			)
			(pin passive line
				(at -6.35 -36.83 0)
				(length 3.81)
				(name "Pin_c15")
				(number "c15")
			)
			(pin passive line
				(at -6.35 62.23 0)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at -6.35 -74.93 0)
				(length 3.81)
				(name "Pin_c20")
				(number "c20")
			)
			(pin passive line
				(at 6.35 46.99 180)
				(length 3.81)
				(name "Pin_c24")
				(number "c24")
			)
			(pin passive line
				(at 6.35 16.51 180)
				(length 3.81)
				(name "Pin_c28")
				(number "c28")
			)
			(pin passive line
				(at 6.35 8.89 180)
				(length 3.81)
				(name "Pin_c29")
				(number "c29")
			)
			(pin passive line
				(at 6.35 -21.59 180)
				(length 3.81)
				(name "Pin_c33")
				(number "c33")
			)
			(pin passive line
				(at 6.35 -52.07 180)
				(length 3.81)
				(name "Pin_c37")
				(number "c37")
			)
			(pin passive line
				(at -6.35 31.75 0)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at -6.35 24.13 0)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
		)
	)
	(symbol "DIN41612_04x32_GROUPED"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 82.55 0)
		)
		(property "Value" "DIN41612_04x32_GROUPED"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at -1.27 41.91 0)
		)
		(property "Datasheet" "~"
			(at -1.27 41.91 0)
		)
		(property "Description" "DIN41612 connector, four row, 04x32"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_04x32_GROUPED_1_0"
			(pin passive line
				(at -6.35 80.01 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at 6.35 80.01 180)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at 6.35 69.85 180)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at 6.35 59.69 180)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -6.35 69.85 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at 6.35 49.53 180)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at 6.35 39.37 180)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at 6.35 29.21 180)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at 6.35 19.05 180)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at 6.35 8.89 180)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -6.35 59.69 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -6.35 49.53 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -6.35 39.37 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -6.35 29.21 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -6.35 19.05 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -6.35 8.89 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -6.35 77.47 0)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 6.35 77.47 180)
				(length 3.81)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 6.35 67.31 180)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 6.35 57.15 180)
				(length 3.81)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at -6.35 67.31 0)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 6.35 46.99 180)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 6.35 36.83 180)
				(length 3.81)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 6.35 26.67 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 6.35 16.51 180)
				(length 3.81)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 6.35 6.35 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at -6.35 57.15 0)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at -6.35 46.99 0)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at -6.35 36.83 0)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at -6.35 26.67 0)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at -6.35 16.51 0)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at -6.35 6.35 0)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at -6.35 74.93 0)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at 6.35 74.93 180)
				(length 3.81)
				(name "Pin_c17")
				(number "c17")
			)
			(pin passive line
				(at 6.35 64.77 180)
				(length 3.81)
				(name "Pin_c18")
				(number "c18")
			)
			(pin passive line
				(at 6.35 54.61 180)
				(length 3.81)
				(name "Pin_c19")
				(number "c19")
			)
			(pin passive line
				(at -6.35 64.77 0)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 6.35 44.45 180)
				(length 3.81)
				(name "Pin_c20")
				(number "c20")
			)
			(pin passive line
				(at 6.35 34.29 180)
				(length 3.81)
				(name "Pin_c21")
				(number "c21")
			)
			(pin passive line
				(at 6.35 24.13 180)
				(length 3.81)
				(name "Pin_c22")
				(number "c22")
			)
			(pin passive line
				(at 6.35 13.97 180)
				(length 3.81)
				(name "Pin_c23")
				(number "c23")
			)
			(pin passive line
				(at 6.35 3.81 180)
				(length 3.81)
				(name "Pin_c24")
				(number "c24")
			)
			(pin passive line
				(at -6.35 54.61 0)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at -6.35 44.45 0)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at -6.35 34.29 0)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at -6.35 24.13 0)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at -6.35 13.97 0)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
			(pin passive line
				(at -6.35 3.81 0)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at -6.35 72.39 0)
				(length 3.81)
				(name "Pin_d1")
				(number "d1")
			)
			(pin passive line
				(at 6.35 72.39 180)
				(length 3.81)
				(name "Pin_d17")
				(number "d17")
			)
			(pin passive line
				(at 6.35 62.23 180)
				(length 3.81)
				(name "Pin_d18")
				(number "d18")
			)
			(pin passive line
				(at 6.35 52.07 180)
				(length 3.81)
				(name "Pin_d19")
				(number "d19")
			)
			(pin passive line
				(at -6.35 62.23 0)
				(length 3.81)
				(name "Pin_d2")
				(number "d2")
			)
			(pin passive line
				(at 6.35 41.91 180)
				(length 3.81)
				(name "Pin_d20")
				(number "d20")
			)
			(pin passive line
				(at 6.35 31.75 180)
				(length 3.81)
				(name "Pin_d21")
				(number "d21")
			)
			(pin passive line
				(at 6.35 21.59 180)
				(length 3.81)
				(name "Pin_d22")
				(number "d22")
			)
			(pin passive line
				(at 6.35 11.43 180)
				(length 3.81)
				(name "Pin_d23")
				(number "d23")
			)
			(pin passive line
				(at 6.35 1.27 180)
				(length 3.81)
				(name "Pin_d24")
				(number "d24")
			)
			(pin passive line
				(at -6.35 52.07 0)
				(length 3.81)
				(name "Pin_d3")
				(number "d3")
			)
			(pin passive line
				(at -6.35 41.91 0)
				(length 3.81)
				(name "Pin_d4")
				(number "d4")
			)
			(pin passive line
				(at -6.35 31.75 0)
				(length 3.81)
				(name "Pin_d5")
				(number "d5")
			)
			(pin passive line
				(at -6.35 21.59 0)
				(length 3.81)
				(name "Pin_d6")
				(number "d6")
			)
			(pin passive line
				(at -6.35 11.43 0)
				(length 3.81)
				(name "Pin_d7")
				(number "d7")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 3.81)
				(name "Pin_d8")
				(number "d8")
			)
		)
		(symbol "DIN41612_04x32_GROUPED_1_1"
			(pin passive line
				(at -6.35 -11.43 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -6.35 -21.59 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -6.35 -31.75 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -6.35 -41.91 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -6.35 -52.07 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -6.35 -62.23 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -6.35 -72.39 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at 6.35 -11.43 180)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at 6.35 -21.59 180)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at 6.35 -31.75 180)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at 6.35 -41.91 180)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at 6.35 -52.07 180)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at 6.35 -62.23 180)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at 6.35 -72.39 180)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -6.35 -1.27 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -6.35 -13.97 0)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at -6.35 -24.13 0)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at -6.35 -34.29 0)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at -6.35 -44.45 0)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at -6.35 -54.61 0)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at -6.35 -64.77 0)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at -6.35 -74.93 0)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 3.81)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 6.35 -13.97 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 6.35 -24.13 180)
				(length 3.81)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 6.35 -34.29 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 6.35 -44.45 180)
				(length 3.81)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 6.35 -54.61 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 6.35 -64.77 180)
				(length 3.81)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 6.35 -74.93 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at -6.35 -3.81 0)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at -6.35 -16.51 0)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at -6.35 -26.67 0)
				(length 3.81)
				(name "Pin_c11")
				(number "c11")
			)
			(pin passive line
				(at -6.35 -36.83 0)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at -6.35 -46.99 0)
				(length 3.81)
				(name "Pin_c13")
				(number "c13")
			)
			(pin passive line
				(at -6.35 -57.15 0)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at -6.35 -67.31 0)
				(length 3.81)
				(name "Pin_c15")
				(number "c15")
			)
			(pin passive line
				(at -6.35 -77.47 0)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
			(pin passive line
				(at 6.35 -6.35 180)
				(length 3.81)
				(name "Pin_c25")
				(number "c25")
			)
			(pin passive line
				(at 6.35 -16.51 180)
				(length 3.81)
				(name "Pin_c26")
				(number "c26")
			)
			(pin passive line
				(at 6.35 -26.67 180)
				(length 3.81)
				(name "Pin_c27")
				(number "c27")
			)
			(pin passive line
				(at 6.35 -36.83 180)
				(length 3.81)
				(name "Pin_c28")
				(number "c28")
			)
			(pin passive line
				(at 6.35 -46.99 180)
				(length 3.81)
				(name "Pin_c29")
				(number "c29")
			)
			(pin passive line
				(at 6.35 -57.15 180)
				(length 3.81)
				(name "Pin_c30")
				(number "c30")
			)
			(pin passive line
				(at 6.35 -67.31 180)
				(length 3.81)
				(name "Pin_c31")
				(number "c31")
			)
			(pin passive line
				(at 6.35 -77.47 180)
				(length 3.81)
				(name "Pin_c32")
				(number "c32")
			)
			(pin passive line
				(at -6.35 -6.35 0)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
			(pin passive line
				(at -6.35 -19.05 0)
				(length 3.81)
				(name "Pin_d10")
				(number "d10")
			)
			(pin passive line
				(at -6.35 -29.21 0)
				(length 3.81)
				(name "Pin_d11")
				(number "d11")
			)
			(pin passive line
				(at -6.35 -39.37 0)
				(length 3.81)
				(name "Pin_d12")
				(number "d12")
			)
			(pin passive line
				(at -6.35 -49.53 0)
				(length 3.81)
				(name "Pin_d13")
				(number "d13")
			)
			(pin passive line
				(at -6.35 -59.69 0)
				(length 3.81)
				(name "Pin_d14")
				(number "d14")
			)
			(pin passive line
				(at -6.35 -69.85 0)
				(length 3.81)
				(name "Pin_d15")
				(number "d15")
			)
			(pin passive line
				(at -6.35 -80.01 0)
				(length 3.81)
				(name "Pin_d16")
				(number "d16")
			)
			(pin passive line
				(at 6.35 -8.89 180)
				(length 3.81)
				(name "Pin_d25")
				(number "d25")
			)
			(pin passive line
				(at 6.35 -19.05 180)
				(length 3.81)
				(name "Pin_d26")
				(number "d26")
			)
			(pin passive line
				(at 6.35 -29.21 180)
				(length 3.81)
				(name "Pin_d27")
				(number "d27")
			)
			(pin passive line
				(at 6.35 -39.37 180)
				(length 3.81)
				(name "Pin_d28")
				(number "d28")
			)
			(pin passive line
				(at 6.35 -49.53 180)
				(length 3.81)
				(name "Pin_d29")
				(number "d29")
			)
			(pin passive line
				(at 6.35 -59.69 180)
				(length 3.81)
				(name "Pin_d30")
				(number "d30")
			)
			(pin passive line
				(at 6.35 -69.85 180)
				(length 3.81)
				(name "Pin_d31")
				(number "d31")
			)
			(pin passive line
				(at 6.35 -80.01 180)
				(length 3.81)
				(name "Pin_d32")
				(number "d32")
			)
			(pin passive line
				(at -6.35 -8.89 0)
				(length 3.81)
				(name "Pin_d9")
				(number "d9")
			)
		)
	)
	(symbol "DS1813"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.271 -2.54 90)
		)
		(property "Value" "DS1813"
			(at -6.9596 -2.54 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "DS1813_0_1")
		(symbol "DS1813_1_1"
			(pin bidirectional line
				(at -2.54 -11.43 90)
				(length 2.54)
				(name "/RST")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -11.43 90)
				(length 2.54)
				(name "Vcc")
				(number "2")
			)
			(pin power_in line
				(at 0 6.35 270)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
	)
	(symbol "Ferrite_Bead"
		(pin_numbers hide)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FB"
			(at 1.27 -5.588 90)
		)
		(property "Value" "80R"
			(at 3.048 -4.572 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at -1.778 0 90)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Inductor_* L_* *Ferrite*"
			(at 0 0 0)
		)
		(symbol "Ferrite_Bead_0_1")
		(symbol "Ferrite_Bead_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
	)
	(symbol "ICE40HX1K-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.3319 69.3826 0)
		)
		(property "Value" "ICE40HX1K-VQ100"
			(at -20.3264 -114.3223 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PARTREV" "3.4"
			(at 0 0 0)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "LATTICE SEMICONDUCTOR"
			(at 0 0 0)
		)
		(property "PACKAGE" "QFP-100"
			(at 0 0 0)
		)
		(symbol "ICE40HX1K-VQ100_0_0"
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IOL_1A")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IOL_5B")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IOT_95")
				(number "100")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "VCC")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IOL_6A")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IOL_6B_GBIN7")
				(number "13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "VCCIO_3__1")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IOL_7A_GBIN6")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IOL_7B")
				(number "16")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 5.08)
				(name "GND__1")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IOL_8A")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IOL_8B")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "IOL_1B")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IOL_10A")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IOL_10B")
				(number "21")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "VCCIO_3__2")
				(number "22")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 5.08)
				(name "GND__2")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "IOL_12A")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IOL_12B")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IOB_26")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IOB_27")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IOB_28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IOB_29")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IOL_2A")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IOB_30")
				(number "30")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "VCCIO_2")
				(number "31")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 5.08)
				(name "GND__3")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IOB_35_GBIN5")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IOB_36_GBIN4")
				(number "34")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "VCC__1")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IOB_34")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IOB_37")
				(number "37")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "VCCIO_2__1")
				(number "38")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 5.08)
				(name "GND__4")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IOL_2B")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IOB_41")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IOB_42_CBSEL0")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "IOB_43_CBSEL1")
				(number "42")
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "CDONE")
				(number "43")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "CRESET_B")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "IOB_44_SDO")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "IOB_45_SDI")
				(number "46")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 5.08)
				(name "GND__5")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "IOB_46_SCK")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "IOB_47_SS")
				(number "49")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "VCC_SPI")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -81.28 180)
				(length 5.08)
				(name "IOR_52")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 -78.74 180)
				(length 5.08)
				(name "IOR_53")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -76.2 180)
				(length 5.08)
				(name "IOR_54")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -73.66 180)
				(length 5.08)
				(name "IOR_55")
				(number "54")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 5.08)
				(name "GND__6")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -71.12 180)
				(length 5.08)
				(name "IOR_56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -68.58 180)
				(length 5.08)
				(name "IOR_57")
				(number "57")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 5.08)
				(name "VCCIO_1")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 -66.04 180)
				(length 5.08)
				(name "IOR_58")
				(number "59")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "VCCIO_3")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -63.5 180)
				(length 5.08)
				(name "IOR_59")
				(number "60")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "VCC__2")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "IOR_60_GBIN3")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "IOR_61_GBIN2")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "IOR_63")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "IOR_64")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IOR_65")
				(number "66")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "VCCIO_1__1")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IOR_67")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IOR_68")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IOL_3A")
				(number "7")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 5.08)
				(name "GND__7")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IOR_69")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IOR_70")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IOR_71")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "IOR_72")
				(number "74")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "VPP_2V5")
				(number "75")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "VPP_FAST")
				(number "76")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "VCC__3")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "IOT_73")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IOT_74")
				(number "79")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IOL_3B")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IOT_75")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IOT_77")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IOT_78")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IOT_79")
				(number "83")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 5.08)
				(name "GND__8")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IOT_80")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IOT_81")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IOT_82")
				(number "87")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "VCCIO_0")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IOT_84_GBIN1")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IOL_5A")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IOT_85_GBIN0")
				(number "90")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IOT_86")
				(number "91")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "VCCIO_0__1")
				(number "92")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IOT_87")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IOT_88")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IOT_89")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IOT_90")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IOT_91")
				(number "97")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 5.08)
				(name "GND__9")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IOT_93")
				(number "99")
			)
		)
	)
	(symbol "ICE40HX4K-TQ144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 88.9 0)
		)
		(property "Value" "ICE40HX4K-TQ144"
			(at -20.32 -106.68 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" ""
			(at 0 -12.7 0)
		)
		(property "Description" "IC FPGA 107 I/O 144TQFP"
			(at 0 -12.7 0)
		)
		(property "MF" "Lattice Semiconductor"
			(at 0 -12.7 0)
		)
		(property "Package" "TQFP-144 Lattice Semiconductor"
			(at 0 -12.7 0)
		)
		(property "Price" "None"
			(at 0 -12.7 0)
		)
		(property "MP" "ICE40HX4K-TQ144"
			(at 0 -12.7 0)
		)
		(property "Availability" "Unavailable"
			(at 0 -12.7 0)
		)
		(symbol "ICE40HX4K-TQ144_0_0"
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "IO3_2A")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "IO3_5B")
				(number "10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 5.08)
				(name "VCCIO_1__1")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "IO1_160")
				(number "101")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IO1_161")
				(number "102")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 5.08)
				(name "GND__6")
				(number "103")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "IO1_164")
				(number "104")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "IO1_165")
				(number "105")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "IO1_166")
				(number "106")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "IO1_167")
				(number "107")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 5.08)
				(name "VPP_2V5")
				(number "108")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 5.08)
				(name "VPP_FAST")
				(number "109")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "IO3_8A")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "IO0_168")
				(number "110")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 5.08)
				(name "VCC__3")
				(number "111")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 5.08)
				(name "IO0_169")
				(number "112")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 5.08)
				(name "IO0_170")
				(number "113")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 5.08)
				(name "IO0_171")
				(number "114")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 5.08)
				(name "IO0_172")
				(number "115")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 5.08)
				(name "IO0_173")
				(number "116")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 5.08)
				(name "IO0_174")
				(number "117")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 5.08)
				(name "IO0_177")
				(number "118")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 5.08)
				(name "IO0_178")
				(number "119")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "IO3_8B")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 5.08)
				(name "IO0_179")
				(number "120")
			)
			(pin bidirectional line
				(at 25.4 -63.5 180)
				(length 5.08)
				(name "IO0_181")
				(number "121")
			)
			(pin bidirectional line
				(at 25.4 -66.04 180)
				(length 5.08)
				(name "IO0_190")
				(number "122")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 5.08)
				(name "VCCIO_0")
				(number "123")
			)
			(pin bidirectional line
				(at 25.4 -68.58 180)
				(length 5.08)
				(name "IO0_191")
				(number "124")
			)
			(pin bidirectional line
				(at 25.4 -71.12 180)
				(length 5.08)
				(name "IO0_192")
				(number "125")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 5.08)
				(name "VCCPLL1")
				(number "126")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 5.08)
				(name "GNDPLL1")
				(number "127")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "IO0_197_GBIN1")
				(number "128")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "IO0_198_GBIN0")
				(number "129")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 5.08)
				(name "GND__1")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -73.66 180)
				(length 5.08)
				(name "IO0_206")
				(number "130")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 5.08)
				(name "VCCIO_0__1")
				(number "131")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 5.08)
				(name "GND__7")
				(number "132")
			)
			(pin bidirectional line
				(at 25.4 -76.2 180)
				(length 5.08)
				(name "IO0_212")
				(number "134")
			)
			(pin bidirectional line
				(at 25.4 -78.74 180)
				(length 5.08)
				(name "IO0_213")
				(number "135")
			)
			(pin bidirectional line
				(at 25.4 -81.28 180)
				(length 5.08)
				(name "IO0_214")
				(number "136")
			)
			(pin bidirectional line
				(at 25.4 -83.82 180)
				(length 5.08)
				(name "IO0_215")
				(number "137")
			)
			(pin bidirectional line
				(at 25.4 -86.36 180)
				(length 5.08)
				(name "IO0_216")
				(number "138")
			)
			(pin bidirectional line
				(at 25.4 -88.9 180)
				(length 5.08)
				(name "IO0_217")
				(number "139")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 5.08)
				(name "GND__2")
				(number "14")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 5.08)
				(name "GND__8")
				(number "140")
			)
			(pin bidirectional line
				(at 25.4 -91.44 180)
				(length 5.08)
				(name "IO0_219")
				(number "141")
			)
			(pin bidirectional line
				(at 25.4 -93.98 180)
				(length 5.08)
				(name "IO0_220")
				(number "142")
			)
			(pin bidirectional line
				(at 25.4 -96.52 180)
				(length 5.08)
				(name "IO0_221")
				(number "143")
			)
			(pin bidirectional line
				(at 25.4 -99.06 180)
				(length 5.08)
				(name "IO0_222")
				(number "144")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "IO3_10A")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "IO3_10B")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 5.08)
				(name "IO3_12A")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "IO3_12B")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 5.08)
				(name "IO3_13A")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "IO3_2B")
				(number "2")
			)
			(pin input line
				(at -25.4 60.96 0)
				(length 5.08)
				(name "IO3_13B_GBIN7")
				(number "20")
			)
			(pin input line
				(at -25.4 58.42 0)
				(length 5.08)
				(name "IO3_14A_GBIN6")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "IO3_14B")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 5.08)
				(name "IO3_17A")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 5.08)
				(name "IO3_17B")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 5.08)
				(name "IO3_18A")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 5.08)
				(name "IO3_18B")
				(number "26")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 5.08)
				(name "VCC")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 5.08)
				(name "IO3_23A")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 5.08)
				(name "IO3_23B")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "IO3_3A")
				(number "3")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 5.08)
				(name "VCCIO_3__1")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 5.08)
				(name "IO3_24A")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 5.08)
				(name "IO3_24B")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 5.08)
				(name "IO3_25A")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 5.08)
				(name "IO3_25B")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "IO2_56")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "IO2_57")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "IO2_61")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "IO3_3B")
				(number "4")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 5.08)
				(name "VCC__1")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "IO2_63")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "IO2_64")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "IO2_71")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "IO2_72")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "IO2_73")
				(number "45")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 5.08)
				(name "VCCIO_2")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "IO2_79")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "IO2_80")
				(number "48")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 5.08)
				(name "IO2_81_GBIN5")
				(number "49")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 5.08)
				(name "IO2_82_GBIN4")
				(number "52")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 5.08)
				(name "GNDPLL0")
				(number "53")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 5.08)
				(name "VCCPLL0")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IO2_91")
				(number "55")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "IO2_94")
				(number "56")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 5.08)
				(name "VCCIO_2__1")
				(number "57")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 5.08)
				(name "GND__3")
				(number "59")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 5.08)
				(name "VCCIO_3")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "IO2_95")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "IO2_96")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 5.08)
				(name "IO2_102")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 78.74 0)
				(length 5.08)
				(name "IO2_103_CBSEL0")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 76.2 0)
				(length 5.08)
				(name "IO2_104_CBSEL1")
				(number "64")
			)
			(pin input line
				(at -25.4 86.36 0)
				(length 5.08)
				(name "CDONE")
				(number "65")
			)
			(pin input line
				(at -25.4 83.82 0)
				(length 5.08)
				(name "CRESET_B")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 73.66 0)
				(length 5.08)
				(name "IOB_105_SDO")
				(number "67")
			)
			(pin bidirectional line
				(at -25.4 71.12 0)
				(length 5.08)
				(name "IOB_106_SDI")
				(number "68")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 5.08)
				(name "GND__4")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "IO3_4A")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 68.58 0)
				(length 5.08)
				(name "IOB_107_SCK")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 66.04 0)
				(length 5.08)
				(name "IOB_108_SS")
				(number "71")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 5.08)
				(name "VCC_SPI")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 5.08)
				(name "IO1_109")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 5.08)
				(name "IO1_110")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 5.08)
				(name "IO1_111")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "IO1_112")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 5.08)
				(name "IO1_114")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "IO1_115")
				(number "79")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "IO3_4B")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "IO1_116")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "IO1_117")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "IO1_118")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "IO1_119")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "IO1_120")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "IO1_128")
				(number "85")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 5.08)
				(name "GND__5")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "IO1_136")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "IO1_137")
				(number "88")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 5.08)
				(name "VCCIO_1")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "IO3_5A")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "IO1_138")
				(number "90")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "IO1_139")
				(number "91")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 5.08)
				(name "VCC__2")
				(number "92")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "IO1_140_GBIN3")
				(number "93")
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "IO1_141_GBIN2")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "IO1_144")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "IO1_146")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "IO1_147")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IO1_148")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IO1_152")
				(number "99")
			)
		)
	)
	(symbol "LF347"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "LF347"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "LF347_1_1"
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
		)
		(symbol "LF347_2_1"
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "5")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "6")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LF347_3_1"
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "10")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "9")
			)
		)
		(symbol "LF347_4_1"
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "12")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "13")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
		(symbol "LF347_5_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "11")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
		)
	)
	(symbol "LM833"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "LM833"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "LM833_1_1"
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
		)
		(symbol "LM833_2_1"
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LM833_3_1"
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "Vcc")
				(number "8")
			)
		)
	)
	(symbol "MC68040RC33"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 86.36 0)
		)
		(property "Value" "MC68040"
			(at 0 83.82 0)
		)
		(property "Footprint" "AmigaPCI:PGA179"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 13.97 44.45 0)
		)
		(property "Description" "Motorola MC68040RC33 PGA"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "MC68040RC33_1_0"
			(pin bidirectional line
				(at -13.97 1.27 0)
				(length 5.08)
				(name "A31")
				(number "1")
			)
			(pin bidirectional line
				(at 13.97 49.53 180)
				(length 5.08)
				(name "D12")
				(number "10")
			)
			(pin bidirectional line
				(at -13.97 80.01 0)
				(length 5.08)
				(name "A0")
				(number "102")
			)
			(pin bidirectional line
				(at -13.97 46.99 0)
				(length 5.08)
				(name "A13")
				(number "103")
			)
			(pin output line
				(at -13.97 -11.43 0)
				(length 5.08)
				(name "TM1")
				(number "108")
			)
			(pin bidirectional line
				(at -13.97 49.53 0)
				(length 5.08)
				(name "A12")
				(number "109")
			)
			(pin bidirectional line
				(at 13.97 46.99 180)
				(length 5.08)
				(name "D13")
				(number "11")
			)
			(pin bidirectional line
				(at -13.97 52.07 0)
				(length 5.08)
				(name "A11")
				(number "111")
			)
			(pin bidirectional line
				(at -13.97 -26.67 0)
				(length 5.08)
				(name "R_W")
				(number "112")
			)
			(pin output line
				(at -13.97 -8.89 0)
				(length 5.08)
				(name "TM0")
				(number "114")
			)
			(pin bidirectional line
				(at -13.97 54.61 0)
				(length 5.08)
				(name "A10")
				(number "115")
			)
			(pin bidirectional line
				(at -13.97 -6.35 0)
				(length 5.08)
				(name "TT1")
				(number "116")
			)
			(pin bidirectional line
				(at -13.97 -3.81 0)
				(length 5.08)
				(name "TT0")
				(number "117")
			)
			(pin bidirectional line
				(at -13.97 -31.75 0)
				(length 5.08)
				(name "SIZ1")
				(number "118")
			)
			(pin bidirectional line
				(at -13.97 -29.21 0)
				(length 5.08)
				(name "SIZ0")
				(number "119")
			)
			(pin bidirectional line
				(at 13.97 44.45 180)
				(length 5.08)
				(name "D14")
				(number "12")
			)
			(pin output line
				(at -13.97 -19.05 0)
				(length 5.08)
				(name "TLN1")
				(number "120")
			)
			(pin output line
				(at -13.97 -24.13 0)
				(length 5.08)
				(name "UPA1")
				(number "121")
			)
			(pin output line
				(at -13.97 -21.59 0)
				(length 5.08)
				(name "UPA0")
				(number "123")
			)
			(pin output line
				(at 13.97 -8.89 180)
				(length 5.08)
				(name "_MI")
				(number "124")
			)
			(pin output line
				(at -13.97 -16.51 0)
				(length 5.08)
				(name "TLN0")
				(number "126")
			)
			(pin output line
				(at -13.97 -39.37 0)
				(length 5.08)
				(name "_CIOUT")
				(number "127")
			)
			(pin output line
				(at 13.97 -31.75 180)
				(length 5.08)
				(name "_RSTO")
				(number "129")
			)
			(pin bidirectional line
				(at 13.97 41.91 180)
				(length 5.08)
				(name "D15")
				(number "13")
			)
			(pin input line
				(at 13.97 -62.23 180)
				(length 5.08)
				(name "BCLK")
				(number "133")
			)
			(pin input line
				(at 13.97 -64.77 180)
				(length 5.08)
				(name "PCLK")
				(number "135")
			)
			(pin bidirectional line
				(at 13.97 36.83 180)
				(length 5.08)
				(name "D17")
				(number "14")
			)
			(pin output line
				(at 13.97 -57.15 180)
				(length 5.08)
				(name "PST2")
				(number "140")
			)
			(pin output line
				(at -13.97 -46.99 0)
				(length 5.08)
				(name "_TIP")
				(number "141")
			)
			(pin bidirectional line
				(at -13.97 -44.45 0)
				(length 5.08)
				(name "_TS")
				(number "142")
			)
			(pin output line
				(at -13.97 -36.83 0)
				(length 5.08)
				(name "_LOCKE")
				(number "144")
			)
			(pin output line
				(at 13.97 -44.45 180)
				(length 5.08)
				(name "_IPEND")
				(number "145")
			)
			(pin input line
				(at 13.97 -74.93 180)
				(length 5.08)
				(name "TDI")
				(number "147")
			)
			(pin input line
				(at 13.97 -69.85 180)
				(length 5.08)
				(name "TCK")
				(number "148")
			)
			(pin input line
				(at 13.97 -72.39 180)
				(length 5.08)
				(name "TMS")
				(number "149")
			)
			(pin bidirectional line
				(at 13.97 31.75 180)
				(length 5.08)
				(name "D19")
				(number "15")
			)
			(pin input line
				(at 13.97 -26.67 180)
				(length 5.08)
				(name "_MDIS")
				(number "150")
			)
			(pin input line
				(at 13.97 -29.21 180)
				(length 5.08)
				(name "_RSTI")
				(number "151")
			)
			(pin input line
				(at -13.97 -59.69 0)
				(length 5.08)
				(name "_TBI")
				(number "155")
			)
			(pin bidirectional line
				(at 13.97 -6.35 180)
				(length 5.08)
				(name "SC1")
				(number "156")
			)
			(pin input line
				(at -13.97 -54.61 0)
				(length 5.08)
				(name "_TEA")
				(number "157")
			)
			(pin output line
				(at 13.97 -54.61 180)
				(length 5.08)
				(name "PST1")
				(number "158")
			)
			(pin bidirectional line
				(at 13.97 29.21 180)
				(length 5.08)
				(name "D20")
				(number "16")
			)
			(pin output line
				(at -13.97 -34.29 0)
				(length 5.08)
				(name "_LOCK")
				(number "162")
			)
			(pin output line
				(at 13.97 -77.47 180)
				(length 5.08)
				(name "TDO")
				(number "163")
			)
			(pin input line
				(at 13.97 -80.01 180)
				(length 5.08)
				(name "_TRST")
				(number "164")
			)
			(pin input line
				(at 13.97 -24.13 180)
				(length 5.08)
				(name "_CDIS")
				(number "166")
			)
			(pin input line
				(at 13.97 -41.91 180)
				(length 5.08)
				(name "_IPL2")
				(number "167")
			)
			(pin input line
				(at 13.97 -39.37 180)
				(length 5.08)
				(name "_IPL1")
				(number "168")
			)
			(pin input line
				(at 13.97 -36.83 180)
				(length 5.08)
				(name "_IPL0")
				(number "169")
			)
			(pin bidirectional line
				(at 13.97 26.67 180)
				(length 5.08)
				(name "D21")
				(number "17")
			)
			(pin input line
				(at -13.97 -62.23 0)
				(length 5.08)
				(name "DLE")
				(number "170")
			)
			(pin input line
				(at -13.97 -57.15 0)
				(length 5.08)
				(name "_TCI")
				(number "171")
			)
			(pin input line
				(at 13.97 -46.99 180)
				(length 5.08)
				(name "_AVEC")
				(number "172")
			)
			(pin bidirectional line
				(at 13.97 -3.81 180)
				(length 5.08)
				(name "SC0")
				(number "173")
			)
			(pin output line
				(at 13.97 -16.51 180)
				(length 5.08)
				(name "_BG")
				(number "174")
			)
			(pin bidirectional line
				(at -13.97 -52.07 0)
				(length 5.08)
				(name "_TA")
				(number "175")
			)
			(pin output line
				(at 13.97 -52.07 180)
				(length 5.08)
				(name "PST0")
				(number "176")
			)
			(pin output line
				(at 13.97 -59.69 180)
				(length 5.08)
				(name "PST3")
				(number "177")
			)
			(pin bidirectional line
				(at 13.97 -19.05 180)
				(length 5.08)
				(name "_BB")
				(number "178")
			)
			(pin input line
				(at 13.97 -13.97 180)
				(length 5.08)
				(name "_BR")
				(number "179")
			)
			(pin bidirectional line
				(at 13.97 19.05 180)
				(length 5.08)
				(name "D24")
				(number "18")
			)
			(pin bidirectional line
				(at -13.97 6.35 0)
				(length 5.08)
				(name "A29")
				(number "19")
			)
			(pin bidirectional line
				(at 13.97 72.39 180)
				(length 5.08)
				(name "D3")
				(number "2")
			)
			(pin bidirectional line
				(at 13.97 77.47 180)
				(length 5.08)
				(name "D1")
				(number "21")
			)
			(pin bidirectional line
				(at 13.97 59.69 180)
				(length 5.08)
				(name "D8")
				(number "25")
			)
			(pin bidirectional line
				(at 13.97 39.37 180)
				(length 5.08)
				(name "D16")
				(number "29")
			)
			(pin bidirectional line
				(at 13.97 69.85 180)
				(length 5.08)
				(name "D4")
				(number "3")
			)
			(pin bidirectional line
				(at 13.97 34.29 180)
				(length 5.08)
				(name "D18")
				(number "30")
			)
			(pin bidirectional line
				(at 13.97 24.13 180)
				(length 5.08)
				(name "D22")
				(number "34")
			)
			(pin bidirectional line
				(at 13.97 13.97 180)
				(length 5.08)
				(name "D26")
				(number "36")
			)
			(pin bidirectional line
				(at -13.97 11.43 0)
				(length 5.08)
				(name "A27")
				(number "37")
			)
			(pin bidirectional line
				(at 13.97 80.01 180)
				(length 5.08)
				(name "D0")
				(number "39")
			)
			(pin bidirectional line
				(at 13.97 67.31 180)
				(length 5.08)
				(name "D5")
				(number "4")
			)
			(pin bidirectional line
				(at 13.97 74.93 180)
				(length 5.08)
				(name "D2")
				(number "40")
			)
			(pin bidirectional line
				(at 13.97 64.77 180)
				(length 5.08)
				(name "D6")
				(number "5")
			)
			(pin bidirectional line
				(at 13.97 21.59 180)
				(length 5.08)
				(name "D23")
				(number "51")
			)
			(pin bidirectional line
				(at 13.97 16.51 180)
				(length 5.08)
				(name "D25")
				(number "52")
			)
			(pin bidirectional line
				(at 13.97 8.89 180)
				(length 5.08)
				(name "D28")
				(number "54")
			)
			(pin bidirectional line
				(at -13.97 19.05 0)
				(length 5.08)
				(name "A24")
				(number "55")
			)
			(pin bidirectional line
				(at -13.97 3.81 0)
				(length 5.08)
				(name "A30")
				(number "57")
			)
			(pin bidirectional line
				(at 13.97 11.43 180)
				(length 5.08)
				(name "D27")
				(number "58")
			)
			(pin bidirectional line
				(at 13.97 62.23 180)
				(length 5.08)
				(name "D7")
				(number "6")
			)
			(pin bidirectional line
				(at 13.97 1.27 180)
				(length 5.08)
				(name "D31")
				(number "60")
			)
			(pin bidirectional line
				(at -13.97 24.13 0)
				(length 5.08)
				(name "A22")
				(number "61")
			)
			(pin bidirectional line
				(at -13.97 13.97 0)
				(length 5.08)
				(name "A26")
				(number "62")
			)
			(pin bidirectional line
				(at -13.97 8.89 0)
				(length 5.08)
				(name "A28")
				(number "63")
			)
			(pin bidirectional line
				(at 13.97 6.35 180)
				(length 5.08)
				(name "D29")
				(number "64")
			)
			(pin bidirectional line
				(at 13.97 3.81 180)
				(length 5.08)
				(name "D30")
				(number "65")
			)
			(pin bidirectional line
				(at -13.97 59.69 0)
				(length 5.08)
				(name "A8")
				(number "66")
			)
			(pin bidirectional line
				(at -13.97 26.67 0)
				(length 5.08)
				(name "A21")
				(number "67")
			)
			(pin bidirectional line
				(at -13.97 16.51 0)
				(length 5.08)
				(name "A25")
				(number "69")
			)
			(pin bidirectional line
				(at 13.97 57.15 180)
				(length 5.08)
				(name "D9")
				(number "7")
			)
			(pin bidirectional line
				(at -13.97 57.15 0)
				(length 5.08)
				(name "A9")
				(number "70")
			)
			(pin bidirectional line
				(at -13.97 62.23 0)
				(length 5.08)
				(name "A7")
				(number "72")
			)
			(pin bidirectional line
				(at -13.97 29.21 0)
				(length 5.08)
				(name "A20")
				(number "73")
			)
			(pin bidirectional line
				(at -13.97 21.59 0)
				(length 5.08)
				(name "A23")
				(number "75")
			)
			(pin bidirectional line
				(at -13.97 64.77 0)
				(length 5.08)
				(name "A6")
				(number "76")
			)
			(pin bidirectional line
				(at -13.97 67.31 0)
				(length 5.08)
				(name "A5")
				(number "78")
			)
			(pin bidirectional line
				(at -13.97 34.29 0)
				(length 5.08)
				(name "A18")
				(number "79")
			)
			(pin bidirectional line
				(at 13.97 54.61 180)
				(length 5.08)
				(name "D10")
				(number "8")
			)
			(pin bidirectional line
				(at -13.97 69.85 0)
				(length 5.08)
				(name "A4")
				(number "84")
			)
			(pin bidirectional line
				(at -13.97 36.83 0)
				(length 5.08)
				(name "A17")
				(number "85")
			)
			(pin bidirectional line
				(at -13.97 31.75 0)
				(length 5.08)
				(name "A19")
				(number "86")
			)
			(pin bidirectional line
				(at -13.97 74.93 0)
				(length 5.08)
				(name "A2")
				(number "89")
			)
			(pin bidirectional line
				(at 13.97 52.07 180)
				(length 5.08)
				(name "D11")
				(number "9")
			)
			(pin bidirectional line
				(at -13.97 72.39 0)
				(length 5.08)
				(name "A3")
				(number "90")
			)
			(pin bidirectional line
				(at -13.97 41.91 0)
				(length 5.08)
				(name "A15")
				(number "91")
			)
			(pin bidirectional line
				(at -13.97 39.37 0)
				(length 5.08)
				(name "A16")
				(number "92")
			)
			(pin input line
				(at -13.97 -13.97 0)
				(length 5.08)
				(name "TM2")
				(number "95")
			)
			(pin bidirectional line
				(at -13.97 77.47 0)
				(length 5.08)
				(name "A1")
				(number "96")
			)
			(pin bidirectional line
				(at -13.97 44.45 0)
				(length 5.08)
				(name "A14")
				(number "97")
			)
		)
		(symbol "MC68040RC33_1_1")
		(symbol "MC68040RC33_2_0"
			(pin power_in line
				(at -13.97 7.62 0)
				(length 5.08)
				(name "Vcc")
				(number "100")
			)
			(pin power_in line
				(at 13.97 -10.16 180)
				(length 5.08)
				(name "GND")
				(number "101")
			)
			(pin power_in line
				(at -13.97 2.54 0)
				(length 5.08)
				(name "Vcc")
				(number "104")
			)
			(pin power_in line
				(at -13.97 5.08 0)
				(length 5.08)
				(name "Vcc")
				(number "105")
			)
			(pin power_in line
				(at 13.97 -12.7 180)
				(length 5.08)
				(name "GND")
				(number "106")
			)
			(pin power_in line
				(at -13.97 0 0)
				(length 5.08)
				(name "Vcc")
				(number "107")
			)
			(pin power_in line
				(at 13.97 -15.24 180)
				(length 5.08)
				(name "GND")
				(number "110")
			)
			(pin power_in line
				(at 13.97 -17.78 180)
				(length 5.08)
				(name "GND")
				(number "113")
			)
			(pin power_in line
				(at 13.97 -20.32 180)
				(length 5.08)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 13.97 -22.86 180)
				(length 5.08)
				(name "GND")
				(number "125")
			)
			(pin power_in line
				(at -13.97 -2.54 0)
				(length 5.08)
				(name "Vcc")
				(number "128")
			)
			(pin power_in line
				(at 13.97 -25.4 180)
				(length 5.08)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at -13.97 -5.08 0)
				(length 5.08)
				(name "Vcc")
				(number "131")
			)
			(pin power_in line
				(at 13.97 -27.94 180)
				(length 5.08)
				(name "GND")
				(number "132")
			)
			(pin power_in line
				(at -13.97 -7.62 0)
				(length 5.08)
				(name "Vcc")
				(number "134")
			)
			(pin power_in line
				(at 13.97 -30.48 180)
				(length 5.08)
				(name "GND")
				(number "136")
			)
			(pin power_in line
				(at 13.97 -33.02 180)
				(length 5.08)
				(name "GND")
				(number "137")
			)
			(pin power_in line
				(at -13.97 -10.16 0)
				(length 5.08)
				(name "Vcc")
				(number "138")
			)
			(pin power_in line
				(at 13.97 -35.56 180)
				(length 5.08)
				(name "GND")
				(number "139")
			)
			(pin power_in line
				(at -13.97 -12.7 0)
				(length 5.08)
				(name "Vcc")
				(number "143")
			)
			(pin power_in line
				(at 13.97 -38.1 180)
				(length 5.08)
				(name "GND")
				(number "146")
			)
			(pin power_in line
				(at -13.97 -15.24 0)
				(length 5.08)
				(name "Vcc")
				(number "152")
			)
			(pin power_in line
				(at 13.97 -40.64 180)
				(length 5.08)
				(name "GND")
				(number "153")
			)
			(pin power_in line
				(at 13.97 -43.18 180)
				(length 5.08)
				(name "GND")
				(number "154")
			)
			(pin power_in line
				(at 13.97 -45.72 180)
				(length 5.08)
				(name "GND")
				(number "159")
			)
			(pin power_in line
				(at -13.97 -17.78 0)
				(length 5.08)
				(name "Vcc")
				(number "160")
			)
			(pin power_in line
				(at 13.97 -48.26 180)
				(length 5.08)
				(name "GND")
				(number "161")
			)
			(pin power_in line
				(at 13.97 -50.8 180)
				(length 5.08)
				(name "GND")
				(number "165")
			)
			(pin power_in line
				(at 13.97 48.26 180)
				(length 5.08)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 13.97 45.72 180)
				(length 5.08)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at -13.97 48.26 0)
				(length 5.08)
				(name "Vcc")
				(number "23")
			)
			(pin power_in line
				(at 13.97 43.18 180)
				(length 5.08)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at 13.97 40.64 180)
				(length 5.08)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at -13.97 45.72 0)
				(length 5.08)
				(name "Vcc")
				(number "27")
			)
			(pin power_in line
				(at 13.97 38.1 180)
				(length 5.08)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 13.97 35.56 180)
				(length 5.08)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -13.97 43.18 0)
				(length 5.08)
				(name "Vcc")
				(number "32")
			)
			(pin power_in line
				(at 13.97 33.02 180)
				(length 5.08)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 13.97 30.48 180)
				(length 5.08)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at -13.97 40.64 0)
				(length 5.08)
				(name "Vcc")
				(number "38")
			)
			(pin power_in line
				(at -13.97 38.1 0)
				(length 5.08)
				(name "Vcc")
				(number "41")
			)
			(pin power_in line
				(at 13.97 27.94 180)
				(length 5.08)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 13.97 25.4 180)
				(length 5.08)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at -13.97 35.56 0)
				(length 5.08)
				(name "Vcc")
				(number "44")
			)
			(pin power_in line
				(at 13.97 22.86 180)
				(length 5.08)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at -13.97 33.02 0)
				(length 5.08)
				(name "Vcc")
				(number "46")
			)
			(pin power_in line
				(at 13.97 20.32 180)
				(length 5.08)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at -13.97 30.48 0)
				(length 5.08)
				(name "Vcc")
				(number "48")
			)
			(pin power_in line
				(at 13.97 17.78 180)
				(length 5.08)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at -13.97 27.94 0)
				(length 5.08)
				(name "Vcc")
				(number "50")
			)
			(pin power_in line
				(at -13.97 25.4 0)
				(length 5.08)
				(name "Vcc")
				(number "53")
			)
			(pin power_in line
				(at 13.97 15.24 180)
				(length 5.08)
				(name "GND")
				(number "56")
			)
			(pin power_in line
				(at 13.97 12.7 180)
				(length 5.08)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 13.97 10.16 180)
				(length 5.08)
				(name "GND")
				(number "68")
			)
			(pin power_in line
				(at 13.97 7.62 180)
				(length 5.08)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at -13.97 22.86 0)
				(length 5.08)
				(name "Vcc")
				(number "74")
			)
			(pin power_in line
				(at -13.97 20.32 0)
				(length 5.08)
				(name "Vcc")
				(number "77")
			)
			(pin power_in line
				(at 13.97 5.08 180)
				(length 5.08)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at -13.97 17.78 0)
				(length 5.08)
				(name "Vcc")
				(number "81")
			)
			(pin power_in line
				(at -13.97 15.24 0)
				(length 5.08)
				(name "Vcc")
				(number "82")
			)
			(pin power_in line
				(at 13.97 2.54 180)
				(length 5.08)
				(name "GND")
				(number "83")
			)
			(pin power_in line
				(at -13.97 12.7 0)
				(length 5.08)
				(name "Vcc")
				(number "87")
			)
			(pin power_in line
				(at -13.97 10.16 0)
				(length 5.08)
				(name "Vcc")
				(number "88")
			)
			(pin power_in line
				(at 13.97 0 180)
				(length 5.08)
				(name "GND")
				(number "93")
			)
			(pin power_in line
				(at 13.97 -2.54 180)
				(length 5.08)
				(name "GND")
				(number "94")
			)
			(pin power_in line
				(at 13.97 -5.08 180)
				(length 5.08)
				(name "GND")
				(number "98")
			)
			(pin power_in line
				(at 13.97 -7.62 180)
				(length 5.08)
				(name "GND")
				(number "99")
			)
		)
		(symbol "MC68040RC33_2_1")
	)
	(symbol "MOS 8362 Denise"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.127 21.844 0)
		)
		(property "Value" "DENISE"
			(at 5.08 -10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-48_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "MOS 8362 Denise_1_1"
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "DRD6")
				(number "1")
			)
			(pin input line
				(at -12.7 -43.18 0)
				(length 5.08)
				(name "RGA8")
				(number "10")
			)
			(pin input line
				(at -12.7 -45.72 0)
				(length 5.08)
				(name "RGA7")
				(number "11")
			)
			(pin input line
				(at -12.7 -48.26 0)
				(length 5.08)
				(name "RGA6")
				(number "12")
			)
			(pin input line
				(at -12.7 -50.8 0)
				(length 5.08)
				(name "RGA5")
				(number "13")
			)
			(pin input line
				(at -12.7 -53.34 0)
				(length 5.08)
				(name "RGA4")
				(number "14")
			)
			(pin input line
				(at -12.7 -55.88 0)
				(length 5.08)
				(name "RGA3")
				(number "15")
			)
			(pin input line
				(at -12.7 -58.42 0)
				(length 5.08)
				(name "RGA2")
				(number "16")
			)
			(pin input line
				(at -12.7 -60.96 0)
				(length 5.08)
				(name "RGA1")
				(number "17")
			)
			(pin output inverted
				(at 13.97 -20.32 180)
				(length 5.08)
				(name "BURST")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 5.08)
				(name "DRD5")
				(number "2")
			)
			(pin output line
				(at 13.97 -43.18 180)
				(length 5.08)
				(name "R0")
				(number "20")
			)
			(pin output line
				(at 13.97 -40.64 180)
				(length 5.08)
				(name "R1")
				(number "21")
			)
			(pin output line
				(at 13.97 -38.1 180)
				(length 5.08)
				(name "R2")
				(number "22")
			)
			(pin output line
				(at 13.97 -35.56 180)
				(length 5.08)
				(name "R3")
				(number "23")
			)
			(pin output line
				(at 13.97 -83.82 180)
				(length 5.08)
				(name "B0")
				(number "24")
			)
			(pin output line
				(at 13.97 -81.28 180)
				(length 5.08)
				(name "B1")
				(number "25")
			)
			(pin output line
				(at 13.97 -78.74 180)
				(length 5.08)
				(name "B2")
				(number "26")
			)
			(pin output line
				(at 13.97 -76.2 180)
				(length 5.08)
				(name "B3")
				(number "27")
			)
			(pin output line
				(at 13.97 -63.5 180)
				(length 5.08)
				(name "G0")
				(number "28")
			)
			(pin output line
				(at 13.97 -60.96 180)
				(length 5.08)
				(name "G1")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "DRD4")
				(number "3")
			)
			(pin output line
				(at 13.97 -58.42 180)
				(length 5.08)
				(name "G2")
				(number "30")
			)
			(pin output line
				(at 13.97 -55.88 180)
				(length 5.08)
				(name "G3")
				(number "31")
			)
			(pin input inverted
				(at -12.7 17.78 0)
				(length 5.08)
				(name "/CSYNC")
				(number "32")
			)
			(pin output inverted
				(at 13.97 -25.4 180)
				(length 5.08)
				(name "PIXELSW")
				(number "33")
			)
			(pin input inverted
				(at -12.7 12.7 0)
				(length 5.08)
				(name "/CDAC")
				(number "34")
			)
			(pin input line
				(at -12.7 -81.28 0)
				(length 5.08)
				(name "7M")
				(number "35")
			)
			(pin input line
				(at -12.7 -72.39 0)
				(length 5.08)
				(name "CCK")
				(number "36")
			)
			(pin input line
				(at 13.97 7.62 180)
				(length 5.08)
				(name "M0V")
				(number "38")
			)
			(pin input line
				(at 13.97 17.78 180)
				(length 5.08)
				(name "M1V")
				(number "39")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 5.08)
				(name "DRD3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "DRD15")
				(number "40")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "DRD14")
				(number "41")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "DRD13")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "DRD12")
				(number "43")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "DRD11")
				(number "44")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "DRD10")
				(number "45")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "DRD9")
				(number "46")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "DRD8")
				(number "47")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "DRD7")
				(number "48")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 5.08)
				(name "DRD2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 5.08)
				(name "DRD1")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 5.08)
				(name "DRD0")
				(number "7")
			)
			(pin input line
				(at 13.97 12.7 180)
				(length 5.08)
				(name "M1H")
				(number "8")
			)
			(pin input line
				(at 13.97 2.54 180)
				(length 5.08)
				(name "M0H")
				(number "9")
			)
		)
		(symbol "MOS 8362 Denise_2_1"
			(pin power_in line
				(at 0 8.89 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND1")
				(number "37")
			)
		)
	)
	(symbol "MOS 8364 Paula"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.635 -69.1642 0)
		)
		(property "Value" "PAULA"
			(at -0.635 -71.4756 0)
		)
		(property "Footprint" "Package_DIP:DIP-48_W15.24mm"
			(at 3.81 0 0)
		)
		(property "Datasheet" ""
			(at 3.81 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MOS 8364 Paula_0_1")
		(symbol "MOS 8364 Paula_1_1"
			(pin passive line
				(at -16.51 33.02 0)
				(length 5.08)
				(name "DRD8")
				(number "1")
			)
			(pin passive line
				(at -16.51 12.7 0)
				(length 5.08)
				(name "DRD0")
				(number "10")
			)
			(pin passive line
				(at -16.51 -64.77 0)
				(length 5.08)
				(name "_RESET")
				(number "11")
			)
			(pin passive line
				(at -16.51 -45.72 0)
				(length 5.08)
				(name "DMAL")
				(number "12")
			)
			(pin passive inverted
				(at -16.51 -33.02 0)
				(length 5.08)
				(name "_IPL0")
				(number "13")
			)
			(pin passive inverted
				(at -16.51 -30.48 0)
				(length 5.08)
				(name "_IPL1")
				(number "14")
			)
			(pin passive inverted
				(at -16.51 -27.94 0)
				(length 5.08)
				(name "_IPL2")
				(number "15")
			)
			(pin passive inverted
				(at 15.24 5.08 180)
				(length 5.08)
				(name "_INT2")
				(number "16")
			)
			(pin passive inverted
				(at 15.24 10.16 180)
				(length 5.08)
				(name "_INT3")
				(number "17")
			)
			(pin passive inverted
				(at 15.24 15.24 180)
				(length 5.08)
				(name "_INT6")
				(number "18")
			)
			(pin passive line
				(at -16.51 0 0)
				(length 5.08)
				(name "RGA8")
				(number "19")
			)
			(pin passive line
				(at -16.51 30.48 0)
				(length 5.08)
				(name "DRD7")
				(number "2")
			)
			(pin passive line
				(at -16.51 -2.54 0)
				(length 5.08)
				(name "RGA7")
				(number "20")
			)
			(pin passive line
				(at -16.51 -5.08 0)
				(length 5.08)
				(name "RGA6")
				(number "21")
			)
			(pin passive line
				(at -16.51 -7.62 0)
				(length 5.08)
				(name "RGA5")
				(number "22")
			)
			(pin passive line
				(at -16.51 -10.16 0)
				(length 5.08)
				(name "RGA4")
				(number "23")
			)
			(pin passive line
				(at -16.51 -12.7 0)
				(length 5.08)
				(name "RGA3")
				(number "24")
			)
			(pin passive line
				(at -16.51 -15.24 0)
				(length 5.08)
				(name "RGA2")
				(number "25")
			)
			(pin passive line
				(at -16.51 -17.78 0)
				(length 5.08)
				(name "RGA1")
				(number "26")
			)
			(pin passive line
				(at -6.35 63.5 270)
				(length 5.08)
				(name "VCC")
				(number "27")
			)
			(pin passive line
				(at -16.51 -53.34 0)
				(length 5.08)
				(name "CCK")
				(number "28")
			)
			(pin passive line
				(at -16.51 -58.42 0)
				(length 5.08)
				(name "CCKQ")
				(number "29")
			)
			(pin passive line
				(at -16.51 27.94 0)
				(length 5.08)
				(name "DRD6")
				(number "3")
			)
			(pin passive line
				(at 15.24 -22.86 180)
				(length 5.08)
				(name "RIGHT")
				(number "30")
			)
			(pin passive line
				(at 15.24 -11.43 180)
				(length 5.08)
				(name "LEFT")
				(number "31")
			)
			(pin passive line
				(at 15.24 -35.56 180)
				(length 5.08)
				(name "P0X")
				(number "32")
			)
			(pin passive line
				(at 15.24 -40.64 180)
				(length 5.08)
				(name "P0Y")
				(number "33")
			)
			(pin passive line
				(at 15.24 -64.77 180)
				(length 5.08)
				(name "A_GND")
				(number "34")
			)
			(pin passive line
				(at 15.24 -45.72 180)
				(length 5.08)
				(name "P1X")
				(number "35")
			)
			(pin passive line
				(at 15.24 -50.8 180)
				(length 5.08)
				(name "P1Y")
				(number "36")
			)
			(pin passive inverted
				(at 15.24 50.8 180)
				(length 5.08)
				(name "_DKRD")
				(number "37")
			)
			(pin passive inverted
				(at 15.24 45.72 180)
				(length 5.08)
				(name "_DKWD")
				(number "38")
			)
			(pin passive line
				(at 15.24 40.64 180)
				(length 5.08)
				(name "DKWE")
				(number "39")
			)
			(pin passive line
				(at -16.51 25.4 0)
				(length 5.08)
				(name "DRD5")
				(number "4")
			)
			(pin passive inverted
				(at 15.24 25.4 180)
				(length 5.08)
				(name "_TXD")
				(number "40")
			)
			(pin passive inverted
				(at 15.24 30.48 180)
				(length 5.08)
				(name "_RxD")
				(number "41")
			)
			(pin passive line
				(at -16.51 50.8 0)
				(length 5.08)
				(name "DRD15")
				(number "42")
			)
			(pin passive line
				(at -16.51 48.26 0)
				(length 5.08)
				(name "DRD14")
				(number "43")
			)
			(pin passive line
				(at -16.51 45.72 0)
				(length 5.08)
				(name "DRD13")
				(number "44")
			)
			(pin passive line
				(at -16.51 43.18 0)
				(length 5.08)
				(name "DRD12")
				(number "45")
			)
			(pin passive line
				(at -16.51 40.64 0)
				(length 5.08)
				(name "DRD11")
				(number "46")
			)
			(pin passive line
				(at -16.51 38.1 0)
				(length 5.08)
				(name "DRD10")
				(number "47")
			)
			(pin passive line
				(at -16.51 35.56 0)
				(length 5.08)
				(name "DRD9")
				(number "48")
			)
			(pin passive line
				(at -16.51 22.86 0)
				(length 5.08)
				(name "DRD4")
				(number "5")
			)
			(pin passive line
				(at -16.51 20.32 0)
				(length 5.08)
				(name "DRD3")
				(number "6")
			)
			(pin passive line
				(at -16.51 17.78 0)
				(length 5.08)
				(name "DRD2")
				(number "7")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -16.51 15.24 0)
				(length 5.08)
				(name "DRD1")
				(number "9")
			)
		)
	)
	(symbol "MOS 8520"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 53.34 0)
		)
		(property "Value" "8520"
			(at 0 40.64 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm_Socket"
			(at 0 34.29 0)
		)
		(property "Datasheet" ""
			(at 0 34.29 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "MOS 8520_1_1"
			(pin bidirectional line
				(at 10.16 -63.5 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -58.42 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -53.34 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -48.26 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -43.18 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -38.1 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -33.02 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -27.94 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin output line
				(at 10.16 30.48 180)
				(length 2.54)
				(name "_PC")
				(number "18")
			)
			(pin input line
				(at -11.43 -43.18 0)
				(length 2.54)
				(name "TICK")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin output line
				(at -11.43 -33.02 0)
				(length 2.54)
				(name "_INT")
				(number "21")
			)
			(pin input line
				(at -11.43 -17.78 0)
				(length 2.54)
				(name "_W")
				(number "22")
			)
			(pin input line
				(at -11.43 -12.7 0)
				(length 2.54)
				(name "_CS")
				(number "23")
			)
			(pin input line
				(at 10.16 35.56 180)
				(length 2.54)
				(name "_F")
				(number "24")
			)
			(pin input line
				(at -11.43 -22.86 0)
				(length 2.54)
				(name "E")
				(number "25")
			)
			(pin bidirectional line
				(at -11.43 38.1 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin bidirectional line
				(at -11.43 35.56 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -11.43 33.02 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -11.43 30.48 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at -11.43 27.94 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -11.43 25.4 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -11.43 22.86 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -11.43 20.32 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin input line
				(at -11.43 -53.34 0)
				(length 2.54)
				(name "_RESET")
				(number "34")
			)
			(pin input line
				(at -11.43 10.16 0)
				(length 2.54)
				(name "RS3")
				(number "35")
			)
			(pin input line
				(at -11.43 7.62 0)
				(length 2.54)
				(name "RS2")
				(number "36")
			)
			(pin input line
				(at -11.43 5.08 0)
				(length 2.54)
				(name "RS1")
				(number "37")
			)
			(pin input line
				(at -11.43 2.54 0)
				(length 2.54)
				(name "RS0")
				(number "38")
			)
			(pin input line
				(at 10.16 45.72 180)
				(length 2.54)
				(name "S")
				(number "39")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin input line
				(at 10.16 50.8 180)
				(length 2.54)
				(name "C")
				(number "40")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA3")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "9")
			)
		)
		(symbol "MOS 8520_2_1"
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin power_in line
				(at 0 8.89 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
		)
	)
	(symbol "PCI32-3V3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 0 119.38 0)
		)
		(property "Value" "PCI32-3V3"
			(at 0 -124.206 0)
		)
		(property "Footprint" "A2900:PCI-3V3"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PCI32-3V3_0_0"
			(pin input line
				(at 11.43 114.3 180)
				(length 3.81)
				(name "_TRST")
				(number "A1")
			)
			(pin power_in line
				(at 11.43 80.01 180)
				(length 3.81)
				(name "+5Vio")
				(number "A10")
			)
			(pin no_connect line
				(at 11.43 76.2 180)
				(length 3.81)
				(name "NC")
				(number "A11")
			)
			(pin no_connect line
				(at 11.43 64.77 180)
				(length 3.81)
				(name "+3V3aux")
				(number "A14")
			)
			(pin input line
				(at 11.43 60.96 180)
				(length 3.81)
				(name "_RESET")
				(number "A15")
			)
			(pin power_in line
				(at 11.43 57.15 180)
				(length 3.81)
				(name "+5Vio")
				(number "A16")
			)
			(pin input line
				(at 11.43 53.34 180)
				(length 3.81)
				(name "_GNT")
				(number "A17")
			)
			(pin power_in line
				(at 11.43 49.53 180)
				(length 3.81)
				(name "GND")
				(number "A18")
			)
			(pin no_connect line
				(at 11.43 45.72 180)
				(length 3.81)
				(name "_PME")
				(number "A19")
			)
			(pin power_in line
				(at 11.43 110.49 180)
				(length 3.81)
				(name "+12V")
				(number "A2")
			)
			(pin bidirectional line
				(at 11.43 41.91 180)
				(length 3.81)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at 11.43 38.1 180)
				(length 3.81)
				(name "+3V3")
				(number "A21")
			)
			(pin bidirectional line
				(at 11.43 34.29 180)
				(length 3.81)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 11.43 30.48 180)
				(length 3.81)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at 11.43 26.67 180)
				(length 3.81)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 11.43 22.86 180)
				(length 3.81)
				(name "AD[24]")
				(number "A25")
			)
			(pin input line
				(at 11.43 19.05 180)
				(length 3.81)
				(name "IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at 11.43 15.24 180)
				(length 3.81)
				(name "+3V3")
				(number "A27")
			)
			(pin bidirectional line
				(at 11.43 11.43 180)
				(length 3.81)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 11.43 7.62 180)
				(length 3.81)
				(name "AD[20]")
				(number "A29")
			)
			(pin input line
				(at 11.43 106.68 180)
				(length 3.81)
				(name "TMS")
				(number "A3")
			)
			(pin power_in line
				(at 11.43 3.81 180)
				(length 3.81)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 11.43 0 180)
				(length 3.81)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 11.43 -3.81 180)
				(length 3.81)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at 11.43 -7.62 180)
				(length 3.81)
				(name "+3V3")
				(number "A33")
			)
			(pin bidirectional line
				(at 11.43 -11.43 180)
				(length 3.81)
				(name "_FRAME")
				(number "A34")
			)
			(pin power_in line
				(at 11.43 -15.24 180)
				(length 3.81)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional line
				(at 11.43 -19.05 180)
				(length 3.81)
				(name "_TRDY")
				(number "A36")
			)
			(pin power_in line
				(at 11.43 -22.86 180)
				(length 3.81)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional line
				(at 11.43 -26.67 180)
				(length 3.81)
				(name "_STOP")
				(number "A38")
			)
			(pin power_in line
				(at 11.43 -30.48 180)
				(length 3.81)
				(name "+3V3")
				(number "A39")
			)
			(pin input line
				(at 11.43 102.87 180)
				(length 3.81)
				(name "TDI")
				(number "A4")
			)
			(pin input line
				(at 11.43 -34.29 180)
				(length 3.81)
				(name "SMBCLK")
				(number "A40")
			)
			(pin input line
				(at 11.43 -38.1 180)
				(length 3.81)
				(name "SMBDAT")
				(number "A41")
			)
			(pin power_in line
				(at 11.43 -41.91 180)
				(length 3.81)
				(name "GND")
				(number "A42")
			)
			(pin input line
				(at 11.43 -45.72 180)
				(length 3.81)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 11.43 -49.53 180)
				(length 3.81)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at 11.43 -53.34 180)
				(length 3.81)
				(name "+3V3")
				(number "A45")
			)
			(pin bidirectional line
				(at 11.43 -57.15 180)
				(length 3.81)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 11.43 -60.96 180)
				(length 3.81)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at 11.43 -64.77 180)
				(length 3.81)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 11.43 -68.58 180)
				(length 3.81)
				(name "AD[09]")
				(number "A49")
			)
			(pin power_in line
				(at 11.43 99.06 180)
				(length 3.81)
				(name "+5V")
				(number "A5")
			)
			(pin power_in line
				(at 11.43 -72.39 180)
				(length 3.81)
				(name "GND")
				(number "A50")
			)
			(pin power_in line
				(at 11.43 -76.2 180)
				(length 3.81)
				(name "GND")
				(number "A51")
			)
			(pin input line
				(at 11.43 -80.01 180)
				(length 3.81)
				(name "_CBE[0]")
				(number "A52")
			)
			(pin power_in line
				(at 11.43 -83.82 180)
				(length 3.81)
				(name "+3V3")
				(number "A53")
			)
			(pin bidirectional line
				(at 11.43 -87.63 180)
				(length 3.81)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 11.43 -91.44 180)
				(length 3.81)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at 11.43 -95.25 180)
				(length 3.81)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 11.43 -99.06 180)
				(length 3.81)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 11.43 -102.87 180)
				(length 3.81)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at 11.43 -106.68 180)
				(length 3.81)
				(name "+5Vio")
				(number "A59")
			)
			(pin output line
				(at 11.43 95.25 180)
				(length 3.81)
				(name "_INTA")
				(number "A6")
			)
			(pin output line
				(at 11.43 -110.49 180)
				(length 3.81)
				(name "_REQ64")
				(number "A60")
			)
			(pin power_in line
				(at 11.43 -114.3 180)
				(length 3.81)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at 11.43 -118.11 180)
				(length 3.81)
				(name "+5V")
				(number "A62")
			)
			(pin output line
				(at 11.43 91.44 180)
				(length 3.81)
				(name "_INTC")
				(number "A7")
			)
			(pin power_in line
				(at 11.43 87.63 180)
				(length 3.81)
				(name "+5V")
				(number "A8")
			)
			(pin no_connect line
				(at 11.43 83.82 180)
				(length 3.81)
				(name "NC")
				(number "A9")
			)
			(pin power_in line
				(at -11.43 113.03 0)
				(length 3.81)
				(name "-12V")
				(number "B1")
			)
			(pin no_connect line
				(at -11.43 78.74 0)
				(length 3.81)
				(name "NC")
				(number "B10")
			)
			(pin output line
				(at -11.43 74.93 0)
				(length 3.81)
				(name "_PRSNT2")
				(number "B11")
			)
			(pin no_connect line
				(at -11.43 63.5 0)
				(length 3.81)
				(name "NC")
				(number "B14")
			)
			(pin power_in line
				(at -11.43 59.69 0)
				(length 3.81)
				(name "GND")
				(number "B15")
			)
			(pin input line
				(at -11.43 55.88 0)
				(length 3.81)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -11.43 52.07 0)
				(length 3.81)
				(name "GND")
				(number "B17")
			)
			(pin output line
				(at -11.43 48.26 0)
				(length 3.81)
				(name "_REQ")
				(number "B18")
			)
			(pin power_in line
				(at -11.43 44.45 0)
				(length 3.81)
				(name "+5Vio")
				(number "B19")
			)
			(pin input line
				(at -11.43 109.22 0)
				(length 3.81)
				(name "TCK")
				(number "B2")
			)
			(pin bidirectional line
				(at -11.43 40.64 0)
				(length 3.81)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at -11.43 36.83 0)
				(length 3.81)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -11.43 33.02 0)
				(length 3.81)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at -11.43 29.21 0)
				(length 3.81)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at -11.43 25.4 0)
				(length 3.81)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -11.43 21.59 0)
				(length 3.81)
				(name "3V3")
				(number "B25")
			)
			(pin input line
				(at -11.43 17.78 0)
				(length 3.81)
				(name "_CBE[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at -11.43 13.97 0)
				(length 3.81)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -11.43 10.16 0)
				(length 3.81)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at -11.43 6.35 0)
				(length 3.81)
				(name "AD[21]")
				(number "B29")
			)
			(pin power_in line
				(at -11.43 105.41 0)
				(length 3.81)
				(name "GND")
				(number "B3")
			)
			(pin bidirectional line
				(at -11.43 2.54 0)
				(length 3.81)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -11.43 -1.27 0)
				(length 3.81)
				(name "+3V3")
				(number "B31")
			)
			(pin bidirectional line
				(at -11.43 -5.08 0)
				(length 3.81)
				(name "AD[17]")
				(number "B32")
			)
			(pin input line
				(at -11.43 -8.89 0)
				(length 3.81)
				(name "_CBE[2]")
				(number "B33")
			)
			(pin power_in line
				(at -11.43 -12.7 0)
				(length 3.81)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional line
				(at -11.43 -16.51 0)
				(length 3.81)
				(name "_IRDY")
				(number "B35")
			)
			(pin power_in line
				(at -11.43 -20.32 0)
				(length 3.81)
				(name "+3V3")
				(number "B36")
			)
			(pin bidirectional line
				(at -11.43 -24.13 0)
				(length 3.81)
				(name "_DEVSEL")
				(number "B37")
			)
			(pin power_in line
				(at -11.43 -27.94 0)
				(length 3.81)
				(name "GND")
				(number "B38")
			)
			(pin no_connect line
				(at -11.43 -31.75 0)
				(length 3.81)
				(name "_LOCK")
				(number "B39")
			)
			(pin no_connect line
				(at -11.43 101.6 0)
				(length 3.81)
				(name "TDO")
				(number "B4")
			)
			(pin output line
				(at -11.43 -35.56 0)
				(length 3.81)
				(name "_PERR")
				(number "B40")
			)
			(pin power_in line
				(at -11.43 -39.37 0)
				(length 3.81)
				(name "+3V3")
				(number "B41")
			)
			(pin output line
				(at -11.43 -43.18 0)
				(length 3.81)
				(name "_SERR")
				(number "B42")
			)
			(pin power_in line
				(at -11.43 -46.99 0)
				(length 3.81)
				(name "+3V3")
				(number "B43")
			)
			(pin input line
				(at -11.43 -50.8 0)
				(length 3.81)
				(name "_CBE[1]")
				(number "B44")
			)
			(pin bidirectional line
				(at -11.43 -54.61 0)
				(length 3.81)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -11.43 -58.42 0)
				(length 3.81)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at -11.43 -62.23 0)
				(length 3.81)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at -11.43 -66.04 0)
				(length 3.81)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -11.43 -69.85 0)
				(length 3.81)
				(name "GND")
				(number "B49")
			)
			(pin power_in line
				(at -11.43 97.79 0)
				(length 3.81)
				(name "+5V")
				(number "B5")
			)
			(pin power_in line
				(at -11.43 -73.66 0)
				(length 3.81)
				(name "GND")
				(number "B50")
			)
			(pin power_in line
				(at -11.43 -77.47 0)
				(length 3.81)
				(name "GND")
				(number "B51")
			)
			(pin bidirectional line
				(at -11.43 -81.28 0)
				(length 3.81)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at -11.43 -85.09 0)
				(length 3.81)
				(name "AD[07]")
				(number "B53")
			)
			(pin power_in line
				(at -11.43 -88.9 0)
				(length 3.81)
				(name "+3V3")
				(number "B54")
			)
			(pin bidirectional line
				(at -11.43 -92.71 0)
				(length 3.81)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at -11.43 -96.52 0)
				(length 3.81)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -11.43 -100.33 0)
				(length 3.81)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at -11.43 -104.14 0)
				(length 3.81)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -11.43 -107.95 0)
				(length 3.81)
				(name "+5Vio")
				(number "B59")
			)
			(pin power_in line
				(at -11.43 93.98 0)
				(length 3.81)
				(name "+5V")
				(number "B6")
			)
			(pin output line
				(at -11.43 -111.76 0)
				(length 3.81)
				(name "_ACK64")
				(number "B60")
			)
			(pin power_in line
				(at -11.43 -115.57 0)
				(length 3.81)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -11.43 -119.38 0)
				(length 3.81)
				(name "+5V")
				(number "B62")
			)
			(pin output line
				(at -11.43 90.17 0)
				(length 3.81)
				(name "_INTB")
				(number "B7")
			)
			(pin output line
				(at -11.43 86.36 0)
				(length 3.81)
				(name "_INTD")
				(number "B8")
			)
			(pin output line
				(at -11.43 82.55 0)
				(length 3.81)
				(name "_PRSNT1")
				(number "B9")
			)
		)
		(symbol "PCI32-3V3_0_1")
	)
	(symbol "PCI32-5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 0 119.38 0)
		)
		(property "Value" "PCI32-5V"
			(at 0 -124.206 0)
		)
		(property "Footprint" "A2900:PCI-5V"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PCI32-5V_0_0"
			(pin input line
				(at 11.43 114.3 180)
				(length 3.81)
				(name "_TRST")
				(number "A1")
			)
			(pin power_in line
				(at 11.43 80.01 180)
				(length 3.81)
				(name "+5Vio")
				(number "A10")
			)
			(pin no_connect line
				(at 11.43 76.2 180)
				(length 3.81)
				(name "NC")
				(number "A11")
			)
			(pin power_in line
				(at 11.43 72.39 180)
				(length 3.81)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at 11.43 68.58 180)
				(length 3.81)
				(name "GND")
				(number "A13")
			)
			(pin no_connect line
				(at 11.43 64.77 180)
				(length 3.81)
				(name "+3V3aux")
				(number "A14")
			)
			(pin input line
				(at 11.43 60.96 180)
				(length 3.81)
				(name "_RESET")
				(number "A15")
			)
			(pin power_in line
				(at 11.43 57.15 180)
				(length 3.81)
				(name "+5Vio")
				(number "A16")
			)
			(pin input line
				(at 11.43 53.34 180)
				(length 3.81)
				(name "_GNT")
				(number "A17")
			)
			(pin power_in line
				(at 11.43 49.53 180)
				(length 3.81)
				(name "GND")
				(number "A18")
			)
			(pin no_connect line
				(at 11.43 45.72 180)
				(length 3.81)
				(name "_PME")
				(number "A19")
			)
			(pin power_in line
				(at 11.43 110.49 180)
				(length 3.81)
				(name "+12V")
				(number "A2")
			)
			(pin bidirectional line
				(at 11.43 41.91 180)
				(length 3.81)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at 11.43 38.1 180)
				(length 3.81)
				(name "+3V3")
				(number "A21")
			)
			(pin bidirectional line
				(at 11.43 34.29 180)
				(length 3.81)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 11.43 30.48 180)
				(length 3.81)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at 11.43 26.67 180)
				(length 3.81)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 11.43 22.86 180)
				(length 3.81)
				(name "AD[24]")
				(number "A25")
			)
			(pin input line
				(at 11.43 19.05 180)
				(length 3.81)
				(name "IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at 11.43 15.24 180)
				(length 3.81)
				(name "+3V3")
				(number "A27")
			)
			(pin bidirectional line
				(at 11.43 11.43 180)
				(length 3.81)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 11.43 7.62 180)
				(length 3.81)
				(name "AD[20]")
				(number "A29")
			)
			(pin input line
				(at 11.43 106.68 180)
				(length 3.81)
				(name "TMS")
				(number "A3")
			)
			(pin power_in line
				(at 11.43 3.81 180)
				(length 3.81)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 11.43 0 180)
				(length 3.81)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 11.43 -3.81 180)
				(length 3.81)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at 11.43 -7.62 180)
				(length 3.81)
				(name "+3V3")
				(number "A33")
			)
			(pin bidirectional line
				(at 11.43 -11.43 180)
				(length 3.81)
				(name "_FRAME")
				(number "A34")
			)
			(pin power_in line
				(at 11.43 -15.24 180)
				(length 3.81)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional line
				(at 11.43 -19.05 180)
				(length 3.81)
				(name "_TRDY")
				(number "A36")
			)
			(pin power_in line
				(at 11.43 -22.86 180)
				(length 3.81)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional line
				(at 11.43 -26.67 180)
				(length 3.81)
				(name "_STOP")
				(number "A38")
			)
			(pin power_in line
				(at 11.43 -30.48 180)
				(length 3.81)
				(name "+3V3")
				(number "A39")
			)
			(pin input line
				(at 11.43 102.87 180)
				(length 3.81)
				(name "TDI")
				(number "A4")
			)
			(pin input line
				(at 11.43 -34.29 180)
				(length 3.81)
				(name "SMBCLK")
				(number "A40")
			)
			(pin input line
				(at 11.43 -38.1 180)
				(length 3.81)
				(name "SMBDAT")
				(number "A41")
			)
			(pin power_in line
				(at 11.43 -41.91 180)
				(length 3.81)
				(name "GND")
				(number "A42")
			)
			(pin input line
				(at 11.43 -45.72 180)
				(length 3.81)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 11.43 -49.53 180)
				(length 3.81)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at 11.43 -53.34 180)
				(length 3.81)
				(name "+3V3")
				(number "A45")
			)
			(pin bidirectional line
				(at 11.43 -57.15 180)
				(length 3.81)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 11.43 -60.96 180)
				(length 3.81)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at 11.43 -64.77 180)
				(length 3.81)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 11.43 -68.58 180)
				(length 3.81)
				(name "AD[09]")
				(number "A49")
			)
			(pin power_in line
				(at 11.43 99.06 180)
				(length 3.81)
				(name "+5V")
				(number "A5")
			)
			(pin input line
				(at 11.43 -80.01 180)
				(length 3.81)
				(name "_CBE[0]")
				(number "A52")
			)
			(pin power_in line
				(at 11.43 -83.82 180)
				(length 3.81)
				(name "+3V3")
				(number "A53")
			)
			(pin bidirectional line
				(at 11.43 -87.63 180)
				(length 3.81)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 11.43 -91.44 180)
				(length 3.81)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at 11.43 -95.25 180)
				(length 3.81)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 11.43 -99.06 180)
				(length 3.81)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 11.43 -102.87 180)
				(length 3.81)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at 11.43 -106.68 180)
				(length 3.81)
				(name "+5Vio")
				(number "A59")
			)
			(pin output line
				(at 11.43 95.25 180)
				(length 3.81)
				(name "_INTA")
				(number "A6")
			)
			(pin output line
				(at 11.43 -110.49 180)
				(length 3.81)
				(name "_REQ64")
				(number "A60")
			)
			(pin power_in line
				(at 11.43 -114.3 180)
				(length 3.81)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at 11.43 -118.11 180)
				(length 3.81)
				(name "+5V")
				(number "A62")
			)
			(pin output line
				(at 11.43 91.44 180)
				(length 3.81)
				(name "_INTC")
				(number "A7")
			)
			(pin power_in line
				(at 11.43 87.63 180)
				(length 3.81)
				(name "+5V")
				(number "A8")
			)
			(pin no_connect line
				(at 11.43 83.82 180)
				(length 3.81)
				(name "NC")
				(number "A9")
			)
			(pin power_in line
				(at -11.43 113.03 0)
				(length 3.81)
				(name "-12V")
				(number "B1")
			)
			(pin no_connect line
				(at -11.43 78.74 0)
				(length 3.81)
				(name "NC")
				(number "B10")
			)
			(pin output line
				(at -11.43 74.93 0)
				(length 3.81)
				(name "_PRSNT2")
				(number "B11")
			)
			(pin power_in line
				(at -11.43 71.12 0)
				(length 3.81)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -11.43 67.31 0)
				(length 3.81)
				(name "GND")
				(number "B13")
			)
			(pin no_connect line
				(at -11.43 63.5 0)
				(length 3.81)
				(name "NC")
				(number "B14")
			)
			(pin power_in line
				(at -11.43 59.69 0)
				(length 3.81)
				(name "GND")
				(number "B15")
			)
			(pin input line
				(at -11.43 55.88 0)
				(length 3.81)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -11.43 52.07 0)
				(length 3.81)
				(name "GND")
				(number "B17")
			)
			(pin output line
				(at -11.43 48.26 0)
				(length 3.81)
				(name "_REQ")
				(number "B18")
			)
			(pin power_in line
				(at -11.43 44.45 0)
				(length 3.81)
				(name "+5Vio")
				(number "B19")
			)
			(pin input line
				(at -11.43 109.22 0)
				(length 3.81)
				(name "TCK")
				(number "B2")
			)
			(pin bidirectional line
				(at -11.43 40.64 0)
				(length 3.81)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at -11.43 36.83 0)
				(length 3.81)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -11.43 33.02 0)
				(length 3.81)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at -11.43 29.21 0)
				(length 3.81)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at -11.43 25.4 0)
				(length 3.81)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -11.43 21.59 0)
				(length 3.81)
				(name "3V3")
				(number "B25")
			)
			(pin input line
				(at -11.43 17.78 0)
				(length 3.81)
				(name "_CBE[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at -11.43 13.97 0)
				(length 3.81)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -11.43 10.16 0)
				(length 3.81)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at -11.43 6.35 0)
				(length 3.81)
				(name "AD[21]")
				(number "B29")
			)
			(pin power_in line
				(at -11.43 105.41 0)
				(length 3.81)
				(name "GND")
				(number "B3")
			)
			(pin bidirectional line
				(at -11.43 2.54 0)
				(length 3.81)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -11.43 -1.27 0)
				(length 3.81)
				(name "+3V3")
				(number "B31")
			)
			(pin bidirectional line
				(at -11.43 -5.08 0)
				(length 3.81)
				(name "AD[17]")
				(number "B32")
			)
			(pin input line
				(at -11.43 -8.89 0)
				(length 3.81)
				(name "_CBE[2]")
				(number "B33")
			)
			(pin power_in line
				(at -11.43 -12.7 0)
				(length 3.81)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional line
				(at -11.43 -16.51 0)
				(length 3.81)
				(name "_IRDY")
				(number "B35")
			)
			(pin power_in line
				(at -11.43 -20.32 0)
				(length 3.81)
				(name "+3V3")
				(number "B36")
			)
			(pin bidirectional line
				(at -11.43 -24.13 0)
				(length 3.81)
				(name "_DEVSEL")
				(number "B37")
			)
			(pin power_in line
				(at -11.43 -27.94 0)
				(length 3.81)
				(name "GND")
				(number "B38")
			)
			(pin no_connect line
				(at -11.43 -31.75 0)
				(length 3.81)
				(name "_LOCK")
				(number "B39")
			)
			(pin no_connect line
				(at -11.43 101.6 0)
				(length 3.81)
				(name "TDO")
				(number "B4")
			)
			(pin output line
				(at -11.43 -35.56 0)
				(length 3.81)
				(name "_PERR")
				(number "B40")
			)
			(pin power_in line
				(at -11.43 -39.37 0)
				(length 3.81)
				(name "+3V3")
				(number "B41")
			)
			(pin output line
				(at -11.43 -43.18 0)
				(length 3.81)
				(name "_SERR")
				(number "B42")
			)
			(pin power_in line
				(at -11.43 -46.99 0)
				(length 3.81)
				(name "+3V3")
				(number "B43")
			)
			(pin input line
				(at -11.43 -50.8 0)
				(length 3.81)
				(name "_CBE[1]")
				(number "B44")
			)
			(pin bidirectional line
				(at -11.43 -54.61 0)
				(length 3.81)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -11.43 -58.42 0)
				(length 3.81)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at -11.43 -62.23 0)
				(length 3.81)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at -11.43 -66.04 0)
				(length 3.81)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -11.43 -69.85 0)
				(length 3.81)
				(name "GND")
				(number "B49")
			)
			(pin power_in line
				(at -11.43 97.79 0)
				(length 3.81)
				(name "+5V")
				(number "B5")
			)
			(pin bidirectional line
				(at -11.43 -81.28 0)
				(length 3.81)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at -11.43 -85.09 0)
				(length 3.81)
				(name "AD[07]")
				(number "B53")
			)
			(pin power_in line
				(at -11.43 -88.9 0)
				(length 3.81)
				(name "+3V3")
				(number "B54")
			)
			(pin bidirectional line
				(at -11.43 -92.71 0)
				(length 3.81)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at -11.43 -96.52 0)
				(length 3.81)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -11.43 -100.33 0)
				(length 3.81)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at -11.43 -104.14 0)
				(length 3.81)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -11.43 -107.95 0)
				(length 3.81)
				(name "+5Vio")
				(number "B59")
			)
			(pin power_in line
				(at -11.43 93.98 0)
				(length 3.81)
				(name "+5V")
				(number "B6")
			)
			(pin output line
				(at -11.43 -111.76 0)
				(length 3.81)
				(name "_ACK64")
				(number "B60")
			)
			(pin power_in line
				(at -11.43 -115.57 0)
				(length 3.81)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -11.43 -119.38 0)
				(length 3.81)
				(name "+5V")
				(number "B62")
			)
			(pin output line
				(at -11.43 90.17 0)
				(length 3.81)
				(name "_INTB")
				(number "B7")
			)
			(pin output line
				(at -11.43 86.36 0)
				(length 3.81)
				(name "_INTD")
				(number "B8")
			)
			(pin output line
				(at -11.43 82.55 0)
				(length 3.81)
				(name "_PRSNT1")
				(number "B9")
			)
		)
		(symbol "PCI32-5V_0_1")
	)
	(symbol "PCI32-5V-Option2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 0 119.38 0)
		)
		(property "Value" "PCI32-5V"
			(at 0 -116.84 0)
		)
		(property "Footprint" "A2900:PCI-5V"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PCI32-5V-Option2_0_0"
			(pin input line
				(at 11.43 -106.68 180)
				(length 3.81)
				(name "_TRST")
				(number "A1")
			)
			(pin power_in line
				(at -11.43 29.21 0)
				(length 3.81)
				(name "+5Vio")
				(number "A10")
			)
			(pin no_connect line
				(at -11.43 -88.9 0)
				(length 3.81)
				(name "NC")
				(number "A11")
			)
			(pin power_in line
				(at -11.43 -1.27 0)
				(length 3.81)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at -11.43 -5.08 0)
				(length 3.81)
				(name "GND")
				(number "A13")
			)
			(pin no_connect line
				(at -11.43 63.5 0)
				(length 3.81)
				(name "+3V3aux")
				(number "A14")
			)
			(pin input line
				(at 11.43 -91.44 180)
				(length 3.81)
				(name "_RESET")
				(number "A15")
			)
			(pin power_in line
				(at -11.43 25.4 0)
				(length 3.81)
				(name "+5Vio")
				(number "A16")
			)
			(pin input line
				(at 11.43 -45.72 180)
				(length 3.81)
				(name "_GNT")
				(number "A17")
			)
			(pin power_in line
				(at -11.43 -8.89 0)
				(length 3.81)
				(name "GND")
				(number "A18")
			)
			(pin no_connect line
				(at 11.43 -76.2 180)
				(length 3.81)
				(name "_PME")
				(number "A19")
			)
			(pin power_in line
				(at -11.43 113.03 0)
				(length 3.81)
				(name "+12V")
				(number "A2")
			)
			(pin bidirectional line
				(at 11.43 -3.81 180)
				(length 3.81)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at -11.43 109.22 0)
				(length 3.81)
				(name "+3V3")
				(number "A21")
			)
			(pin bidirectional line
				(at 11.43 3.81 180)
				(length 3.81)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 11.43 11.43 180)
				(length 3.81)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at -11.43 -12.7 0)
				(length 3.81)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 11.43 19.05 180)
				(length 3.81)
				(name "AD[24]")
				(number "A25")
			)
			(pin input line
				(at 11.43 -11.43 180)
				(length 3.81)
				(name "_IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at -11.43 105.41 0)
				(length 3.81)
				(name "+3V3")
				(number "A27")
			)
			(pin bidirectional line
				(at 11.43 26.67 180)
				(length 3.81)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 11.43 34.29 180)
				(length 3.81)
				(name "AD[20]")
				(number "A29")
			)
			(pin input line
				(at -11.43 -111.76 0)
				(length 3.81)
				(name "TMS")
				(number "A3")
			)
			(pin power_in line
				(at -11.43 -16.51 0)
				(length 3.81)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 11.43 41.91 180)
				(length 3.81)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 11.43 49.53 180)
				(length 3.81)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at -11.43 101.6 0)
				(length 3.81)
				(name "+3V3")
				(number "A33")
			)
			(pin bidirectional line
				(at 11.43 -38.1 180)
				(length 3.81)
				(name "_FRAME")
				(number "A34")
			)
			(pin power_in line
				(at -11.43 -20.32 0)
				(length 3.81)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional line
				(at 11.43 -102.87 180)
				(length 3.81)
				(name "_TRDY")
				(number "A36")
			)
			(pin power_in line
				(at -11.43 -24.13 0)
				(length 3.81)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional line
				(at 11.43 -99.06 180)
				(length 3.81)
				(name "_STOP")
				(number "A38")
			)
			(pin power_in line
				(at -11.43 97.79 0)
				(length 3.81)
				(name "+3V3")
				(number "A39")
			)
			(pin input line
				(at -11.43 -104.14 0)
				(length 3.81)
				(name "TDI")
				(number "A4")
			)
			(pin input line
				(at -11.43 6.35 0)
				(length 3.81)
				(name "SMBCLK")
				(number "A40")
			)
			(pin input line
				(at -11.43 2.54 0)
				(length 3.81)
				(name "SMBDAT")
				(number "A41")
			)
			(pin power_in line
				(at -11.43 -27.94 0)
				(length 3.81)
				(name "GND")
				(number "A42")
			)
			(pin input line
				(at 11.43 -87.63 180)
				(length 3.81)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 11.43 53.34 180)
				(length 3.81)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at -11.43 93.98 0)
				(length 3.81)
				(name "+3V3")
				(number "A45")
			)
			(pin bidirectional line
				(at 11.43 60.96 180)
				(length 3.81)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 11.43 68.58 180)
				(length 3.81)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at -11.43 -31.75 0)
				(length 3.81)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 11.43 76.2 180)
				(length 3.81)
				(name "AD[09]")
				(number "A49")
			)
			(pin power_in line
				(at -11.43 59.69 0)
				(length 3.81)
				(name "+5V")
				(number "A5")
			)
			(pin input line
				(at 11.43 -15.24 180)
				(length 3.81)
				(name "_CBE[0]")
				(number "A52")
			)
			(pin power_in line
				(at -11.43 90.17 0)
				(length 3.81)
				(name "+3V3")
				(number "A53")
			)
			(pin bidirectional line
				(at 11.43 87.63 180)
				(length 3.81)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 11.43 95.25 180)
				(length 3.81)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at -11.43 -35.56 0)
				(length 3.81)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 11.43 102.87 180)
				(length 3.81)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 11.43 110.49 180)
				(length 3.81)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at -11.43 21.59 0)
				(length 3.81)
				(name "+5Vio")
				(number "A59")
			)
			(pin output line
				(at 11.43 -49.53 180)
				(length 3.81)
				(name "_INTA")
				(number "A6")
			)
			(pin output line
				(at -11.43 10.16 0)
				(length 3.81)
				(name "_REQ64")
				(number "A60")
			)
			(pin power_in line
				(at -11.43 52.07 0)
				(length 3.81)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at -11.43 48.26 0)
				(length 3.81)
				(name "+5V")
				(number "A62")
			)
			(pin output line
				(at 11.43 -57.15 180)
				(length 3.81)
				(name "_INTC")
				(number "A7")
			)
			(pin power_in line
				(at -11.43 55.88 0)
				(length 3.81)
				(name "+5V")
				(number "A8")
			)
			(pin no_connect line
				(at -11.43 -85.09 0)
				(length 3.81)
				(name "NC")
				(number "A9")
			)
			(pin power_in line
				(at 11.43 114.3 180)
				(length 3.81)
				(name "-12V")
				(number "B1")
			)
			(pin no_connect line
				(at -11.43 -92.71 0)
				(length 3.81)
				(name "NC")
				(number "B10")
			)
			(pin output line
				(at 11.43 -83.82 180)
				(length 3.81)
				(name "_PRSNT2")
				(number "B11")
			)
			(pin power_in line
				(at -11.43 -43.18 0)
				(length 3.81)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -11.43 -46.99 0)
				(length 3.81)
				(name "GND")
				(number "B13")
			)
			(pin no_connect line
				(at -11.43 -96.52 0)
				(length 3.81)
				(name "NC")
				(number "B14")
			)
			(pin power_in line
				(at -11.43 -50.8 0)
				(length 3.81)
				(name "GND")
				(number "B15")
			)
			(pin input line
				(at 11.43 -110.49 180)
				(length 3.81)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -11.43 -54.61 0)
				(length 3.81)
				(name "GND")
				(number "B17")
			)
			(pin output line
				(at 11.43 -41.91 180)
				(length 3.81)
				(name "_REQ")
				(number "B18")
			)
			(pin power_in line
				(at -11.43 17.78 0)
				(length 3.81)
				(name "+5Vio")
				(number "B19")
			)
			(pin input line
				(at -11.43 -100.33 0)
				(length 3.81)
				(name "TCK")
				(number "B2")
			)
			(pin bidirectional line
				(at 11.43 -7.62 180)
				(length 3.81)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at 11.43 0 180)
				(length 3.81)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -11.43 -58.42 0)
				(length 3.81)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at 11.43 7.62 180)
				(length 3.81)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at 11.43 15.24 180)
				(length 3.81)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -11.43 67.31 0)
				(length 3.81)
				(name "+3V3")
				(number "B25")
			)
			(pin input line
				(at 11.43 -26.67 180)
				(length 3.81)
				(name "_CBE[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at 11.43 22.86 180)
				(length 3.81)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -11.43 -62.23 0)
				(length 3.81)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at 11.43 30.48 180)
				(length 3.81)
				(name "AD[21]")
				(number "B29")
			)
			(pin power_in line
				(at -11.43 -39.37 0)
				(length 3.81)
				(name "GND")
				(number "B3")
			)
			(pin bidirectional line
				(at 11.43 38.1 180)
				(length 3.81)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -11.43 86.36 0)
				(length 3.81)
				(name "+3V3")
				(number "B31")
			)
			(pin bidirectional line
				(at 11.43 45.72 180)
				(length 3.81)
				(name "AD[17]")
				(number "B32")
			)
			(pin input line
				(at 11.43 -22.86 180)
				(length 3.81)
				(name "_CBE[2]")
				(number "B33")
			)
			(pin power_in line
				(at -11.43 -66.04 0)
				(length 3.81)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional line
				(at 11.43 -64.77 180)
				(length 3.81)
				(name "_IRDY")
				(number "B35")
			)
			(pin power_in line
				(at -11.43 82.55 0)
				(length 3.81)
				(name "+3V3")
				(number "B36")
			)
			(pin bidirectional line
				(at 11.43 -34.29 180)
				(length 3.81)
				(name "_DEVSEL")
				(number "B37")
			)
			(pin power_in line
				(at -11.43 -69.85 0)
				(length 3.81)
				(name "GND")
				(number "B38")
			)
			(pin bidirectional line
				(at 11.43 -68.58 180)
				(length 3.81)
				(name "_LOCK")
				(number "B39")
			)
			(pin no_connect line
				(at -11.43 -107.95 0)
				(length 3.81)
				(name "TDO")
				(number "B4")
			)
			(pin output line
				(at 11.43 -72.39 180)
				(length 3.81)
				(name "_PERR")
				(number "B40")
			)
			(pin power_in line
				(at -11.43 78.74 0)
				(length 3.81)
				(name "+3V3")
				(number "B41")
			)
			(pin output line
				(at 11.43 -95.25 180)
				(length 3.81)
				(name "_SERR")
				(number "B42")
			)
			(pin power_in line
				(at -11.43 74.93 0)
				(length 3.81)
				(name "+3V3")
				(number "B43")
			)
			(pin input line
				(at 11.43 -19.05 180)
				(length 3.81)
				(name "_CBE[1]")
				(number "B44")
			)
			(pin bidirectional line
				(at 11.43 57.15 180)
				(length 3.81)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -11.43 -73.66 0)
				(length 3.81)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at 11.43 64.77 180)
				(length 3.81)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at 11.43 72.39 180)
				(length 3.81)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -11.43 -77.47 0)
				(length 3.81)
				(name "GND")
				(number "B49")
			)
			(pin power_in line
				(at -11.43 44.45 0)
				(length 3.81)
				(name "+5V")
				(number "B5")
			)
			(pin bidirectional line
				(at 11.43 80.01 180)
				(length 3.81)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at 11.43 83.82 180)
				(length 3.81)
				(name "AD[07]")
				(number "B53")
			)
			(pin power_in line
				(at -11.43 71.12 0)
				(length 3.81)
				(name "+3V3")
				(number "B54")
			)
			(pin bidirectional line
				(at 11.43 91.44 180)
				(length 3.81)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at 11.43 99.06 180)
				(length 3.81)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -11.43 -81.28 0)
				(length 3.81)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at 11.43 106.68 180)
				(length 3.81)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -11.43 13.97 0)
				(length 3.81)
				(name "+5Vio")
				(number "B59")
			)
			(pin power_in line
				(at -11.43 40.64 0)
				(length 3.81)
				(name "+5V")
				(number "B6")
			)
			(pin output line
				(at 11.43 -30.48 180)
				(length 3.81)
				(name "_ACK64")
				(number "B60")
			)
			(pin power_in line
				(at -11.43 36.83 0)
				(length 3.81)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -11.43 33.02 0)
				(length 3.81)
				(name "+5V")
				(number "B62")
			)
			(pin output line
				(at 11.43 -53.34 180)
				(length 3.81)
				(name "_INTB")
				(number "B7")
			)
			(pin output line
				(at 11.43 -60.96 180)
				(length 3.81)
				(name "_INTD")
				(number "B8")
			)
			(pin output line
				(at 11.43 -80.01 180)
				(length 3.81)
				(name "_PRSNT1")
				(number "B9")
			)
		)
		(symbol "PCI32-5V-Option2_0_1")
	)
	(symbol "R_SM_Network08"
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RN"
			(at -12.7 0 90)
		)
		(property "Value" "R_SM_Network08"
			(at 10.795 0.0254 90)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_5x1206"
			(at 12.7 0.0254 90)
		)
		(property "Datasheet" "https://www.ctscorp.com/wp-content/uploads/74x.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 resistor network, SMD, bussed resistors, small symbol"
			(at 0 0 0)
		)
		(property "Part" "746X101102JP"
			(at 0 0 0)
		)
		(property "ki_keywords" "R network"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R?Array?SIP*"
			(at 0 0 0)
		)
		(symbol "R_SM_Network08_0_1")
		(symbol "R_SM_Network08_1_0"
			(pin passive line
				(at 7.62 6.35 270)
				(length 3.81)
				(name "common")
				(number "10")
			)
		)
		(symbol "R_SM_Network08_1_1"
			(pin passive line
				(at -10.16 -5.08 90)
				(length 1.27)
				(name "R1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -5.08 90)
				(length 1.27)
				(name "R2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 90)
				(length 1.27)
				(name "R3")
				(number "3")
			)
			(pin passive line
				(at -2.54 -5.08 90)
				(length 1.27)
				(name "R4")
				(number "4")
			)
			(pin passive line
				(at -10.16 6.35 270)
				(length 3.81)
				(name "common")
				(number "5")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 1.27)
				(name "R5")
				(number "6")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 1.27)
				(name "R6")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 90)
				(length 1.27)
				(name "R7")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 90)
				(length 1.27)
				(name "R8")
				(number "9")
			)
		)
	)
	(symbol "SDRAM(16Mx32)"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "SDRAM(16Mx32)"
			(at 0 -2.54 0)
		)
		(property "Footprint" "AmigaPCI:TSOP-II-86"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/42-45R-S-32160F.pdf"
			(at 0 3.81 0)
		)
		(property "Description" "16M x 32 bit Synchronous DRAM (SDRAM), TSOP II 86pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronus DRAM PC166 PC143 MEMORY"
			(at 0 0 0)
		)
		(symbol "SDRAM(16Mx32)_0_0"
			(pin power_in line
				(at -15.24 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
		)
		(symbol "SDRAM(16Mx32)_0_1")
		(symbol "SDRAM(16Mx32)_1_0"
			(pin power_in line
				(at -12.7 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "A11")
				(number "21")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "DQ28")
				(number "51")
			)
			(pin power_in line
				(at 10.16 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "DQ29")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "DQ30")
				(number "54")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "DQ31")
				(number "56")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "57")
			)
			(pin power_in line
				(at -10.16 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "58")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "DQM3")
				(number "59")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "A3")
				(number "60")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "A4")
				(number "61")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "A5")
				(number "62")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "A6")
				(number "63")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "A7")
				(number "64")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "A8")
				(number "65")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "A9")
				(number "66")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "CKE")
				(number "67")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "CLK")
				(number "68")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "A12")
				(number "69")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "69")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "70")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "DQM1")
				(number "71")
			)
			(pin power_in line
				(at -7.62 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "72")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "73")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "DQ8")
				(number "74")
			)
			(pin power_in line
				(at 12.7 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "DQ9")
				(number "76")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "DQ10")
				(number "77")
			)
			(pin power_in line
				(at 12.7 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "78")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "DQ11")
				(number "79")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "DQ12")
				(number "80")
			)
			(pin power_in line
				(at 15.24 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "81")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "DQ13")
				(number "82")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "DQ14")
				(number "83")
			)
			(pin power_in line
				(at 15.24 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "84")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "DQ15")
				(number "85")
			)
			(pin power_in line
				(at -12.7 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "86")
			)
		)
		(symbol "SDRAM(16Mx32)_1_1"
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "DQ6")
				(number "11")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "DQ7")
				(number "13")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "NC")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "DQM0")
				(number "16")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "_WE")
				(number "17")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "_CAS")
				(number "18")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "_RAS")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "DQ0")
				(number "2")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "_CS")
				(number "20")
			)
			(pin no_connect line
				(at -22.86 -38.1 0)
				(length 5.08) hide
				(name "NC")
				(number "21")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "BA0")
				(number "22")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "BA1")
				(number "23")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "A10")
				(number "24")
			)
			(pin input line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "A0")
				(number "25")
			)
			(pin input line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "A1")
				(number "26")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "A2")
				(number "27")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "DQM2")
				(number "28")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "29")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "DQ16")
				(number "31")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "DQ17")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "DQ18")
				(number "34")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "DQ19")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "DQ20")
				(number "37")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "DQ21")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "DQ1")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "DQ22")
				(number "40")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "DQ23")
				(number "42")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at -15.24 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "DQ24")
				(number "45")
			)
			(pin power_in line
				(at 7.62 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "DQ25")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "DQ26")
				(number "48")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "DQ27")
				(number "50")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSSQ")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "DQ4")
				(number "8")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDDQ")
				(number "9")
			)
		)
	)
	(symbol "SDRAM_256MB(16Mx16)"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "SDRAM(16Mx16)"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 -6.35 0)
		)
		(property "Description" "256Mb – (16M x 16 bit) Synchronous DRAM (SDRAM), TSOP II 54pin"
			(at 0 0 0)
		)
		(symbol "SDRAM_256MB(16Mx16)_0_0"
			(pin input line
				(at -20.32 -3.81 0)
				(length 3.81)
				(name "A12")
				(number "36")
			)
		)
		(symbol "SDRAM_256MB(16Mx16)_0_1")
		(symbol "SDRAM_256MB(16Mx16)_1_0"
			(pin no_connect line
				(at 10.16 31.75 270)
				(length 2.54) hide
				(name "NC")
				(number "40")
			)
		)
		(symbol "SDRAM_256MB(16Mx16)_1_1"
			(pin power_in line
				(at -7.62 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 13.97 180)
				(length 3.81)
				(name "DQ5")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 11.43 180)
				(length 3.81)
				(name "DQ6")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "VSSQ")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 8.89 180)
				(length 3.81)
				(name "DQ7")
				(number "13")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "LDQM")
				(number "15")
			)
			(pin input inverted
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "WE")
				(number "16")
			)
			(pin input inverted
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "CAS")
				(number "17")
			)
			(pin input inverted
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "RAS")
				(number "18")
			)
			(pin input inverted
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "CS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 26.67 180)
				(length 3.81)
				(name "DQ0")
				(number "2")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "BA0")
				(number "20")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "BA1")
				(number "21")
			)
			(pin input line
				(at -20.32 1.27 0)
				(length 3.81)
				(name "A10")
				(number "22")
			)
			(pin input line
				(at -20.32 26.67 0)
				(length 3.81)
				(name "A0")
				(number "23")
			)
			(pin input line
				(at -20.32 24.13 0)
				(length 3.81)
				(name "A1")
				(number "24")
			)
			(pin input line
				(at -20.32 21.59 0)
				(length 3.81)
				(name "A2")
				(number "25")
			)
			(pin input line
				(at -20.32 19.05 0)
				(length 3.81)
				(name "A3")
				(number "26")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -7.62 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "28")
			)
			(pin input line
				(at -20.32 16.51 0)
				(length 3.81)
				(name "A4")
				(number "29")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDDQ")
				(number "3")
			)
			(pin input line
				(at -20.32 13.97 0)
				(length 3.81)
				(name "A5")
				(number "30")
			)
			(pin input line
				(at -20.32 11.43 0)
				(length 3.81)
				(name "A6")
				(number "31")
			)
			(pin input line
				(at -20.32 8.89 0)
				(length 3.81)
				(name "A7")
				(number "32")
			)
			(pin input line
				(at -20.32 6.35 0)
				(length 3.81)
				(name "A8")
				(number "33")
			)
			(pin input line
				(at -20.32 3.81 0)
				(length 3.81)
				(name "A9")
				(number "34")
			)
			(pin input line
				(at -20.32 -1.27 0)
				(length 3.81)
				(name "A11")
				(number "35")
			)
			(pin input line
				(at -20.32 -16.51 0)
				(length 3.81)
				(name "CKE")
				(number "37")
			)
			(pin input line
				(at -20.32 -13.97 0)
				(length 3.81)
				(name "CLK")
				(number "38")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "UDQM")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 24.13 180)
				(length 3.81)
				(name "DQ1")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 6.35 180)
				(length 3.81)
				(name "DQ8")
				(number "42")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VDDQ")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 3.81 180)
				(length 3.81)
				(name "DQ9")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 1.27 180)
				(length 3.81)
				(name "DQ10")
				(number "45")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 3.81)
				(name "VSSQ")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -1.27 180)
				(length 3.81)
				(name "DQ11")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -3.81 180)
				(length 3.81)
				(name "DQ12")
				(number "48")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 3.81)
				(name "VDDQ")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 21.59 180)
				(length 3.81)
				(name "DQ2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -6.35 180)
				(length 3.81)
				(name "DQ13")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -8.89 180)
				(length 3.81)
				(name "DQ14")
				(number "51")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 3.81)
				(name "VSSQ")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -11.43 180)
				(length 3.81)
				(name "DQ15")
				(number "53")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSSQ")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 19.05 180)
				(length 3.81)
				(name "DQ3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 16.51 180)
				(length 3.81)
				(name "DQ4")
				(number "8")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VDDQ")
				(number "9")
			)
		)
	)
	(symbol "SDRAM_2M(1Mx16)"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 3.81 0)
		)
		(property "Value" "SDRAM_2M(1Mx16)"
			(at 0 -3.81 0)
		)
		(property "Footprint" "TSOPII-54"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.issi.com/WW/pdf/42-45S16100H.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "2M – (1M x 16 bit) Synchronous DRAM (SDRAM), TSOP II 50pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDRAM Synchronus DRAM PC166 PC143 MEMORY"
			(at 0 0 0)
		)
		(symbol "SDRAM_2M(1Mx16)_0_0"
			(pin power_in line
				(at -6.35 34.29 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
		)
		(symbol "SDRAM_2M(1Mx16)_0_1")
		(symbol "SDRAM_2M(1Mx16)_1_0"
			(pin input line
				(at -21.59 -17.78 0)
				(length 5.08)
				(name "_WE")
				(number "15")
			)
		)
		(symbol "SDRAM_2M(1Mx16)_1_1"
			(pin power_in line
				(at 1.27 -34.29 90)
				(length 5.08)
				(name "VSSQ")
				(number "10")
			)
			(pin bidirectional line
				(at 21.59 11.43 180)
				(length 5.08)
				(name "DQ6")
				(number "11")
			)
			(pin bidirectional line
				(at 21.59 8.89 180)
				(length 5.08)
				(name "DQ7")
				(number "12")
			)
			(pin power_in line
				(at 1.27 34.29 270)
				(length 5.08)
				(name "VDDQ")
				(number "13")
			)
			(pin input line
				(at 21.59 -16.51 180)
				(length 5.08)
				(name "_LDQM")
				(number "14")
			)
			(pin input line
				(at -21.59 -15.24 0)
				(length 5.08)
				(name "_CAS")
				(number "16")
			)
			(pin input line
				(at -21.59 -12.7 0)
				(length 5.08)
				(name "_RAS")
				(number "17")
			)
			(pin input line
				(at 21.59 -24.13 180)
				(length 5.08)
				(name "_CS")
				(number "18")
			)
			(pin input line
				(at -21.59 -1.27 0)
				(length 5.08)
				(name "A11")
				(number "19")
			)
			(pin bidirectional line
				(at 21.59 26.67 180)
				(length 5.08)
				(name "DQ0")
				(number "2")
			)
			(pin input line
				(at -21.59 1.27 0)
				(length 5.08)
				(name "A10")
				(number "20")
			)
			(pin input line
				(at -21.59 26.67 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -21.59 24.13 0)
				(length 5.08)
				(name "A1")
				(number "22")
			)
			(pin input line
				(at -21.59 21.59 0)
				(length 5.08)
				(name "A2")
				(number "23")
			)
			(pin input line
				(at -21.59 19.05 0)
				(length 5.08)
				(name "A3")
				(number "24")
			)
			(pin power_in line
				(at -3.81 34.29 270)
				(length 5.08)
				(name "VDD")
				(number "25")
			)
			(pin power_in line
				(at -6.35 -34.29 90)
				(length 5.08)
				(name "VSS")
				(number "26")
			)
			(pin input line
				(at -21.59 16.51 0)
				(length 5.08)
				(name "A4")
				(number "27")
			)
			(pin input line
				(at -21.59 13.97 0)
				(length 5.08)
				(name "A5")
				(number "28")
			)
			(pin input line
				(at -21.59 11.43 0)
				(length 5.08)
				(name "A6")
				(number "29")
			)
			(pin bidirectional line
				(at 21.59 24.13 180)
				(length 5.08)
				(name "DQ1")
				(number "3")
			)
			(pin input line
				(at -21.59 8.89 0)
				(length 5.08)
				(name "A7")
				(number "30")
			)
			(pin input line
				(at -21.59 6.35 0)
				(length 5.08)
				(name "A8")
				(number "31")
			)
			(pin input line
				(at -21.59 3.81 0)
				(length 5.08)
				(name "A9")
				(number "32")
			)
			(pin no_connect line
				(at -21.59 -22.86 0)
				(length 5.08)
				(name "NC")
				(number "33")
			)
			(pin input line
				(at -21.59 -8.89 0)
				(length 5.08)
				(name "CKE")
				(number "34")
			)
			(pin input line
				(at -21.59 -6.35 0)
				(length 5.08)
				(name "CLK")
				(number "35")
			)
			(pin input line
				(at 21.59 -19.05 180)
				(length 5.08)
				(name "_UDQM")
				(number "36")
			)
			(pin no_connect line
				(at -21.59 -25.4 0)
				(length 5.08)
				(name "NC")
				(number "37")
			)
			(pin power_in line
				(at 3.81 34.29 270)
				(length 5.08)
				(name "VDDQ")
				(number "38")
			)
			(pin bidirectional line
				(at 21.59 6.35 180)
				(length 5.08)
				(name "DQ8")
				(number "39")
			)
			(pin power_in line
				(at -1.27 -34.29 90)
				(length 5.08)
				(name "VSSQ")
				(number "4")
			)
			(pin bidirectional line
				(at 21.59 3.81 180)
				(length 5.08)
				(name "DQ9")
				(number "40")
			)
			(pin power_in line
				(at 3.81 -34.29 90)
				(length 5.08)
				(name "VSSQ")
				(number "41")
			)
			(pin bidirectional line
				(at 21.59 1.27 180)
				(length 5.08)
				(name "DQ10")
				(number "42")
			)
			(pin bidirectional line
				(at 21.59 -1.27 180)
				(length 5.08)
				(name "DQ11")
				(number "43")
			)
			(pin power_in line
				(at 6.35 34.29 270)
				(length 5.08)
				(name "VDDQ")
				(number "44")
			)
			(pin bidirectional line
				(at 21.59 -3.81 180)
				(length 5.08)
				(name "DQ12")
				(number "45")
			)
			(pin bidirectional line
				(at 21.59 -6.35 180)
				(length 5.08)
				(name "DQ13")
				(number "46")
			)
			(pin power_in line
				(at 6.35 -34.29 90)
				(length 5.08)
				(name "VSSQ")
				(number "47")
			)
			(pin bidirectional line
				(at 21.59 -8.89 180)
				(length 5.08)
				(name "DQ14")
				(number "48")
			)
			(pin bidirectional line
				(at 21.59 -11.43 180)
				(length 5.08)
				(name "DQ15")
				(number "49")
			)
			(pin bidirectional line
				(at 21.59 21.59 180)
				(length 5.08)
				(name "DQ2")
				(number "5")
			)
			(pin power_in line
				(at -3.81 -34.29 90)
				(length 5.08)
				(name "VSS")
				(number "50")
			)
			(pin bidirectional line
				(at 21.59 19.05 180)
				(length 5.08)
				(name "DQ3")
				(number "6")
			)
			(pin power_in line
				(at -1.27 34.29 270)
				(length 5.08)
				(name "VDDQ")
				(number "7")
			)
			(pin bidirectional line
				(at 21.59 16.51 180)
				(length 5.08)
				(name "DQ4")
				(number "8")
			)
			(pin bidirectional line
				(at 21.59 13.97 180)
				(length 5.08)
				(name "DQ5")
				(number "9")
			)
		)
	)
	(symbol "SN74LVC16T245DLR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 38.1 0)
		)
		(property "Value" "SN74LVC16T245DLR"
			(at 0 35.56 0)
		)
		(property "Footprint" "AmigaPCI:48-BSSOP"
			(at -20.32 29.21 0)
		)
		(property "Datasheet" "SN74LVC16T245DLR"
			(at -20.32 26.67 0)
		)
		(property "Description" ""
			(at -30.48 27.94 0)
		)
		(property "ki_keywords" "SN74LVC16T245DLR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DL48 DL48-M DL48-L"
			(at 0 0 0)
		)
		(symbol "SN74LVC16T245DLR_0_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 7.62)
				(name "1DIR")
				(number "1")
			)
			(pin power_in line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "1B7")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 7.62)
				(name "1B8")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 7.62)
				(name "2B1")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 7.62)
				(name "2B2")
				(number "14")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 7.62)
				(name "GND")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 7.62)
				(name "2B3")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 7.62)
				(name "2B4")
				(number "17")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 7.62)
				(name "VCCB")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 7.62)
				(name "2B5")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 7.62)
				(name "1B1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 7.62)
				(name "2B6")
				(number "20")
			)
			(pin power_in line
				(at -17.78 -22.86 0)
				(length 7.62)
				(name "GND")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 7.62)
				(name "2B7")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 7.62)
				(name "2B8")
				(number "23")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 7.62)
				(name "2DIR")
				(number "24")
			)
			(pin input inverted
				(at 17.78 -30.48 180)
				(length 7.62)
				(name "2OE")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 7.62)
				(name "2A8")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 7.62)
				(name "2A7")
				(number "27")
			)
			(pin power_in line
				(at 17.78 -22.86 180)
				(length 7.62)
				(name "GND")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 7.62)
				(name "2A6")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 7.62)
				(name "1B2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 7.62)
				(name "2A5")
				(number "30")
			)
			(pin power_in line
				(at 17.78 -15.24 180)
				(length 7.62)
				(name "VCCA")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "2A4")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 7.62)
				(name "2A3")
				(number "33")
			)
			(pin power_in line
				(at 17.78 -7.62 180)
				(length 7.62)
				(name "GND")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "2A2")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "2A1")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 7.62)
				(name "1A8")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "1A7")
				(number "38")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at -17.78 20.32 0)
				(length 7.62)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "1A6")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 7.62)
				(name "1A5")
				(number "41")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "VCCA")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 7.62)
				(name "1A4")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 7.62)
				(name "1A3")
				(number "44")
			)
			(pin power_in line
				(at 17.78 20.32 180)
				(length 7.62)
				(name "GND")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 7.62)
				(name "1A2")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 7.62)
				(name "1A1")
				(number "47")
			)
			(pin input inverted
				(at 17.78 27.94 180)
				(length 7.62)
				(name "1OE")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 7.62)
				(name "1B3")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 7.62)
				(name "1B4")
				(number "6")
			)
			(pin power_in line
				(at -17.78 12.7 0)
				(length 7.62)
				(name "VCCB")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 7.62)
				(name "1B5")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 7.62)
				(name "1B6")
				(number "9")
			)
		)
		(symbol "SN74LVC16T245DLR_1_1")
	)
	(symbol "SODIMM 144 AMP 390113-1"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CN"
			(at 3.81 63.5 0)
		)
		(property "Value" "SODIMM 144 AMP 390113-1"
			(at -5.08 52.07 0)
		)
		(property "Footprint" "SODIMM 144 AMP 3-390113-1_TYC"
			(at -5.08 52.07 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=114-1114&DocType=Specification%20Or%20Standard&DocLang=English&DocFormat=pdf&PartCntxt=390113-1"
			(at -5.08 52.07 0)
		)
		(property "Description" ""
			(at -5.08 52.07 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "SODIMM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CONN_3-390113-1_TYC"
			(at 0 0 0)
		)
		(symbol "SODIMM 144 AMP 390113-1_1_1"
			(pin power_in line
				(at -5.08 57.15 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at -5.08 34.29 0)
				(length 5.08)
				(name "DQ35")
				(number "10")
			)
			(pin power_in line
				(at -5.08 31.75 0)
				(length 5.08)
				(name "Vcc")
				(number "11")
			)
			(pin power_in line
				(at -5.08 29.21 0)
				(length 5.08)
				(name "Vcc")
				(number "12")
			)
			(pin bidirectional line
				(at -5.08 26.67 0)
				(length 5.08)
				(name "DQ4")
				(number "13")
			)
			(pin bidirectional line
				(at -5.08 24.13 0)
				(length 5.08)
				(name "DQ36")
				(number "14")
			)
			(pin bidirectional line
				(at -5.08 21.59 0)
				(length 5.08)
				(name "DQ5")
				(number "15")
			)
			(pin bidirectional line
				(at -5.08 19.05 0)
				(length 5.08)
				(name "DQ37")
				(number "16")
			)
			(pin bidirectional line
				(at -5.08 16.51 0)
				(length 5.08)
				(name "DQ6")
				(number "17")
			)
			(pin bidirectional line
				(at -5.08 13.97 0)
				(length 5.08)
				(name "DQ38")
				(number "18")
			)
			(pin bidirectional line
				(at -5.08 11.43 0)
				(length 5.08)
				(name "DQ7")
				(number "19")
			)
			(pin power_in line
				(at -5.08 54.61 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -5.08 8.89 0)
				(length 5.08)
				(name "DQ39")
				(number "20")
			)
			(pin power_in line
				(at -5.08 6.35 0)
				(length 5.08)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at -5.08 3.81 0)
				(length 5.08)
				(name "GND")
				(number "22")
			)
			(pin input line
				(at -5.08 1.27 0)
				(length 5.08)
				(name "DQMB0")
				(number "23")
			)
			(pin input line
				(at -5.08 -1.27 0)
				(length 5.08)
				(name "DQMB4")
				(number "24")
			)
			(pin input line
				(at -5.08 -3.81 0)
				(length 5.08)
				(name "DQMB1")
				(number "25")
			)
			(pin input line
				(at -5.08 -6.35 0)
				(length 5.08)
				(name "DQMB5")
				(number "26")
			)
			(pin power_in line
				(at -5.08 -8.89 0)
				(length 5.08)
				(name "Vcc")
				(number "27")
			)
			(pin power_in line
				(at -5.08 -11.43 0)
				(length 5.08)
				(name "Vcc")
				(number "28")
			)
			(pin input line
				(at -5.08 -13.97 0)
				(length 5.08)
				(name "A0")
				(number "29")
			)
			(pin bidirectional line
				(at -5.08 52.07 0)
				(length 5.08)
				(name "DQ0")
				(number "3")
			)
			(pin input line
				(at -5.08 -16.51 0)
				(length 5.08)
				(name "A3")
				(number "30")
			)
			(pin input line
				(at -5.08 -19.05 0)
				(length 5.08)
				(name "A1")
				(number "31")
			)
			(pin input line
				(at -5.08 -21.59 0)
				(length 5.08)
				(name "A4")
				(number "32")
			)
			(pin input line
				(at -5.08 -24.13 0)
				(length 5.08)
				(name "A2")
				(number "33")
			)
			(pin input line
				(at -5.08 -26.67 0)
				(length 5.08)
				(name "A5")
				(number "34")
			)
			(pin power_in line
				(at -5.08 -29.21 0)
				(length 5.08)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at -5.08 -31.75 0)
				(length 5.08)
				(name "GND")
				(number "36")
			)
			(pin bidirectional line
				(at -5.08 -34.29 0)
				(length 5.08)
				(name "DQ8")
				(number "37")
			)
			(pin bidirectional line
				(at -5.08 -36.83 0)
				(length 5.08)
				(name "DQ40")
				(number "38")
			)
			(pin bidirectional line
				(at -5.08 -39.37 0)
				(length 5.08)
				(name "DQ9")
				(number "39")
			)
			(pin bidirectional line
				(at -5.08 49.53 0)
				(length 5.08)
				(name "DQ32")
				(number "4")
			)
			(pin bidirectional line
				(at -5.08 -41.91 0)
				(length 5.08)
				(name "DQ41")
				(number "40")
			)
			(pin bidirectional line
				(at -5.08 -44.45 0)
				(length 5.08)
				(name "DQ10")
				(number "41")
			)
			(pin bidirectional line
				(at -5.08 -46.99 0)
				(length 5.08)
				(name "DQ42")
				(number "42")
			)
			(pin bidirectional line
				(at -5.08 -49.53 0)
				(length 5.08)
				(name "DQ11")
				(number "43")
			)
			(pin bidirectional line
				(at -5.08 -52.07 0)
				(length 5.08)
				(name "DQ43")
				(number "44")
			)
			(pin power_in line
				(at -5.08 -54.61 0)
				(length 5.08)
				(name "Vcc")
				(number "45")
			)
			(pin power_in line
				(at -5.08 -57.15 0)
				(length 5.08)
				(name "Vcc")
				(number "46")
			)
			(pin bidirectional line
				(at -5.08 -59.69 0)
				(length 5.08)
				(name "DQ12")
				(number "47")
			)
			(pin bidirectional line
				(at -5.08 -62.23 0)
				(length 5.08)
				(name "DQ44")
				(number "48")
			)
			(pin bidirectional line
				(at -5.08 46.99 0)
				(length 5.08)
				(name "DQ1")
				(number "5")
			)
			(pin bidirectional line
				(at -5.08 44.45 0)
				(length 5.08)
				(name "DQ33")
				(number "6")
			)
			(pin bidirectional line
				(at -5.08 41.91 0)
				(length 5.08)
				(name "DQ2")
				(number "7")
			)
			(pin bidirectional line
				(at -5.08 39.37 0)
				(length 5.08)
				(name "DQ34")
				(number "8")
			)
			(pin bidirectional line
				(at -5.08 36.83 0)
				(length 5.08)
				(name "DQ3")
				(number "9")
			)
		)
		(symbol "SODIMM 144 AMP 390113-1_2_1"
			(pin bidirectional line
				(at -5.08 57.15 0)
				(length 5.08)
				(name "DQ13")
				(number "49")
			)
			(pin bidirectional line
				(at -5.08 54.61 0)
				(length 5.08)
				(name "DQ45")
				(number "50")
			)
			(pin bidirectional line
				(at -5.08 52.07 0)
				(length 5.08)
				(name "DQ14")
				(number "51")
			)
			(pin bidirectional line
				(at -5.08 49.53 0)
				(length 5.08)
				(name "DQ46")
				(number "52")
			)
			(pin bidirectional line
				(at -5.08 46.99 0)
				(length 5.08)
				(name "DQ15")
				(number "53")
			)
			(pin bidirectional line
				(at -5.08 44.45 0)
				(length 5.08)
				(name "DQ47")
				(number "54")
			)
			(pin power_in line
				(at -5.08 41.91 0)
				(length 5.08)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at -5.08 39.37 0)
				(length 5.08)
				(name "GND")
				(number "56")
			)
			(pin no_connect line
				(at -5.08 36.83 0)
				(length 5.08)
				(name "NC")
				(number "57")
			)
			(pin no_connect line
				(at -5.08 34.29 0)
				(length 5.08)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at -5.08 31.75 0)
				(length 5.08)
				(name "NC")
				(number "59")
			)
			(pin no_connect line
				(at -5.08 29.21 0)
				(length 5.08)
				(name "NC")
				(number "60")
			)
			(pin power_in line
				(at -5.08 26.67 0)
				(length 5.08)
				(name "CLK0")
				(number "61")
			)
			(pin input line
				(at -5.08 24.13 0)
				(length 5.08)
				(name "CKE0")
				(number "62")
			)
			(pin power_in line
				(at -5.08 21.59 0)
				(length 5.08)
				(name "Vcc")
				(number "63")
			)
			(pin power_in line
				(at -5.08 19.05 0)
				(length 5.08)
				(name "Vcc")
				(number "64")
			)
			(pin input line
				(at -5.08 16.51 0)
				(length 5.08)
				(name "_RAS")
				(number "65")
			)
			(pin input line
				(at -5.08 13.97 0)
				(length 5.08)
				(name "_CAS")
				(number "66")
			)
			(pin input line
				(at -5.08 11.43 0)
				(length 5.08)
				(name "_WE")
				(number "67")
			)
			(pin input line
				(at -5.08 8.89 0)
				(length 5.08)
				(name "CLKE1")
				(number "68")
			)
			(pin input line
				(at -5.08 6.35 0)
				(length 5.08)
				(name "_CS0")
				(number "69")
			)
			(pin input line
				(at -5.08 3.81 0)
				(length 5.08)
				(name "A12")
				(number "70")
			)
			(pin input line
				(at -5.08 1.27 0)
				(length 5.08)
				(name "_CS1")
				(number "71")
			)
			(pin input line
				(at -5.08 -1.27 0)
				(length 5.08)
				(name "A13")
				(number "72")
			)
			(pin no_connect line
				(at -5.08 -3.81 0)
				(length 5.08)
				(name "NC")
				(number "73")
			)
			(pin bidirectional line
				(at -5.08 -6.35 0)
				(length 5.08)
				(name "CLK1")
				(number "74")
			)
			(pin power_in line
				(at -5.08 -8.89 0)
				(length 5.08)
				(name "GND")
				(number "75")
			)
			(pin power_in line
				(at -5.08 -11.43 0)
				(length 5.08)
				(name "GND")
				(number "76")
			)
			(pin no_connect line
				(at -5.08 -13.97 0)
				(length 5.08)
				(name "NC")
				(number "77")
			)
			(pin no_connect line
				(at -5.08 -16.51 0)
				(length 5.08)
				(name "NC")
				(number "78")
			)
			(pin no_connect line
				(at -5.08 -19.05 0)
				(length 5.08)
				(name "NC")
				(number "79")
			)
			(pin no_connect line
				(at -5.08 -21.59 0)
				(length 5.08)
				(name "NC")
				(number "80")
			)
			(pin power_in line
				(at -5.08 -24.13 0)
				(length 5.08)
				(name "Vcc")
				(number "81")
			)
			(pin power_in line
				(at -5.08 -26.67 0)
				(length 5.08)
				(name "Vcc")
				(number "82")
			)
			(pin bidirectional line
				(at -5.08 -29.21 0)
				(length 5.08)
				(name "DQ16")
				(number "83")
			)
			(pin bidirectional line
				(at -5.08 -31.75 0)
				(length 5.08)
				(name "DQ48")
				(number "84")
			)
			(pin bidirectional line
				(at -5.08 -34.29 0)
				(length 5.08)
				(name "DQ17")
				(number "85")
			)
			(pin bidirectional line
				(at -5.08 -36.83 0)
				(length 5.08)
				(name "DQ49")
				(number "86")
			)
			(pin bidirectional line
				(at -5.08 -39.37 0)
				(length 5.08)
				(name "DQ18")
				(number "87")
			)
			(pin bidirectional line
				(at -5.08 -41.91 0)
				(length 5.08)
				(name "DQ50")
				(number "88")
			)
			(pin bidirectional line
				(at -5.08 -44.45 0)
				(length 5.08)
				(name "DQ19")
				(number "89")
			)
			(pin bidirectional line
				(at -5.08 -46.99 0)
				(length 5.08)
				(name "DQ51")
				(number "90")
			)
			(pin power_in line
				(at -5.08 -49.53 0)
				(length 5.08)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at -5.08 -52.07 0)
				(length 5.08)
				(name "GND")
				(number "92")
			)
			(pin bidirectional line
				(at -5.08 -54.61 0)
				(length 5.08)
				(name "DQ20")
				(number "93")
			)
			(pin bidirectional line
				(at -5.08 -57.15 0)
				(length 5.08)
				(name "DQ52")
				(number "94")
			)
			(pin bidirectional line
				(at -5.08 -59.69 0)
				(length 5.08)
				(name "DQ21")
				(number "95")
			)
			(pin bidirectional line
				(at -5.08 -62.23 0)
				(length 5.08)
				(name "DQ53")
				(number "96")
			)
		)
		(symbol "SODIMM 144 AMP 390113-1_3_1"
			(pin bidirectional line
				(at -5.08 49.53 0)
				(length 5.08)
				(name "DQ55")
				(number "100")
			)
			(pin power_in line
				(at -5.08 46.99 0)
				(length 5.08)
				(name "Vcc")
				(number "101")
			)
			(pin power_in line
				(at -5.08 44.45 0)
				(length 5.08)
				(name "Vcc")
				(number "102")
			)
			(pin input line
				(at -5.08 41.91 0)
				(length 5.08)
				(name "A6")
				(number "103")
			)
			(pin input line
				(at -5.08 39.37 0)
				(length 5.08)
				(name "A7")
				(number "104")
			)
			(pin input line
				(at -5.08 36.83 0)
				(length 5.08)
				(name "A8")
				(number "105")
			)
			(pin input line
				(at -5.08 34.29 0)
				(length 5.08)
				(name "BA0")
				(number "106")
			)
			(pin power_in line
				(at -5.08 31.75 0)
				(length 5.08)
				(name "GND")
				(number "107")
			)
			(pin power_in line
				(at -5.08 29.21 0)
				(length 5.08)
				(name "Vcc")
				(number "108")
			)
			(pin input line
				(at -5.08 26.67 0)
				(length 5.08)
				(name "A9")
				(number "109")
			)
			(pin input line
				(at -5.08 24.13 0)
				(length 5.08)
				(name "BA1")
				(number "110")
			)
			(pin input line
				(at -5.08 21.59 0)
				(length 5.08)
				(name "A10")
				(number "111")
			)
			(pin input line
				(at -5.08 19.05 0)
				(length 5.08)
				(name "A11")
				(number "112")
			)
			(pin power_in line
				(at -5.08 16.51 0)
				(length 5.08)
				(name "Vcc")
				(number "113")
			)
			(pin power_in line
				(at -5.08 13.97 0)
				(length 5.08)
				(name "Vcc")
				(number "114")
			)
			(pin input line
				(at -5.08 11.43 0)
				(length 5.08)
				(name "DQMB2")
				(number "115")
			)
			(pin input line
				(at -5.08 8.89 0)
				(length 5.08)
				(name "DQMB6")
				(number "116")
			)
			(pin input line
				(at -5.08 6.35 0)
				(length 5.08)
				(name "DQMB3")
				(number "117")
			)
			(pin input line
				(at -5.08 3.81 0)
				(length 5.08)
				(name "DQMB7")
				(number "118")
			)
			(pin power_in line
				(at -5.08 1.27 0)
				(length 5.08)
				(name "GND")
				(number "119")
			)
			(pin power_in line
				(at -5.08 -1.27 0)
				(length 5.08)
				(name "GND")
				(number "120")
			)
			(pin bidirectional line
				(at -5.08 -3.81 0)
				(length 5.08)
				(name "DQ24")
				(number "121")
			)
			(pin bidirectional line
				(at -5.08 -6.35 0)
				(length 5.08)
				(name "DQ56")
				(number "122")
			)
			(pin bidirectional line
				(at -5.08 -8.89 0)
				(length 5.08)
				(name "DQ25")
				(number "123")
			)
			(pin bidirectional line
				(at -5.08 -11.43 0)
				(length 5.08)
				(name "DQ57")
				(number "124")
			)
			(pin bidirectional line
				(at -5.08 -13.97 0)
				(length 5.08)
				(name "DQ26")
				(number "125")
			)
			(pin bidirectional line
				(at -5.08 -16.51 0)
				(length 5.08)
				(name "DQ58")
				(number "126")
			)
			(pin bidirectional line
				(at -5.08 -19.05 0)
				(length 5.08)
				(name "DQ27")
				(number "127")
			)
			(pin bidirectional line
				(at -5.08 -21.59 0)
				(length 5.08)
				(name "DQ59")
				(number "128")
			)
			(pin power_in line
				(at -5.08 -24.13 0)
				(length 5.08)
				(name "Vcc")
				(number "129")
			)
			(pin power_in line
				(at -5.08 -26.67 0)
				(length 5.08)
				(name "Vcc")
				(number "130")
			)
			(pin bidirectional line
				(at -5.08 -29.21 0)
				(length 5.08)
				(name "DQ28")
				(number "131")
			)
			(pin bidirectional line
				(at -5.08 -31.75 0)
				(length 5.08)
				(name "DQ60")
				(number "132")
			)
			(pin bidirectional line
				(at -5.08 -34.29 0)
				(length 5.08)
				(name "DQ29")
				(number "133")
			)
			(pin bidirectional line
				(at -5.08 -36.83 0)
				(length 5.08)
				(name "DQ61")
				(number "134")
			)
			(pin bidirectional line
				(at -5.08 -39.37 0)
				(length 5.08)
				(name "DQ30")
				(number "135")
			)
			(pin bidirectional line
				(at -5.08 -41.91 0)
				(length 5.08)
				(name "DQ62")
				(number "136")
			)
			(pin bidirectional line
				(at -5.08 -44.45 0)
				(length 5.08)
				(name "DQ31")
				(number "137")
			)
			(pin bidirectional line
				(at -5.08 -46.99 0)
				(length 5.08)
				(name "DQ63")
				(number "138")
			)
			(pin power_in line
				(at -5.08 -49.53 0)
				(length 5.08)
				(name "GND")
				(number "139")
			)
			(pin power_in line
				(at -5.08 -52.07 0)
				(length 5.08)
				(name "GND")
				(number "140")
			)
			(pin bidirectional line
				(at -5.08 -54.61 0)
				(length 5.08)
				(name "SDA")
				(number "141")
			)
			(pin bidirectional line
				(at -5.08 -57.15 0)
				(length 5.08)
				(name "SCL")
				(number "142")
			)
			(pin power_in line
				(at -5.08 -59.69 0)
				(length 5.08)
				(name "Vcc")
				(number "143")
			)
			(pin power_in line
				(at -5.08 -62.23 0)
				(length 5.08)
				(name "Vcc")
				(number "144")
			)
			(pin bidirectional line
				(at -5.08 57.15 0)
				(length 5.08)
				(name "DQ22")
				(number "97")
			)
			(pin bidirectional line
				(at -5.08 54.61 0)
				(length 5.08)
				(name "DQ54")
				(number "98")
			)
			(pin bidirectional line
				(at -5.08 52.07 0)
				(length 5.08)
				(name "DQ23")
				(number "99")
			)
		)
	)
)
