(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ICE40HX1K-VQ100" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -20.3319 69.3826 0))
    (property "Value" "ICE40HX1K-VQ100" (id 1) (at -20.3264 -114.3223 0))
    (property "Footprint" "ICE40HX1K-VQ100:QFP50P1600X1600X120-100N" (id 2) (at 0 0 0))
    (property "PARTREV" "3.4" (id 4) (at 0 0 0))
    (property "STANDARD" "IPC 7351B" (id 5) (at 0 0 0))
    (property "MANUFACTURER" "LATTICE SEMICONDUCTOR" (id 6) (at 0 0 0))
    (property "PACKAGE" "QFP-100" (id 7) (at 0 0 0))
    (symbol "ICE40HX1K-VQ100_0_0"
      (pin bidirectional line (at 25.4 -30.48 180.0) (length 5.08)
        (name "IOT_73")
        (number "78")
      )
      (pin bidirectional line (at 25.4 -27.94 180.0) (length 5.08)
        (name "IOT_74")
        (number "79")
      )
      (pin bidirectional line (at 25.4 -25.4 180.0) (length 5.08)
        (name "IOT_75")
        (number "80")
      )
      (pin bidirectional line (at 25.4 15.24 180.0) (length 5.08)
        (name "IOT_95")
        (number "100")
      )
      (pin bidirectional line (at 25.4 -22.86 180.0) (length 5.08)
        (name "IOT_77")
        (number "81")
      )
      (pin bidirectional line (at 25.4 -20.32 180.0) (length 5.08)
        (name "IOT_78")
        (number "82")
      )
      (pin bidirectional line (at 25.4 -17.78 180.0) (length 5.08)
        (name "IOT_79")
        (number "83")
      )
      (pin bidirectional line (at 25.4 -15.24 180.0) (length 5.08)
        (name "IOT_80")
        (number "85")
      )
      (pin bidirectional line (at 25.4 -12.7 180.0) (length 5.08)
        (name "IOT_81")
        (number "86")
      )
      (pin bidirectional line (at 25.4 -10.16 180.0) (length 5.08)
        (name "IOT_82")
        (number "87")
      )
      (pin bidirectional line (at 25.4 -7.62 180.0) (length 5.08)
        (name "IOT_84_GBIN1")
        (number "89")
      )
      (pin bidirectional line (at 25.4 -5.08 180.0) (length 5.08)
        (name "IOT_85_GBIN0")
        (number "90")
      )
      (pin bidirectional line (at 25.4 -2.54 180.0) (length 5.08)
        (name "IOT_86")
        (number "91")
      )
      (pin bidirectional line (at 25.4 0.0 180.0) (length 5.08)
        (name "IOT_87")
        (number "93")
      )
      (pin bidirectional line (at 25.4 2.54 180.0) (length 5.08)
        (name "IOT_88")
        (number "94")
      )
      (pin bidirectional line (at 25.4 5.08 180.0) (length 5.08)
        (name "IOT_89")
        (number "95")
      )
      (pin bidirectional line (at 25.4 7.62 180.0) (length 5.08)
        (name "IOT_90")
        (number "96")
      )
      (pin bidirectional line (at 25.4 10.16 180.0) (length 5.08)
        (name "IOT_91")
        (number "97")
      )
      (pin bidirectional line (at 25.4 12.7 180.0) (length 5.08)
        (name "IOT_93")
        (number "99")
      )
      (pin bidirectional line (at 25.4 -81.28 180.0) (length 5.08)
        (name "IOR_52")
        (number "51")
      )
      (pin bidirectional line (at 25.4 -78.74 180.0) (length 5.08)
        (name "IOR_53")
        (number "52")
      )
      (pin bidirectional line (at 25.4 -76.2 180.0) (length 5.08)
        (name "IOR_54")
        (number "53")
      )
      (pin bidirectional line (at 25.4 -35.56 180.0) (length 5.08)
        (name "IOR_72")
        (number "74")
      )
      (pin bidirectional line (at 25.4 -73.66 180.0) (length 5.08)
        (name "IOR_55")
        (number "54")
      )
      (pin bidirectional line (at 25.4 -71.12 180.0) (length 5.08)
        (name "IOR_56")
        (number "56")
      )
      (pin bidirectional line (at 25.4 -68.58 180.0) (length 5.08)
        (name "IOR_57")
        (number "57")
      )
      (pin bidirectional line (at 25.4 -66.04 180.0) (length 5.08)
        (name "IOR_58")
        (number "59")
      )
      (pin bidirectional line (at 25.4 -63.5 180.0) (length 5.08)
        (name "IOR_59")
        (number "60")
      )
      (pin bidirectional line (at 25.4 -60.96 180.0) (length 5.08)
        (name "IOR_60_GBIN3")
        (number "62")
      )
      (pin bidirectional line (at 25.4 -58.42 180.0) (length 5.08)
        (name "IOR_61_GBIN2")
        (number "63")
      )
      (pin bidirectional line (at 25.4 -55.88 180.0) (length 5.08)
        (name "IOR_63")
        (number "64")
      )
      (pin bidirectional line (at 25.4 -53.34 180.0) (length 5.08)
        (name "IOR_64")
        (number "65")
      )
      (pin bidirectional line (at 25.4 -50.8 180.0) (length 5.08)
        (name "IOR_65")
        (number "66")
      )
      (pin bidirectional line (at 25.4 -48.26 180.0) (length 5.08)
        (name "IOR_67")
        (number "68")
      )
      (pin bidirectional line (at 25.4 -45.72 180.0) (length 5.08)
        (name "IOR_68")
        (number "69")
      )
      (pin bidirectional line (at 25.4 -43.18 180.0) (length 5.08)
        (name "IOR_69")
        (number "71")
      )
      (pin bidirectional line (at 25.4 -40.64 180.0) (length 5.08)
        (name "IOR_70")
        (number "72")
      )
      (pin bidirectional line (at 25.4 -38.1 180.0) (length 5.08)
        (name "IOR_71")
        (number "73")
      )
      (pin bidirectional line (at -25.4 -15.24 0) (length 5.08)
        (name "IOB_26")
        (number "26")
      )
      (pin bidirectional line (at -25.4 -17.78 0) (length 5.08)
        (name "IOB_27")
        (number "27")
      )
      (pin bidirectional line (at -25.4 -20.32 0) (length 5.08)
        (name "IOB_28")
        (number "28")
      )
      (pin bidirectional line (at -25.4 -22.86 0) (length 5.08)
        (name "IOB_29")
        (number "29")
      )
      (pin bidirectional line (at -25.4 -25.4 0) (length 5.08)
        (name "IOB_30")
        (number "30")
      )
      (pin bidirectional line (at -25.4 -27.94 0) (length 5.08)
        (name "IOB_34")
        (number "36")
      )
      (pin bidirectional line (at -25.4 -30.48 0) (length 5.08)
        (name "IOB_35_GBIN5")
        (number "33")
      )
      (pin bidirectional line (at -25.4 -33.02 0) (length 5.08)
        (name "IOB_36_GBIN4")
        (number "34")
      )
      (pin bidirectional line (at -25.4 -35.56 0) (length 5.08)
        (name "IOB_37")
        (number "37")
      )
      (pin bidirectional line (at -25.4 -38.1 0) (length 5.08)
        (name "IOB_41")
        (number "40")
      )
      (pin bidirectional line (at -25.4 -40.64 0) (length 5.08)
        (name "IOB_42_CBSEL0")
        (number "41")
      )
      (pin bidirectional line (at -25.4 -43.18 0) (length 5.08)
        (name "IOB_43_CBSEL1")
        (number "42")
      )
      (pin bidirectional line (at -25.4 -45.72 0) (length 5.08)
        (name "IOB_44_SDO")
        (number "45")
      )
      (pin bidirectional line (at -25.4 -48.26 0) (length 5.08)
        (name "IOB_45_SDI")
        (number "46")
      )
      (pin bidirectional line (at -25.4 -50.8 0) (length 5.08)
        (name "IOB_46_SCK")
        (number "48")
      )
      (pin bidirectional line (at -25.4 -53.34 0) (length 5.08)
        (name "IOB_47_SS")
        (number "49")
      )
      (pin input line (at -25.4 43.18 0) (length 5.08)
        (name "CDONE")
        (number "43")
      )
      (pin input line (at -25.4 40.64 0) (length 5.08)
        (name "CRESET_B")
        (number "44")
      )
      (pin bidirectional line (at -25.4 33.02 0) (length 5.08)
        (name "IOL_1B")
        (number "2")
      )
      (pin bidirectional line (at -25.4 27.94 0) (length 5.08)
        (name "IOL_2B")
        (number "4")
      )
      (pin bidirectional line (at -25.4 22.86 0) (length 5.08)
        (name "IOL_3B")
        (number "8")
      )
      (pin bidirectional line (at -25.4 17.78 0) (length 5.08)
        (name "IOL_5B")
        (number "10")
      )
      (pin bidirectional line (at -25.4 7.62 0) (length 5.08)
        (name "IOL_7B")
        (number "16")
      )
      (pin bidirectional line (at -25.4 5.08 0) (length 5.08)
        (name "IOL_8B")
        (number "19")
      )
      (pin bidirectional line (at -25.4 -2.54 0) (length 5.08)
        (name "IOL_10B")
        (number "21")
      )
      (pin bidirectional line (at -25.4 -7.62 0) (length 5.08)
        (name "IOL_12B")
        (number "25")
      )
      (pin bidirectional line (at -25.4 35.56 0) (length 5.08)
        (name "IOL_1A")
        (number "1")
      )
      (pin bidirectional line (at -25.4 30.48 0) (length 5.08)
        (name "IOL_2A")
        (number "3")
      )
      (pin bidirectional line (at -25.4 25.4 0) (length 5.08)
        (name "IOL_3A")
        (number "7")
      )
      (pin bidirectional line (at -25.4 20.32 0) (length 5.08)
        (name "IOL_5A")
        (number "9")
      )
      (pin bidirectional line (at -25.4 10.16 0) (length 5.08)
        (name "IOL_7A_GBIN6")
        (number "15")
      )
      (pin bidirectional line (at -25.4 2.54 0) (length 5.08)
        (name "IOL_8A")
        (number "18")
      )
      (pin bidirectional line (at -25.4 0.0 0) (length 5.08)
        (name "IOL_10A")
        (number "20")
      )
      (pin bidirectional line (at -25.4 -5.08 0) (length 5.08)
        (name "IOL_12A")
        (number "24")
      )
      (pin bidirectional line (at -25.4 15.24 0) (length 5.08)
        (name "IOL_6B_GBIN7")
        (number "13")
      )
      (pin bidirectional line (at -25.4 12.7 0) (length 5.08)
        (name "IOL_6A")
        (number "12")
      )
      (pin power_in line (at 25.4 27.94 180.0) (length 5.08)
        (name "VCC_SPI")
        (number "50")
      )
      (pin power_in line (at 25.4 30.48 180.0) (length 5.08)
        (name "VPP_2V5")
        (number "75")
      )
      (pin power_in line (at 25.4 33.02 180.0) (length 5.08)
        (name "VPP_FAST")
        (number "76")
      )
      (pin power_in line (at 25.4 38.1 180.0) (length 5.08)
        (name "VCCIO_0")
        (number "88")
      )
      (pin power_in line (at 25.4 43.18 180.0) (length 5.08)
        (name "VCCIO_1")
        (number "58")
      )
      (pin power_in line (at 25.4 48.26 180.0) (length 5.08)
        (name "VCCIO_2")
        (number "31")
      )
      (pin power_in line (at 25.4 55.88 180.0) (length 5.08)
        (name "VCCIO_3")
        (number "6")
      )
      (pin power_in line (at 25.4 66.04 180.0) (length 5.08)
        (name "VCC")
        (number "11")
      )
      (pin power_in line (at 25.4 -86.36 180.0) (length 5.08)
        (name "GND")
        (number "5")
      )
      (pin power_in line (at 25.4 63.5 180.0) (length 5.08)
        (name "VCC__1")
        (number "35")
      )
      (pin power_in line (at 25.4 60.96 180.0) (length 5.08)
        (name "VCC__2")
        (number "61")
      )
      (pin power_in line (at 25.4 58.42 180.0) (length 5.08)
        (name "VCC__3")
        (number "77")
      )
      (pin power_in line (at 25.4 53.34 180.0) (length 5.08)
        (name "VCCIO_3__1")
        (number "14")
      )
      (pin power_in line (at 25.4 50.8 180.0) (length 5.08)
        (name "VCCIO_3__2")
        (number "22")
      )
      (pin power_in line (at 25.4 45.72 180.0) (length 5.08)
        (name "VCCIO_2__1")
        (number "38")
      )
      (pin power_in line (at 25.4 40.64 180.0) (length 5.08)
        (name "VCCIO_1__1")
        (number "67")
      )
      (pin power_in line (at 25.4 35.56 180.0) (length 5.08)
        (name "VCCIO_0__1")
        (number "92")
      )
      (pin power_in line (at 25.4 -88.9 180.0) (length 5.08)
        (name "GND__1")
        (number "17")
      )
      (pin power_in line (at 25.4 -91.44 180.0) (length 5.08)
        (name "GND__2")
        (number "23")
      )
      (pin power_in line (at 25.4 -93.98 180.0) (length 5.08)
        (name "GND__3")
        (number "32")
      )
      (pin power_in line (at 25.4 -96.52 180.0) (length 5.08)
        (name "GND__4")
        (number "39")
      )
      (pin power_in line (at 25.4 -99.06 180.0) (length 5.08)
        (name "GND__5")
        (number "47")
      )
      (pin power_in line (at 25.4 -101.6 180.0) (length 5.08)
        (name "GND__6")
        (number "55")
      )
      (pin power_in line (at 25.4 -104.14 180.0) (length 5.08)
        (name "GND__7")
        (number "70")
      )
      (pin power_in line (at 25.4 -106.68 180.0) (length 5.08)
        (name "GND__8")
        (number "84")
      )
      (pin power_in line (at 25.4 -109.22 180.0) (length 5.08)
        (name "GND__9")
        (number "98")
      )
    )
  )
)