(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Conn_02x20_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "CN901" (at 1.27 27.94 0))
    (property "Value" "SECONDARY IDE" (at 1.27 26.019 0))
    (property "Footprint" "AmigaPCI:ATA_Header_2x20_P2.54mm" (at 0 0 0))
    (property "Datasheet" "~" (at 0 0 0))
    (property "ki_keywords" "connector" (at 0 0 0))
    (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
    (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0))
    (symbol "Conn_02x20_Odd_Even_1_1"
      (pin passive line (at -5.08 22.86 0) (length 3.81)
        (name "Pin_1")
        (number "1")
      )
      (pin passive line (at 7.62 12.7 180) (length 3.81)
        (name "Pin_10")
        (number "10")
      )
      (pin passive line (at -5.08 10.16 0) (length 3.81)
        (name "Pin_11")
        (number "11")
      )
      (pin passive line (at 7.62 10.16 180) (length 3.81)
        (name "Pin_12")
        (number "12")
      )
      (pin passive line (at -5.08 7.62 0) (length 3.81)
        (name "Pin_13")
        (number "13")
      )
      (pin passive line (at 7.62 7.62 180) (length 3.81)
        (name "Pin_14")
        (number "14")
      )
      (pin passive line (at -5.08 5.08 0) (length 3.81)
        (name "Pin_15")
        (number "15")
      )
      (pin passive line (at 7.62 5.08 180) (length 3.81)
        (name "Pin_16")
        (number "16")
      )
      (pin passive line (at -5.08 2.54 0) (length 3.81)
        (name "Pin_17")
        (number "17")
      )
      (pin passive line (at 7.62 2.54 180) (length 3.81)
        (name "Pin_18")
        (number "18")
      )
      (pin passive line (at -5.08 0 0) (length 3.81)
        (name "Pin_19")
        (number "19")
      )
      (pin passive line (at 7.62 22.86 180) (length 3.81)
        (name "Pin_2")
        (number "2")
      )
      (pin passive line (at -5.08 -2.54 0) (length 3.81)
        (name "Pin_21")
        (number "21")
      )
      (pin passive line (at 7.62 -2.54 180) (length 3.81)
        (name "Pin_22")
        (number "22")
      )
      (pin passive line (at -5.08 -5.08 0) (length 3.81)
        (name "Pin_23")
        (number "23")
      )
      (pin passive line (at 7.62 -5.08 180) (length 3.81)
        (name "Pin_24")
        (number "24")
      )
      (pin passive line (at -5.08 -7.62 0) (length 3.81)
        (name "Pin_25")
        (number "25")
      )
      (pin passive line (at 7.62 -7.62 180) (length 3.81)
        (name "Pin_26")
        (number "26")
      )
      (pin passive line (at -5.08 -10.16 0) (length 3.81)
        (name "Pin_27")
        (number "27")
      )
      (pin passive line (at 7.62 -10.16 180) (length 3.81)
        (name "Pin_28")
        (number "28")
      )
      (pin passive line (at -5.08 -12.7 0) (length 3.81)
        (name "Pin_29")
        (number "29")
      )
      (pin passive line (at -5.08 20.32 0) (length 3.81)
        (name "Pin_3")
        (number "3")
      )
      (pin passive line (at 7.62 -12.7 180) (length 3.81)
        (name "Pin_30")
        (number "30")
      )
      (pin passive line (at -5.08 -15.24 0) (length 3.81)
        (name "Pin_31")
        (number "31")
      )
      (pin passive line (at 7.62 -15.24 180) (length 3.81)
        (name "Pin_32")
        (number "32")
      )
      (pin passive line (at -5.08 -17.78 0) (length 3.81)
        (name "Pin_33")
        (number "33")
      )
      (pin passive line (at 7.62 -17.78 180) (length 3.81)
        (name "Pin_34")
        (number "34")
      )
      (pin passive line (at -5.08 -20.32 0) (length 3.81)
        (name "Pin_35")
        (number "35")
      )
      (pin passive line (at 7.62 -20.32 180) (length 3.81)
        (name "Pin_36")
        (number "36")
      )
      (pin passive line (at -5.08 -22.86 0) (length 3.81)
        (name "Pin_37")
        (number "37")
      )
      (pin passive line (at 7.62 -22.86 180) (length 3.81)
        (name "Pin_38")
        (number "38")
      )
      (pin passive line (at -5.08 -25.4 0) (length 3.81)
        (name "Pin_39")
        (number "39")
      )
      (pin passive line (at 7.62 20.32 180) (length 3.81)
        (name "Pin_4")
        (number "4")
      )
      (pin passive line (at 7.62 -25.4 180) (length 3.81)
        (name "Pin_40")
        (number "40")
      )
      (pin passive line (at -5.08 17.78 0) (length 3.81)
        (name "Pin_5")
        (number "5")
      )
      (pin passive line (at 7.62 17.78 180) (length 3.81)
        (name "Pin_6")
        (number "6")
      )
      (pin passive line (at -5.08 15.24 0) (length 3.81)
        (name "Pin_7")
        (number "7")
      )
      (pin passive line (at 7.62 15.24 180) (length 3.81)
        (name "Pin_8")
        (number "8")
      )
      (pin passive line (at -5.08 12.7 0) (length 3.81)
        (name "Pin_9")
        (number "9")
      )
    )
  )
)
