(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Paula" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U500" (at -0.635 -69.1642 0))
    (property "Value" "PAULA" (at -0.635 -71.4756 0))
    (property "Footprint" "Package_DIP:DIP-48_W15.24mm" (at 3.81 0 0))
    (property "Datasheet" "" (at 3.81 0 0))
    (symbol "Paula_0_1")
    (symbol "Paula_1_1"
      (pin passive line (at -16.51 33.02 0) (length 5.08)
        (name "DRD8")
        (number "1")
      )
      (pin passive line (at -16.51 12.7 0) (length 5.08)
        (name "DRD0")
        (number "10")
      )
      (pin passive line (at -16.51 -64.77 0) (length 5.08)
        (name "_RESET")
        (number "11")
      )
      (pin passive line (at -16.51 -45.72 0) (length 5.08)
        (name "DMAL")
        (number "12")
      )
      (pin passive inverted (at -16.51 -33.02 0) (length 5.08)
        (name "_IPL0")
        (number "13")
      )
      (pin passive inverted (at -16.51 -30.48 0) (length 5.08)
        (name "_IPL1")
        (number "14")
      )
      (pin passive inverted (at -16.51 -27.94 0) (length 5.08)
        (name "_IPL2")
        (number "15")
      )
      (pin passive inverted (at 15.24 5.08 180) (length 5.08)
        (name "_INT2")
        (number "16")
      )
      (pin passive inverted (at 15.24 10.16 180) (length 5.08)
        (name "_INT3")
        (number "17")
      )
      (pin passive inverted (at 15.24 15.24 180) (length 5.08)
        (name "_INT6")
        (number "18")
      )
      (pin passive line (at -16.51 0 0) (length 5.08)
        (name "RGA8")
        (number "19")
      )
      (pin passive line (at -16.51 30.48 0) (length 5.08)
        (name "DRD7")
        (number "2")
      )
      (pin passive line (at -16.51 -2.54 0) (length 5.08)
        (name "RGA7")
        (number "20")
      )
      (pin passive line (at -16.51 -5.08 0) (length 5.08)
        (name "RGA6")
        (number "21")
      )
      (pin passive line (at -16.51 -7.62 0) (length 5.08)
        (name "RGA5")
        (number "22")
      )
      (pin passive line (at -16.51 -10.16 0) (length 5.08)
        (name "RGA4")
        (number "23")
      )
      (pin passive line (at -16.51 -12.7 0) (length 5.08)
        (name "RGA3")
        (number "24")
      )
      (pin passive line (at -16.51 -15.24 0) (length 5.08)
        (name "RGA2")
        (number "25")
      )
      (pin passive line (at -16.51 -17.78 0) (length 5.08)
        (name "RGA1")
        (number "26")
      )
      (pin passive line (at -6.35 63.5 270) (length 5.08)
        (name "VCC")
        (number "27")
      )
      (pin passive line (at -16.51 -53.34 0) (length 5.08)
        (name "CCK")
        (number "28")
      )
      (pin passive line (at -16.51 -58.42 0) (length 5.08)
        (name "CCKQ")
        (number "29")
      )
      (pin passive line (at -16.51 27.94 0) (length 5.08)
        (name "DRD6")
        (number "3")
      )
      (pin passive line (at 15.24 -22.86 180) (length 5.08)
        (name "RIGHT")
        (number "30")
      )
      (pin passive line (at 15.24 -11.43 180) (length 5.08)
        (name "LEFT")
        (number "31")
      )
      (pin passive line (at 15.24 -35.56 180) (length 5.08)
        (name "P0X")
        (number "32")
      )
      (pin passive line (at 15.24 -40.64 180) (length 5.08)
        (name "P0Y")
        (number "33")
      )
      (pin passive line (at 15.24 -64.77 180) (length 5.08)
        (name "A_GND")
        (number "34")
      )
      (pin passive line (at 15.24 -45.72 180) (length 5.08)
        (name "P1X")
        (number "35")
      )
      (pin passive line (at 15.24 -50.8 180) (length 5.08)
        (name "P1Y")
        (number "36")
      )
      (pin passive inverted (at 15.24 50.8 180) (length 5.08)
        (name "_DKRD")
        (number "37")
      )
      (pin passive inverted (at 15.24 45.72 180) (length 5.08)
        (name "_DKWD")
        (number "38")
      )
      (pin passive line (at 15.24 40.64 180) (length 5.08)
        (name "DKWE")
        (number "39")
      )
      (pin passive line (at -16.51 25.4 0) (length 5.08)
        (name "DRD5")
        (number "4")
      )
      (pin passive inverted (at 15.24 25.4 180) (length 5.08)
        (name "_TXD")
        (number "40")
      )
      (pin passive inverted (at 15.24 30.48 180) (length 5.08)
        (name "_RxD")
        (number "41")
      )
      (pin passive line (at -16.51 50.8 0) (length 5.08)
        (name "DRD15")
        (number "42")
      )
      (pin passive line (at -16.51 48.26 0) (length 5.08)
        (name "DRD14")
        (number "43")
      )
      (pin passive line (at -16.51 45.72 0) (length 5.08)
        (name "DRD13")
        (number "44")
      )
      (pin passive line (at -16.51 43.18 0) (length 5.08)
        (name "DRD12")
        (number "45")
      )
      (pin passive line (at -16.51 40.64 0) (length 5.08)
        (name "DRD11")
        (number "46")
      )
      (pin passive line (at -16.51 38.1 0) (length 5.08)
        (name "DRD10")
        (number "47")
      )
      (pin passive line (at -16.51 35.56 0) (length 5.08)
        (name "DRD9")
        (number "48")
      )
      (pin passive line (at -16.51 22.86 0) (length 5.08)
        (name "DRD4")
        (number "5")
      )
      (pin passive line (at -16.51 20.32 0) (length 5.08)
        (name "DRD3")
        (number "6")
      )
      (pin passive line (at -16.51 17.78 0) (length 5.08)
        (name "DRD2")
        (number "7")
      )
      (pin passive line (at 5.08 63.5 270) (length 5.08)
        (name "GND")
        (number "8")
      )
      (pin passive line (at -16.51 15.24 0) (length 5.08)
        (name "DRD1")
        (number "9")
      )
    )
  )
)
