(footprint "DL48" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "SN74LVC16T245DLR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value DL48 (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -5.0292 -8.8011) (layer F.SilkS))
  (fp_text user "*" (at -3.4163 -7.9248) (layer F.Fab))
  (fp_text user "*" (at -5.0292 -8.8011 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at -3.4163 -7.9248 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -4.7752 -7.3025) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -4.7752 -6.6675) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -4.7752 -6.0325) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -4.7752 -5.3975) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -4.7752 -4.7625) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -4.7752 -4.1275) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -4.7752 -3.4925) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -4.7752 -2.8575) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -4.7752 -2.2225) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -4.7752 -1.5875) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -4.7752 -0.9525) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -4.7752 -0.3175) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -4.7752 0.3175) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -4.7752 0.9525) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -4.7752 1.5875) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -4.7752 2.2225) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at -4.7752 2.8575) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at -4.7752 3.4925) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at -4.7752 4.1275) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at -4.7752 4.7625) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at -4.7752 5.3975) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at -4.7752 6.0325) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at -4.7752 6.6675) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at -4.7752 7.3025) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 4.7752 7.3025) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 4.7752 6.6675) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 4.7752 6.0325) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 4.7752 5.3975) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 4.7752 4.7625) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 4.7752 4.1275) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 4.7752 3.4925) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 4.7752 2.8575) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 4.7752 2.2225) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 4.7752 1.5875) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 4.7752 0.9525) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 4.7752 0.3175) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at 4.7752 -0.3175) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at 4.7752 -0.9525) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at 4.7752 -1.5875) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at 4.7752 -2.2225) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at 4.7752 -2.8575) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "42" smd rect (at 4.7752 -3.4925) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "43" smd rect (at 4.7752 -4.1275) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "44" smd rect (at 4.7752 -4.7625) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "45" smd rect (at 4.7752 -5.3975) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "46" smd rect (at 4.7752 -6.0325) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "47" smd rect (at 4.7752 -6.6675) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "48" smd rect (at 4.7752 -7.3025) (size 1.4224 0.3556) (layers "F.Cu" "F.Paste" "F.Mask"))
)
