(footprint "C_ARRAY_0612x4 (1632)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Capacitor Array 0612x4 (1632)")
  (attr smd)
  (fp_text reference "CN" (at 0 -2.92 unlocked) (layer "F.SilkS"))
  (fp_text value "C_ARRAY_0612x4 (1632)" (at 0 0 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -0.81 -1.2) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "2" smd rect (at -0.81 -0.4) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "3" smd rect (at -0.81 0.4) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "4" smd rect (at -0.81 1.2) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "5" smd rect (at 0.79 1.2) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "6" smd rect (at 0.79 0.4) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "7" smd rect (at 0.79 -0.4) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "8" smd rect (at 0.79 -1.2) (size 0.6 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
)
