(footprint "Floppy_PinHeader_2x17_P2.54mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 2x17, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x17 2.54mm double row")
  (property "Sheetfile" "floppy.kicad_sch")
  (property "Sheetname" "Floppy and Parallel")
  (property "ki_description" "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (clearance 0.15)
  (attr through_hole)
  (fp_text reference "CN204" (at 1.27 -2.33) (layer "F.SilkS"))
  (fp_text value "INTERNAL FLOPPY" (at 1.27 42.97) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 1.27 20.32 90) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "22" thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "24" thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "26" thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "27" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "28" thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "29" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "30" thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "31" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "32" thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "33" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "34" thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x17_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
