(footprint "TrimmerCap" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -0.0254 7.6708) (layer "F.SilkS"))
  (fp_text value "TrimmerCap" (at 0 -0.5) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -2.5 0) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 2.5 0) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
)
