(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SN74LVC16T245DLR" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 30.48 10.16 0))
    (property "Value" "SN74LVC16T245DLR" (id 1) (at 30.48 7.62 0))
    (property "Footprint" "DL48" (id 2) (at 0 0 0))
    (property "Datasheet" "SN74LVC16T245DLR" (id 3) (at 0 0 0))
    (property "ki_keywords" "SN74LVC16T245DLR" (id 4) (at 0 0 0))
    (property "ki_locked" "" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "DL48 DL48-M DL48-L" (id 6) (at 0 0 0))
    (symbol "SN74LVC16T245DLR_0_1"
      (pin input line (at 0 0 0) (length 7.62)
        (name "1DIR")
        (number "1")
      )
      (pin bidirectional line (at 0 -2.54 0) (length 7.62)
        (name "1B1")
        (number "2")
      )
      (pin bidirectional line (at 0 -5.08 0) (length 7.62)
        (name "1B2")
        (number "3")
      )
      (pin power_in line (at 0 -7.62 0) (length 7.62)
        (name "GND")
        (number "4")
      )
      (pin bidirectional line (at 0 -10.16 0) (length 7.62)
        (name "1B3")
        (number "5")
      )
      (pin bidirectional line (at 0 -12.7 0) (length 7.62)
        (name "1B4")
        (number "6")
      )
      (pin power_in line (at 0 -15.24 0) (length 7.62)
        (name "VCCB")
        (number "7")
      )
      (pin bidirectional line (at 0 -17.78 0) (length 7.62)
        (name "1B5")
        (number "8")
      )
      (pin bidirectional line (at 0 -20.32 0) (length 7.62)
        (name "1B6")
        (number "9")
      )
      (pin power_in line (at 0 -22.86 0) (length 7.62)
        (name "GND")
        (number "10")
      )
      (pin bidirectional line (at 0 -25.4 0) (length 7.62)
        (name "1B7")
        (number "11")
      )
      (pin bidirectional line (at 0 -27.94 0) (length 7.62)
        (name "1B8")
        (number "12")
      )
      (pin bidirectional line (at 0 -30.48 0) (length 7.62)
        (name "2B1")
        (number "13")
      )
      (pin bidirectional line (at 0 -33.02 0) (length 7.62)
        (name "2B2")
        (number "14")
      )
      (pin power_in line (at 0 -35.56 0) (length 7.62)
        (name "GND")
        (number "15")
      )
      (pin bidirectional line (at 0 -38.1 0) (length 7.62)
        (name "2B3")
        (number "16")
      )
      (pin bidirectional line (at 0 -40.64 0) (length 7.62)
        (name "2B4")
        (number "17")
      )
      (pin power_in line (at 0 -43.18 0) (length 7.62)
        (name "VCCB")
        (number "18")
      )
      (pin bidirectional line (at 0 -45.72 0) (length 7.62)
        (name "2B5")
        (number "19")
      )
      (pin bidirectional line (at 0 -48.26 0) (length 7.62)
        (name "2B6")
        (number "20")
      )
      (pin power_in line (at 0 -50.8 0) (length 7.62)
        (name "GND")
        (number "21")
      )
      (pin bidirectional line (at 0 -53.34 0) (length 7.62)
        (name "2B7")
        (number "22")
      )
      (pin bidirectional line (at 0 -55.88 0) (length 7.62)
        (name "2B8")
        (number "23")
      )
      (pin input line (at 0 -58.42 0) (length 7.62)
        (name "2DIR")
        (number "24")
      )
      (pin input line (at 60.96 -58.42 180) (length 7.62)
        (name "*2OE")
        (number "25")
      )
      (pin bidirectional line (at 60.96 -55.88 180) (length 7.62)
        (name "2A8")
        (number "26")
      )
      (pin bidirectional line (at 60.96 -53.34 180) (length 7.62)
        (name "2A7")
        (number "27")
      )
      (pin power_in line (at 60.96 -50.8 180) (length 7.62)
        (name "GND")
        (number "28")
      )
      (pin bidirectional line (at 60.96 -48.26 180) (length 7.62)
        (name "2A6")
        (number "29")
      )
      (pin bidirectional line (at 60.96 -45.72 180) (length 7.62)
        (name "2A5")
        (number "30")
      )
      (pin power_in line (at 60.96 -43.18 180) (length 7.62)
        (name "VCCA")
        (number "31")
      )
      (pin bidirectional line (at 60.96 -40.64 180) (length 7.62)
        (name "2A4")
        (number "32")
      )
      (pin bidirectional line (at 60.96 -38.1 180) (length 7.62)
        (name "2A3")
        (number "33")
      )
      (pin power_in line (at 60.96 -35.56 180) (length 7.62)
        (name "GND")
        (number "34")
      )
      (pin bidirectional line (at 60.96 -33.02 180) (length 7.62)
        (name "2A2")
        (number "35")
      )
      (pin bidirectional line (at 60.96 -30.48 180) (length 7.62)
        (name "2A1")
        (number "36")
      )
      (pin bidirectional line (at 60.96 -27.94 180) (length 7.62)
        (name "1A8")
        (number "37")
      )
      (pin bidirectional line (at 60.96 -25.4 180) (length 7.62)
        (name "1A7")
        (number "38")
      )
      (pin power_in line (at 60.96 -22.86 180) (length 7.62)
        (name "GND")
        (number "39")
      )
      (pin bidirectional line (at 60.96 -20.32 180) (length 7.62)
        (name "1A6")
        (number "40")
      )
      (pin bidirectional line (at 60.96 -17.78 180) (length 7.62)
        (name "1A5")
        (number "41")
      )
      (pin power_in line (at 60.96 -15.24 180) (length 7.62)
        (name "VCCA")
        (number "42")
      )
      (pin bidirectional line (at 60.96 -12.7 180) (length 7.62)
        (name "1A4")
        (number "43")
      )
      (pin bidirectional line (at 60.96 -10.16 180) (length 7.62)
        (name "1A3")
        (number "44")
      )
      (pin power_in line (at 60.96 -7.62 180) (length 7.62)
        (name "GND")
        (number "45")
      )
      (pin bidirectional line (at 60.96 -5.08 180) (length 7.62)
        (name "1A2")
        (number "46")
      )
      (pin bidirectional line (at 60.96 -2.54 180) (length 7.62)
        (name "1A1")
        (number "47")
      )
      (pin input line (at 60.96 0 180) (length 7.62)
        (name "*1OE")
        (number "48")
      )
    )
  )
)
