(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Denise" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U300" (at 0.127 21.844 0))
    (property "Value" "DENISE" (at 5.08 -10.16 0))
    (property "Footprint" "Package_DIP:DIP-48_W15.24mm" (at 0 0 0))
    (property "Datasheet" "" (at 0 0 0))
    (property "ki_locked" "" (at 0 0 0))
    (symbol "Denise_1_1"
      (pin bidirectional line (at -12.7 -17.78 0) (length 5.08)
        (name "DRD6")
        (number "1")
      )
      (pin input line (at -12.7 -43.18 0) (length 5.08)
        (name "RGA8")
        (number "10")
      )
      (pin input line (at -12.7 -45.72 0) (length 5.08)
        (name "RGA7")
        (number "11")
      )
      (pin input line (at -12.7 -48.26 0) (length 5.08)
        (name "RGA6")
        (number "12")
      )
      (pin input line (at -12.7 -50.8 0) (length 5.08)
        (name "RGA5")
        (number "13")
      )
      (pin input line (at -12.7 -53.34 0) (length 5.08)
        (name "RGA4")
        (number "14")
      )
      (pin input line (at -12.7 -55.88 0) (length 5.08)
        (name "RGA3")
        (number "15")
      )
      (pin input line (at -12.7 -58.42 0) (length 5.08)
        (name "RGA2")
        (number "16")
      )
      (pin input line (at -12.7 -60.96 0) (length 5.08)
        (name "RGA1")
        (number "17")
      )
      (pin output inverted (at 13.97 -20.32 180) (length 5.08)
        (name "BURST")
        (number "18")
      )
      (pin bidirectional line (at -12.7 -20.32 0) (length 5.08)
        (name "DRD5")
        (number "2")
      )
      (pin output line (at 13.97 -43.18 180) (length 5.08)
        (name "R0")
        (number "20")
      )
      (pin output line (at 13.97 -40.64 180) (length 5.08)
        (name "R1")
        (number "21")
      )
      (pin output line (at 13.97 -38.1 180) (length 5.08)
        (name "R2")
        (number "22")
      )
      (pin output line (at 13.97 -35.56 180) (length 5.08)
        (name "R3")
        (number "23")
      )
      (pin output line (at 13.97 -83.82 180) (length 5.08)
        (name "B0")
        (number "24")
      )
      (pin output line (at 13.97 -81.28 180) (length 5.08)
        (name "B1")
        (number "25")
      )
      (pin output line (at 13.97 -78.74 180) (length 5.08)
        (name "B2")
        (number "26")
      )
      (pin output line (at 13.97 -76.2 180) (length 5.08)
        (name "B3")
        (number "27")
      )
      (pin output line (at 13.97 -63.5 180) (length 5.08)
        (name "G0")
        (number "28")
      )
      (pin output line (at 13.97 -60.96 180) (length 5.08)
        (name "G1")
        (number "29")
      )
      (pin bidirectional line (at -12.7 -22.86 0) (length 5.08)
        (name "DRD4")
        (number "3")
      )
      (pin output line (at 13.97 -58.42 180) (length 5.08)
        (name "G2")
        (number "30")
      )
      (pin output line (at 13.97 -55.88 180) (length 5.08)
        (name "G3")
        (number "31")
      )
      (pin input inverted (at -12.7 17.78 0) (length 5.08)
        (name "/CSYNC")
        (number "32")
      )
      (pin output inverted (at 13.97 -25.4 180) (length 5.08)
        (name "PIXELSW")
        (number "33")
      )
      (pin input inverted (at -12.7 12.7 0) (length 5.08)
        (name "/CDAC")
        (number "34")
      )
      (pin input line (at -12.7 -81.28 0) (length 5.08)
        (name "7M")
        (number "35")
      )
      (pin input line (at -12.7 -72.39 0) (length 5.08)
        (name "CCK")
        (number "36")
      )
      (pin input line (at 13.97 7.62 180) (length 5.08)
        (name "M0V")
        (number "38")
      )
      (pin input line (at 13.97 17.78 180) (length 5.08)
        (name "M1V")
        (number "39")
      )
      (pin bidirectional line (at -12.7 -25.4 0) (length 5.08)
        (name "DRD3")
        (number "4")
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08)
        (name "DRD15")
        (number "40")
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08)
        (name "DRD14")
        (number "41")
      )
      (pin bidirectional line (at -12.7 0 0) (length 5.08)
        (name "DRD13")
        (number "42")
      )
      (pin bidirectional line (at -12.7 -2.54 0) (length 5.08)
        (name "DRD12")
        (number "43")
      )
      (pin bidirectional line (at -12.7 -5.08 0) (length 5.08)
        (name "DRD11")
        (number "44")
      )
      (pin bidirectional line (at -12.7 -7.62 0) (length 5.08)
        (name "DRD10")
        (number "45")
      )
      (pin bidirectional line (at -12.7 -10.16 0) (length 5.08)
        (name "DRD9")
        (number "46")
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 5.08)
        (name "DRD8")
        (number "47")
      )
      (pin bidirectional line (at -12.7 -15.24 0) (length 5.08)
        (name "DRD7")
        (number "48")
      )
      (pin bidirectional line (at -12.7 -27.94 0) (length 5.08)
        (name "DRD2")
        (number "5")
      )
      (pin bidirectional line (at -12.7 -30.48 0) (length 5.08)
        (name "DRD1")
        (number "6")
      )
      (pin bidirectional line (at -12.7 -33.02 0) (length 5.08)
        (name "DRD0")
        (number "7")
      )
      (pin input line (at 13.97 12.7 180) (length 5.08)
        (name "M1H")
        (number "8")
      )
      (pin input line (at 13.97 2.54 180) (length 5.08)
        (name "M0H")
        (number "9")
      )
    )
    (symbol "Denise_2_1"
      (pin power_in line (at 0 8.89 270) (length 2.54)
        (name "VCC")
        (number "19")
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND1")
        (number "37")
      )
    )
  )
)
