(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "8520" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U204" (at 0 53.34 0))
    (property "Value" "8520" (at 0 40.64 0))
    (property "Footprint" "Package_DIP:DIP-40_W15.24mm_Socket" (at 0 34.29 0))
    (property "Datasheet" "" (at 0 34.29 0))
    (property "ki_locked" "" (at 0 0 0))
    (symbol "8520_1_1"
      (pin bidirectional line (at 10.16 -63.5 180) (length 2.54)
        (name "PB0")
        (number "10")
      )
      (pin bidirectional line (at 10.16 -58.42 180) (length 2.54)
        (name "PB1")
        (number "11")
      )
      (pin bidirectional line (at 10.16 -53.34 180) (length 2.54)
        (name "PB2")
        (number "12")
      )
      (pin bidirectional line (at 10.16 -48.26 180) (length 2.54)
        (name "PB3")
        (number "13")
      )
      (pin bidirectional line (at 10.16 -43.18 180) (length 2.54)
        (name "PB4")
        (number "14")
      )
      (pin bidirectional line (at 10.16 -38.1 180) (length 2.54)
        (name "PB5")
        (number "15")
      )
      (pin bidirectional line (at 10.16 -33.02 180) (length 2.54)
        (name "PB6")
        (number "16")
      )
      (pin bidirectional line (at 10.16 -27.94 180) (length 2.54)
        (name "PB7")
        (number "17")
      )
      (pin output line (at 10.16 30.48 180) (length 2.54)
        (name "_PC")
        (number "18")
      )
      (pin input line (at -11.43 -43.18 0) (length 2.54)
        (name "TICK")
        (number "19")
      )
      (pin bidirectional line (at 10.16 -15.24 180) (length 2.54)
        (name "PA0")
        (number "2")
      )
      (pin output line (at -11.43 -33.02 0) (length 2.54)
        (name "_INT")
        (number "21")
      )
      (pin input line (at -11.43 -17.78 0) (length 2.54)
        (name "_W")
        (number "22")
      )
      (pin input line (at -11.43 -12.7 0) (length 2.54)
        (name "_CS")
        (number "23")
      )
      (pin input line (at 10.16 35.56 180) (length 2.54)
        (name "_F")
        (number "24")
      )
      (pin input line (at -11.43 -22.86 0) (length 2.54)
        (name "E")
        (number "25")
      )
      (pin bidirectional line (at -11.43 38.1 0) (length 2.54)
        (name "D7")
        (number "26")
      )
      (pin bidirectional line (at -11.43 35.56 0) (length 2.54)
        (name "D6")
        (number "27")
      )
      (pin bidirectional line (at -11.43 33.02 0) (length 2.54)
        (name "D5")
        (number "28")
      )
      (pin bidirectional line (at -11.43 30.48 0) (length 2.54)
        (name "D4")
        (number "29")
      )
      (pin bidirectional line (at 10.16 -10.16 180) (length 2.54)
        (name "PA1")
        (number "3")
      )
      (pin bidirectional line (at -11.43 27.94 0) (length 2.54)
        (name "D3")
        (number "30")
      )
      (pin bidirectional line (at -11.43 25.4 0) (length 2.54)
        (name "D2")
        (number "31")
      )
      (pin bidirectional line (at -11.43 22.86 0) (length 2.54)
        (name "D1")
        (number "32")
      )
      (pin bidirectional line (at -11.43 20.32 0) (length 2.54)
        (name "D0")
        (number "33")
      )
      (pin input line (at -11.43 -53.34 0) (length 2.54)
        (name "_RESET")
        (number "34")
      )
      (pin input line (at -11.43 10.16 0) (length 2.54)
        (name "RS3")
        (number "35")
      )
      (pin input line (at -11.43 7.62 0) (length 2.54)
        (name "RS2")
        (number "36")
      )
      (pin input line (at -11.43 5.08 0) (length 2.54)
        (name "RS1")
        (number "37")
      )
      (pin input line (at -11.43 2.54 0) (length 2.54)
        (name "RS0")
        (number "38")
      )
      (pin input line (at 10.16 45.72 180) (length 2.54)
        (name "S")
        (number "39")
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 2.54)
        (name "PA2")
        (number "4")
      )
      (pin input line (at 10.16 50.8 180) (length 2.54)
        (name "C")
        (number "40")
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "PA3")
        (number "5")
      )
      (pin bidirectional line (at 10.16 5.08 180) (length 2.54)
        (name "PA4")
        (number "6")
      )
      (pin bidirectional line (at 10.16 10.16 180) (length 2.54)
        (name "PA5")
        (number "7")
      )
      (pin bidirectional line (at 10.16 15.24 180) (length 2.54)
        (name "PA6")
        (number "8")
      )
      (pin bidirectional line (at 10.16 20.32 180) (length 2.54)
        (name "PA7")
        (number "9")
      )
    )
    (symbol "8520_2_1"
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "GND1")
        (number "1")
      )
      (pin power_in line (at 0 8.89 270) (length 2.54)
        (name "VCC")
        (number "20")
      )
    )
  )
)
