(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SDRAM_128MB(8Mx16)" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -1.27 3.81 0))
    (property "Value" "SDRAM_128MB(8Mx16)" (id 1) (at 0 -3.81 0))
    (property "Footprint" "TSOPII-54" (id 2) (at 0 0 0))
    (property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/dram/64M-AS4C4M16SA-CI_v3.0_March%202015.pdf" (id 3) (at 0 -6.35 0))
    (property "ki_keywords" "SDRAM Synchronus DRAM PC166 PC143 64Mb 16Mbx4 MEMORY" (id 4) (at 0 0 0))
    (property "ki_description" "64M – (4M x 16 bit) Synchronous DRAM (SDRAM), TSOP II 54pin" (id 5) (at 0 0 0))
    (symbol "SDRAM_128MB(8Mx16)_0_0"
      (pin no_connect line (at 19.05 -24.13 180) (length 2.54)
        (name "NC/RFU")
        (number "40")
      )
    )
    (symbol "SDRAM_128MB(8Mx16)_0_1")
    (symbol "SDRAM_128MB(8Mx16)_1_1"
      (pin power_in line (at -7.62 33.02 270) (length 3.81)
        (name "VDD")
        (number "1")
      )
      (pin bidirectional line (at 20.32 13.97 180) (length 3.81)
        (name "DQ5")
        (number "10")
      )
      (pin bidirectional line (at 20.32 11.43 180) (length 3.81)
        (name "DQ6")
        (number "11")
      )
      (pin power_in line (at 2.54 -33.02 90) (length 3.81)
        (name "VSSQ")
        (number "12")
      )
      (pin bidirectional line (at 20.32 8.89 180) (length 3.81)
        (name "DQ7")
        (number "13")
      )
      (pin power_in line (at -5.08 33.02 270) (length 3.81)
        (name "VDD")
        (number "14")
      )
      (pin input line (at 20.32 -17.78 180) (length 3.81)
        (name "LDQM")
        (number "15")
      )
      (pin input inverted (at -20.32 -22.86 0) (length 3.81)
        (name "WE")
        (number "16")
      )
      (pin input inverted (at -20.32 -20.32 0) (length 3.81)
        (name "CAS")
        (number "17")
      )
      (pin input inverted (at -20.32 -17.78 0) (length 3.81)
        (name "RAS")
        (number "18")
      )
      (pin input inverted (at -20.32 -26.67 0) (length 3.81)
        (name "CS")
        (number "19")
      )
      (pin bidirectional line (at 20.32 26.67 180) (length 3.81)
        (name "DQ0")
        (number "2")
      )
      (pin input line (at -20.32 -5.08 0) (length 3.81)
        (name "BA0")
        (number "20")
      )
      (pin input line (at -20.32 -7.62 0) (length 3.81)
        (name "BA1")
        (number "21")
      )
      (pin input line (at -20.32 1.27 0) (length 3.81)
        (name "A10")
        (number "22")
      )
      (pin input line (at -20.32 26.67 0) (length 3.81)
        (name "A0")
        (number "23")
      )
      (pin input line (at -20.32 24.13 0) (length 3.81)
        (name "A1")
        (number "24")
      )
      (pin input line (at -20.32 21.59 0) (length 3.81)
        (name "A2")
        (number "25")
      )
      (pin input line (at -20.32 19.05 0) (length 3.81)
        (name "A3")
        (number "26")
      )
      (pin power_in line (at -2.54 33.02 270) (length 3.81)
        (name "VDD")
        (number "27")
      )
      (pin power_in line (at -7.62 -33.02 90) (length 3.81)
        (name "VSS")
        (number "28")
      )
      (pin input line (at -20.32 16.51 0) (length 3.81)
        (name "A4")
        (number "29")
      )
      (pin power_in line (at 0 33.02 270) (length 3.81)
        (name "VDDQ")
        (number "3")
      )
      (pin input line (at -20.32 13.97 0) (length 3.81)
        (name "A5")
        (number "30")
      )
      (pin input line (at -20.32 11.43 0) (length 3.81)
        (name "A6")
        (number "31")
      )
      (pin input line (at -20.32 8.89 0) (length 3.81)
        (name "A7")
        (number "32")
      )
      (pin input line (at -20.32 6.35 0) (length 3.81)
        (name "A8")
        (number "33")
      )
      (pin input line (at -20.32 3.81 0) (length 3.81)
        (name "A9")
        (number "34")
      )
      (pin input line (at -20.32 -1.27 0) (length 3.81)
        (name "A11")
        (number "35")
      )
      (pin input line (at -20.32 -13.97 0) (length 3.81)
        (name "CKE")
        (number "37")
      )
      (pin input line (at -20.32 -11.43 0) (length 3.81)
        (name "CLK")
        (number "38")
      )
      (pin input line (at 20.32 -20.32 180) (length 3.81)
        (name "UDQM")
        (number "39")
      )
      (pin bidirectional line (at 20.32 24.13 180) (length 3.81)
        (name "DQ1")
        (number "4")
      )
      (pin power_in line (at -5.08 -33.02 90) (length 3.81)
        (name "VSS")
        (number "41")
      )
      (pin bidirectional line (at 20.32 6.35 180) (length 3.81)
        (name "DQ8")
        (number "42")
      )
      (pin power_in line (at 5.08 33.02 270) (length 3.81)
        (name "VDDQ")
        (number "43")
      )
      (pin bidirectional line (at 20.32 3.81 180) (length 3.81)
        (name "DQ9")
        (number "44")
      )
      (pin bidirectional line (at 20.32 1.27 180) (length 3.81)
        (name "DQ10")
        (number "45")
      )
      (pin power_in line (at 5.08 -33.02 90) (length 3.81)
        (name "VSSQ")
        (number "46")
      )
      (pin bidirectional line (at 20.32 -1.27 180) (length 3.81)
        (name "DQ11")
        (number "47")
      )
      (pin bidirectional line (at 20.32 -3.81 180) (length 3.81)
        (name "DQ12")
        (number "48")
      )
      (pin power_in line (at 7.62 33.02 270) (length 3.81)
        (name "VDDQ")
        (number "49")
      )
      (pin bidirectional line (at 20.32 21.59 180) (length 3.81)
        (name "DQ2")
        (number "5")
      )
      (pin bidirectional line (at 20.32 -6.35 180) (length 3.81)
        (name "DQ13")
        (number "50")
      )
      (pin bidirectional line (at 20.32 -8.89 180) (length 3.81)
        (name "DQ14")
        (number "51")
      )
      (pin power_in line (at 7.62 -33.02 90) (length 3.81)
        (name "VSSQ")
        (number "52")
      )
      (pin bidirectional line (at 20.32 -11.43 180) (length 3.81)
        (name "DQ15")
        (number "53")
      )
      (pin power_in line (at -2.54 -33.02 90) (length 3.81)
        (name "VSS")
        (number "54")
      )
      (pin power_in line (at 0 -33.02 90) (length 3.81)
        (name "VSSQ")
        (number "6")
      )
      (pin bidirectional line (at 20.32 19.05 180) (length 3.81)
        (name "DQ3")
        (number "7")
      )
      (pin bidirectional line (at 20.32 16.51 180) (length 3.81)
        (name "DQ4")
        (number "8")
      )
      (pin power_in line (at 2.54 33.02 270) (length 3.81)
        (name "VDDQ")
        (number "9")
      )
    )
  )
)
