(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "Agnus_MULTI" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 11.43 0))
    (property "Value" "Agnus_MULTI" (id 1) (at 0 0 0))
    (property "Footprint" "Package_LCC:PLCC-84_THT-Socket" (id 2) (at 0 -3.048 0))
    (property "Datasheet" "" (id 3) (at -2.54 39.37 0))
    (property "ki_locked" "" (id 4) (at 0 0 0))
    (symbol "Agnus_MULTI_1_1"
      (pin bidirectional line (at -17.78 52.07 0) (length 2.54)
        (name "DRD13")
        (number "1")
      )
      (pin bidirectional line (at -17.78 29.21 0) (length 2.54)
        (name "DRD4")
        (number "10")
      )
      (pin bidirectional line (at -17.78 26.67 0) (length 2.54)
        (name "DRD3")
        (number "11")
      )
      (pin bidirectional line (at -17.78 24.13 0) (length 2.54)
        (name "DRD2")
        (number "12")
      )
      (pin bidirectional line (at -17.78 21.59 0) (length 2.54)
        (name "DRD1")
        (number "13")
      )
      (pin bidirectional line (at -17.78 19.05 0) (length 2.54)
        (name "DRD0")
        (number "14")
      )
      (pin input line (at -17.78 -54.61 0) (length 2.54)
        (name "_RESET")
        (number "16")
      )
      (pin output line (at -17.78 -59.69 0) (length 2.54)
        (name "_INTR")
        (number "17")
      )
      (pin input line (at -17.78 -57.15 0) (length 2.54)
        (name "DMAL")
        (number "18")
      )
      (pin input line (at 0 62.23 270) (length 2.54)
        (name "_BLS")
        (number "19")
      )
      (pin bidirectional line (at -17.78 49.53 0) (length 2.54)
        (name "DRD12")
        (number "2")
      )
      (pin output line (at 2.54 62.23 270) (length 2.54)
        (name "_DBR")
        (number "20")
      )
      (pin output line (at 17.78 20.32 180) (length 2.54)
        (name "_WE")
        (number "21")
      )
      (pin input line (at -17.78 -46.99 0) (length 2.54)
        (name "R/W")
        (number "22")
      )
      (pin input line (at -2.54 62.23 270) (length 2.54)
        (name "_REGEN")
        (number "23")
      )
      (pin input line (at -17.78 -49.53 0) (length 2.54)
        (name "_AS")
        (number "24")
      )
      (pin input line (at -5.08 62.23 270) (length 2.54)
        (name "_RAMEN")
        (number "25")
      )
      (pin output line (at 17.78 -15.24 180) (length 2.54)
        (name "RGA8")
        (number "26")
      )
      (pin output line (at 17.78 -17.78 180) (length 2.54)
        (name "RGA7")
        (number "27")
      )
      (pin output line (at 17.78 -20.32 180) (length 2.54)
        (name "RGA6")
        (number "28")
      )
      (pin output line (at 17.78 -22.86 180) (length 2.54)
        (name "RGA5")
        (number "29")
      )
      (pin bidirectional line (at -17.78 46.99 0) (length 2.54)
        (name "DRD11")
        (number "3")
      )
      (pin output line (at 17.78 -25.4 180) (length 2.54)
        (name "RGA4")
        (number "30")
      )
      (pin output line (at 17.78 -27.94 180) (length 2.54)
        (name "RGA3")
        (number "31")
      )
      (pin output line (at 17.78 -30.48 180) (length 2.54)
        (name "RGA2")
        (number "32")
      )
      (pin output line (at 17.78 -33.02 180) (length 2.54)
        (name "RGA1")
        (number "33")
      )
      (pin output line (at -17.78 -67.31 0) (length 2.54)
        (name "28MHz")
        (number "34")
      )
      (pin bidirectional line (at -17.78 12.7 0) (length 2.54)
        (name "A20/XCLK")
        (number "35")
      )
      (pin output line (at 17.78 -45.72 180) (length 2.54)
        (name "_CDAC/_XCLKEN")
        (number "36")
      )
      (pin output line (at 17.78 -41.91 180) (length 2.54)
        (name "7MHz/_CDAC")
        (number "37")
      )
      (pin output line (at 17.78 52.07 180) (length 2.54)
        (name "CCKQ/7MHz")
        (number "38")
      )
      (pin output line (at 17.78 48.26 180) (length 2.54)
        (name "CCK/CCKQ")
        (number "39")
      )
      (pin bidirectional line (at -17.78 44.45 0) (length 2.54)
        (name "DRD10")
        (number "4")
      )
      (pin output line (at 17.78 44.45 180) (length 2.54)
        (name "14M_or_Vbb/CCK")
        (number "40")
      )
      (pin input line (at 17.78 -67.31 180) (length 2.54)
        (name "GND/PAL-NTSC")
        (number "41")
      )
      (pin output line (at 17.78 -10.16 180) (length 2.54)
        (name "DRA0/GND")
        (number "42")
      )
      (pin output line (at 17.78 -7.62 180) (length 2.54)
        (name "DRA1/DRA0")
        (number "43")
      )
      (pin output line (at 17.78 -5.08 180) (length 2.54)
        (name "DRA2/DRA1")
        (number "44")
      )
      (pin output line (at 17.78 -2.54 180) (length 2.54)
        (name "DRA3/DRA2")
        (number "45")
      )
      (pin output line (at 17.78 0 180) (length 2.54)
        (name "DRA4/DRA3")
        (number "46")
      )
      (pin output line (at 17.78 2.54 180) (length 2.54)
        (name "DRA5/DRA4")
        (number "47")
      )
      (pin output line (at 17.78 5.08 180) (length 2.54)
        (name "DRA6/DRA5")
        (number "48")
      )
      (pin output line (at 17.78 7.62 180) (length 2.54)
        (name "DRA7/DRA6")
        (number "49")
      )
      (pin bidirectional line (at -17.78 41.91 0) (length 2.54)
        (name "DRD9")
        (number "5")
      )
      (pin output line (at 17.78 10.16 180) (length 2.54)
        (name "DRA8/DRA7")
        (number "50")
      )
      (pin input line (at -17.78 -41.91 0) (length 2.54)
        (name "_LDS/DRA8")
        (number "51")
      )
      (pin input line (at -17.78 -44.45 0) (length 2.54)
        (name "_UDS/_LDS")
        (number "52")
      )
      (pin output line (at 17.78 39.37 180) (length 2.54)
        (name "_CASL/_UDS")
        (number "53")
      )
      (pin output line (at 17.78 35.56 180) (length 2.54)
        (name "_CASU/_CASL")
        (number "54")
      )
      (pin output line (at 17.78 12.7 180) (length 2.54)
        (name "DRA9/_CASU")
        (number "55")
      )
      (pin output line (at 17.78 26.67 180) (length 2.54)
        (name "_RAS1")
        (number "56")
      )
      (pin output line (at 17.78 30.48 180) (length 2.54)
        (name "_RAS0")
        (number "57")
      )
      (pin bidirectional line (at -17.78 10.16 0) (length 2.54)
        (name "A19")
        (number "59")
      )
      (pin bidirectional line (at -17.78 39.37 0) (length 2.54)
        (name "DRD8")
        (number "6")
      )
      (pin bidirectional line (at -17.78 -35.56 0) (length 2.54)
        (name "A1")
        (number "60")
      )
      (pin bidirectional line (at -17.78 -33.02 0) (length 2.54)
        (name "A2")
        (number "61")
      )
      (pin bidirectional line (at -17.78 -30.48 0) (length 2.54)
        (name "A3")
        (number "62")
      )
      (pin bidirectional line (at -17.78 -27.94 0) (length 2.54)
        (name "A4")
        (number "63")
      )
      (pin bidirectional line (at -17.78 -25.4 0) (length 2.54)
        (name "A5")
        (number "64")
      )
      (pin bidirectional line (at -17.78 -22.86 0) (length 2.54)
        (name "A6")
        (number "65")
      )
      (pin bidirectional line (at -17.78 -20.32 0) (length 2.54)
        (name "A7")
        (number "66")
      )
      (pin bidirectional line (at -17.78 -17.78 0) (length 2.54)
        (name "A8")
        (number "67")
      )
      (pin bidirectional line (at -17.78 -15.24 0) (length 2.54)
        (name "A9")
        (number "68")
      )
      (pin bidirectional line (at -17.78 -12.7 0) (length 2.54)
        (name "A10")
        (number "69")
      )
      (pin bidirectional line (at -17.78 36.83 0) (length 2.54)
        (name "DRD7")
        (number "7")
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 2.54)
        (name "A11")
        (number "70")
      )
      (pin bidirectional line (at -17.78 -7.62 0) (length 2.54)
        (name "A12")
        (number "71")
      )
      (pin bidirectional line (at -17.78 -5.08 0) (length 2.54)
        (name "A13")
        (number "72")
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 2.54)
        (name "A14")
        (number "73")
      )
      (pin bidirectional line (at -17.78 0 0) (length 2.54)
        (name "A15")
        (number "74")
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 2.54)
        (name "A16")
        (number "75")
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 2.54)
        (name "A17")
        (number "76")
      )
      (pin bidirectional line (at -17.78 7.62 0) (length 2.54)
        (name "A18")
        (number "77")
      )
      (pin input line (at 17.78 -54.61 180) (length 2.54)
        (name "_LPEN")
        (number "78")
      )
      (pin bidirectional line (at 17.78 -59.69 180) (length 2.54)
        (name "_VSYNC")
        (number "79")
      )
      (pin bidirectional line (at -17.78 34.29 0) (length 2.54)
        (name "DRD6")
        (number "8")
      )
      (pin output line (at 17.78 -62.23 180) (length 2.54)
        (name "_CSYNC")
        (number "80")
      )
      (pin bidirectional line (at 17.78 -57.15 180) (length 2.54)
        (name "_HSYNC")
        (number "81")
      )
      (pin bidirectional line (at -17.78 57.15 0) (length 2.54)
        (name "DRD15")
        (number "83")
      )
      (pin bidirectional line (at -17.78 54.61 0) (length 2.54)
        (name "DRD14")
        (number "84")
      )
      (pin bidirectional line (at -17.78 31.75 0) (length 2.54)
        (name "DRD5")
        (number "9")
      )
    )
    (symbol "Agnus_MULTI_2_1"
      (pin power_in line (at 0 8.89 270) (length 2.54)
        (name "VCC")
        (number "15")
      )
      (pin power_in line (at -3.81 -10.16 90) (length 2.54)
        (name "GND")
        (number "58")
      )
      (pin power_in line (at 3.81 -10.16 90) (length 2.54)
        (name "GND")
        (number "82")
      )
    )
  )
)
