(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "ATX-24-Amiga" (in_bom yes) (on_board yes)
    (property "Reference" "CN601" (at 0 16.9418 0))
    (property "Value" "ATX-24" (at 0 14.6304 0))
    (property "Footprint" "Connector_Molex:Molex_Mini-Fit_Jr_5566-24A_2x12_P4.20mm_Vertical" (at 0 -2.54 0))
    (property "Datasheet" "https://www.intel.com/content/dam/www/public/us/en/documents/guides/power-supply-design-guide-june.pdf#page=33" (at 60.96 -13.97 0))
    (property "Part" "39281243" (at 0 0 0))
    (property "ki_keywords" "ATX PSU" (at 0 0 0))
    (property "ki_description" "ATX Power supply 24pins" (at 0 0 0))
    (property "ki_fp_filters" "*Mini?Fit*2x12*Vertical* *Mini?Fit*2x12*Horizontal*" (at 0 0 0))
    (symbol "ATX-24-Amiga_0_0"
      (pin power_out line (at 12.7 -2.54 180) (length 2.54)
        (name "+3.3V")
        (number "1")
      )
      (pin power_out line (at 12.7 -2.54 180) (length 2.54) hide
        (name "+3.3V")
        (number "13")
      )
      (pin power_out line (at 12.7 -2.54 180) (length 2.54) hide
        (name "+3.3V")
        (number "2")
      )
    )
    (symbol "ATX-24-Amiga_0_1")
    (symbol "ATX-24-Amiga_1_0"
      (pin power_out line (at 12.7 -2.54 180) (length 2.54) hide
        (name "+3.3V")
        (number "12")
      )
    )
    (symbol "ATX-24-Amiga_1_1"
      (pin power_out line (at 12.7 5.08 180) (length 2.54)
        (name "+12V")
        (number "10")
      )
      (pin passive line (at 12.7 5.08 180) (length 2.54) hide
        (name "+12V")
        (number "11")
      )
      (pin power_out line (at 12.7 -10.16 180) (length 2.54)
        (name "-12V")
        (number "14")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "15")
      )
      (pin open_collector line (at -12.7 10.16 0) (length 2.54)
        (name "PS_ON#")
        (number "16")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "17")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "18")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "19")
      )
      (pin no_connect line (at -10.16 0 0) (length 2.54) hide
        (name "NC")
        (number "20")
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54) hide
        (name "+5V")
        (number "21")
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54) hide
        (name "+5V")
        (number "22")
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54) hide
        (name "+5V")
        (number "23")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "24")
      )
      (pin power_out line (at 0 -15.24 90) (length 2.54)
        (name "GND")
        (number "3")
      )
      (pin power_out line (at 12.7 2.54 180) (length 2.54)
        (name "+5V")
        (number "4")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "5")
      )
      (pin passive line (at 12.7 2.54 180) (length 2.54) hide
        (name "+5V")
        (number "6")
      )
      (pin passive line (at 0 -15.24 90) (length 2.54) hide
        (name "GND")
        (number "7")
      )
      (pin output line (at 12.7 10.16 180) (length 2.54)
        (name "PWR_OK")
        (number "8")
      )
      (pin power_out line (at 12.7 0 180) (length 2.54)
        (name "+5VSB")
        (number "9")
      )
    )
  )
)
