(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "DIN41612_03x40"
		(pin_names
			(offset 1.016) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 77.724 0)
		)
		(property "Value" "DIN41612_03x40"
			(at -0.254 2.032 0)
		)
		(property "Footprint" ""
			(at -1.27 41.91 0)
		)
		(property "Datasheet" "~"
			(at -1.27 41.91 0)
		)
		(property "Description" "DIN41612 connector, three row, 03x40"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_03x40_1_0"
			(pin passive line
				(at -6.35 74.93 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -6.35 6.35 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -6.35 -16.51 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -6.35 -24.13 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -6.35 -31.75 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -6.35 -46.99 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -6.35 -54.61 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -6.35 -62.23 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -6.35 67.31 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at 6.35 74.93 180)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at 6.35 67.31 180)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at 6.35 59.69 180)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at 6.35 52.07 180)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at 6.35 36.83 180)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at 6.35 29.21 180)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at 6.35 21.59 180)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at 6.35 6.35 180)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at 6.35 -8.89 180)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 6.35 -16.51 180)
				(length 3.81)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at 6.35 -31.75 180)
				(length 3.81)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at 6.35 -39.37 180)
				(length 3.81)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at 6.35 -46.99 180)
				(length 3.81)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at 6.35 -62.23 180)
				(length 3.81)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -6.35 52.07 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at 6.35 -69.85 180)
				(length 3.81)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -6.35 44.45 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -6.35 36.83 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -6.35 21.59 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -6.35 13.97 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -6.35 72.39 0)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at -6.35 3.81 0)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at -6.35 -11.43 0)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at -6.35 -19.05 0)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at -6.35 -26.67 0)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at -6.35 -34.29 0)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at -6.35 -49.53 0)
				(length 3.81)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at -6.35 -57.15 0)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at -6.35 -64.77 0)
				(length 3.81)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 6.35 72.39 180)
				(length 3.81)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 6.35 64.77 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 6.35 57.15 180)
				(length 3.81)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 6.35 34.29 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 6.35 26.67 180)
				(length 3.81)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 6.35 19.05 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 6.35 3.81 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 3.81)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 6.35 -11.43 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 6.35 -26.67 180)
				(length 3.81)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 6.35 -34.29 180)
				(length 3.81)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 6.35 -41.91 180)
				(length 3.81)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 6.35 -49.53 180)
				(length 3.81)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 6.35 -64.77 180)
				(length 3.81)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at -6.35 49.53 0)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 6.35 -72.39 180)
				(length 3.81)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at -6.35 41.91 0)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at -6.35 34.29 0)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at -6.35 19.05 0)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at -6.35 11.43 0)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at -6.35 69.85 0)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at -6.35 -13.97 0)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at -6.35 -21.59 0)
				(length 3.81)
				(name "Pin_c13")
				(number "c13")
			)
			(pin passive line
				(at -6.35 -29.21 0)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at -6.35 -44.45 0)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
			(pin passive line
				(at -6.35 -52.07 0)
				(length 3.81)
				(name "Pin_c17")
				(number "c17")
			)
			(pin passive line
				(at -6.35 -59.69 0)
				(length 3.81)
				(name "Pin_c18")
				(number "c18")
			)
			(pin passive line
				(at -6.35 -67.31 0)
				(length 3.81)
				(name "Pin_c19")
				(number "c19")
			)
			(pin passive line
				(at 6.35 69.85 180)
				(length 3.81)
				(name "Pin_c21")
				(number "c21")
			)
			(pin passive line
				(at 6.35 62.23 180)
				(length 3.81)
				(name "Pin_c22")
				(number "c22")
			)
			(pin passive line
				(at 6.35 54.61 180)
				(length 3.81)
				(name "Pin_c23")
				(number "c23")
			)
			(pin passive line
				(at 6.35 39.37 180)
				(length 3.81)
				(name "Pin_c25")
				(number "c25")
			)
			(pin passive line
				(at 6.35 31.75 180)
				(length 3.81)
				(name "Pin_c26")
				(number "c26")
			)
			(pin passive line
				(at 6.35 24.13 180)
				(length 3.81)
				(name "Pin_c27")
				(number "c27")
			)
			(pin passive line
				(at -6.35 54.61 0)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at 6.35 1.27 180)
				(length 3.81)
				(name "Pin_c30")
				(number "c30")
			)
			(pin passive line
				(at 6.35 -6.35 180)
				(length 3.81)
				(name "Pin_c31")
				(number "c31")
			)
			(pin passive line
				(at 6.35 -13.97 180)
				(length 3.81)
				(name "Pin_c32")
				(number "c32")
			)
			(pin passive line
				(at 6.35 -29.21 180)
				(length 3.81)
				(name "Pin_c34")
				(number "c34")
			)
			(pin passive line
				(at 6.35 -36.83 180)
				(length 3.81)
				(name "Pin_c35")
				(number "c35")
			)
			(pin passive line
				(at 6.35 -44.45 180)
				(length 3.81)
				(name "Pin_c36")
				(number "c36")
			)
			(pin passive line
				(at 6.35 -59.69 180)
				(length 3.81)
				(name "Pin_c38")
				(number "c38")
			)
			(pin passive line
				(at 6.35 -67.31 180)
				(length 3.81)
				(name "Pin_c39")
				(number "c39")
			)
			(pin passive line
				(at -6.35 46.99 0)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 6.35 -74.93 180)
				(length 3.81)
				(name "Pin_c40")
				(number "c40")
			)
			(pin passive line
				(at -6.35 39.37 0)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at -6.35 16.51 0)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at -6.35 8.89 0)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
		)
		(symbol "DIN41612_03x40_1_1"
			(pin passive line
				(at -6.35 -1.27 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -6.35 -8.89 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -6.35 -39.37 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -6.35 -69.85 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at 6.35 44.45 180)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at 6.35 13.97 180)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -6.35 59.69 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at 6.35 -24.13 180)
				(length 3.81)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at 6.35 -54.61 180)
				(length 3.81)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -6.35 29.21 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -6.35 -3.81 0)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at -6.35 -41.91 0)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at -6.35 64.77 0)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at -6.35 -72.39 0)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 6.35 49.53 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 6.35 41.91 180)
				(length 3.81)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 6.35 11.43 180)
				(length 3.81)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at -6.35 57.15 0)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 6.35 -19.05 180)
				(length 3.81)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 6.35 -57.15 180)
				(length 3.81)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at -6.35 26.67 0)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at -6.35 -6.35 0)
				(length 3.81)
				(name "Pin_c11")
				(number "c11")
			)
			(pin passive line
				(at -6.35 -36.83 0)
				(length 3.81)
				(name "Pin_c15")
				(number "c15")
			)
			(pin passive line
				(at -6.35 62.23 0)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at -6.35 -74.93 0)
				(length 3.81)
				(name "Pin_c20")
				(number "c20")
			)
			(pin passive line
				(at 6.35 46.99 180)
				(length 3.81)
				(name "Pin_c24")
				(number "c24")
			)
			(pin passive line
				(at 6.35 16.51 180)
				(length 3.81)
				(name "Pin_c28")
				(number "c28")
			)
			(pin passive line
				(at 6.35 8.89 180)
				(length 3.81)
				(name "Pin_c29")
				(number "c29")
			)
			(pin passive line
				(at 6.35 -21.59 180)
				(length 3.81)
				(name "Pin_c33")
				(number "c33")
			)
			(pin passive line
				(at 6.35 -52.07 180)
				(length 3.81)
				(name "Pin_c37")
				(number "c37")
			)
			(pin passive line
				(at -6.35 31.75 0)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at -6.35 24.13 0)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
		)
	)
)
