(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "DB15_Female_HighDensity" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "CN202" (id 0) (at 0 22.0218 0))
    (property "Value" "DB15_Female_HighDensity" (id 1) (at 0 19.7104 0))
    (property "Footprint" "AmigaFootprints:DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm" (id 2) (at -24.13 10.16 0))
    (property "Datasheet" " ~" (id 3) (at -24.13 10.16 0))
    (property "ki_keywords" "connector db15 VGA female D-SUB" (id 4) (at 0 0 0))
    (property "ki_description" "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "DSUB*Female*" (id 6) (at 0 0 0))
    (symbol "DB15_Female_HighDensity_0_1")
    (symbol "DB15_Female_HighDensity_1_1"
      (pin passive line (at -7.62 10.16 0) (length 5.08)
        (name "~")
        (number "1")
      )
      (pin passive line (at -7.62 -7.62 0) (length 5.08)
        (name "~")
        (number "10")
      )
      (pin passive line (at 7.62 10.16 180) (length 5.08)
        (name "~")
        (number "11")
      )
      (pin passive line (at 7.62 5.08 180) (length 5.08)
        (name "~")
        (number "12")
      )
      (pin passive line (at 7.62 0 180) (length 5.08)
        (name "~")
        (number "13")
      )
      (pin passive line (at 7.62 -5.08 180) (length 5.08)
        (name "~")
        (number "14")
      )
      (pin passive line (at 7.62 -10.16 180) (length 5.08)
        (name "~")
        (number "15")
      )
      (pin passive line (at -7.62 5.08 0) (length 5.08)
        (name "~")
        (number "2")
      )
      (pin passive line (at -7.62 0 0) (length 5.08)
        (name "~")
        (number "3")
      )
      (pin passive line (at -7.62 -5.08 0) (length 5.08)
        (name "~")
        (number "4")
      )
      (pin passive line (at -7.62 -10.16 0) (length 5.08)
        (name "~")
        (number "5")
      )
      (pin passive line (at -7.62 12.7 0) (length 5.08)
        (name "~")
        (number "6")
      )
      (pin passive line (at -7.62 7.62 0) (length 5.08)
        (name "~")
        (number "7")
      )
      (pin passive line (at -7.62 2.54 0) (length 5.08)
        (name "~")
        (number "8")
      )
      (pin passive line (at -7.62 -2.54 0) (length 5.08)
        (name "~")
        (number "9")
      )
    )
  )
)
